InspectionReport
Asphalt Paving Machine & Road Crew Safety Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Mobile Equipment (Paver & Rollers)
	Item
	Pass
	Fail
	N/A
	Notes

	Paver and tandem roller backup alarms are functioning and audible above ambient noise levels (min. 85 dBA).
	☐
	☐
	☐
	____________________

	Paver horn is operational and distinct.
	☐
	☐
	☐
	____________________

	Roller operator has clear, unobstructed visibility, or a spotter is used in blind spots.
	☐
	☐
	☐
	____________________

	Screed is free from defects (cracks, excessive wear) that could cause uneven asphalt distribution.
	☐
	☐
	☐
	____________________

	Hopper safety devices (e.g., locking pins, support arms) are in place and functioning correctly when the hopper is raised for maintenance.
	☐
	☐
	☐
	____________________

	Emergency stop buttons on the paver are clearly marked, accessible, and tested before each shift.
	☐
	☐
	☐
	____________________

	Roller seatbelts are present, undamaged, and used by the operator.
	☐
	☐
	☐
	____________________

	No visible hydraulic fluid, fuel, or oil leaks are present on the paver or rollers.
	☐
	☐
	☐
	____________________

	Paver tires are properly inflated and free from cuts, bulges, or excessive wear.
	☐
	☐
	☐
	____________________

	Roller drums are clean and free of excessive asphalt buildup that could affect compaction.
	☐
	☐
	☐
	____________________

	Paver headlights and taillights are functioning properly, especially for nighttime operations.
	☐
	☐
	☐
	____________________

	Roller parking brake effectively holds the machine on an incline.
	☐
	☐
	☐
	____________________


Site Conditions & Traffic Control
	Item
	Pass
	Fail
	N/A
	Notes

	A site-specific traffic control plan is in place, communicated to all workers, and effectively separates workers from public traffic (MUTCD compliant).
	☐
	☐
	☐
	____________________

	Warning signs (e.g., 'Hot Asphalt', 'Construction Ahead') are clearly visible and properly placed.
	☐
	☐
	☐
	____________________

	Pedestrian barriers are in place to prevent unauthorized access to the work zone.
	☐
	☐
	☐
	____________________

	Adequate lighting is provided for nighttime or low-light conditions (minimum 5 foot-candles).
	☐
	☐
	☐
	____________________

	Clear escape routes are identified and maintained in case of emergencies.
	☐
	☐
	☐
	____________________

	Work area is free from tripping hazards (e.g., tools, debris, materials).
	☐
	☐
	☐
	____________________

	Slopes adjacent to the paving area are stable and properly graded to prevent collapses.
	☐
	☐
	☐
	____________________

	Underground utilities have been located and marked before excavation or paving.
	☐
	☐
	☐
	____________________

	Workers maintain a safe distance from operating rollers and pavers (minimum 10 feet unless directly involved in the operation).
	☐
	☐
	☐
	____________________

	Clear communication methods (e.g., hand signals, radios) are established and understood by all workers.
	☐
	☐
	☐
	____________________

	Asphalt and other materials are stored in designated areas, away from traffic and pedestrian routes.
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	All workers wear high-visibility safety apparel (ANSI/ISEA 107 Class 2 or 3) appropriate for the work environment.
	☐
	☐
	☐
	____________________

	Workers wear safety glasses with side shields to protect against asphalt splash and debris.
	☐
	☐
	☐
	____________________

	Workers handling hot asphalt wear heat-resistant gloves.
	☐
	☐
	☐
	____________________

	Workers wear steel-toe boots that meet ASTM F2413 standards.
	☐
	☐
	☐
	____________________

	Workers wear long-sleeved shirts and pants to protect against asphalt burns and UV exposure.
	☐
	☐
	☐
	____________________

	Workers wear hard hats that meet ANSI Z89.1 standards.
	☐
	☐
	☐
	____________________

	Respiratory protection (e.g., N95 mask) is available and used when asphalt fume exposure exceeds permissible exposure limits (PELs).
	☐
	☐
	☐
	____________________

	Workers are encouraged to apply sunscreen with an SPF of 30 or higher.
	☐
	☐
	☐
	____________________

	PPE is clean, in good condition, and properly fitted.
	☐
	☐
	☐
	____________________

	An eyewash station is readily available in case of asphalt splash in the eyes.
	☐
	☐
	☐
	____________________


Heat Illness Prevention
	Item
	Pass
	Fail
	N/A
	Notes

	An adequate supply of cool, potable water (at least 1 quart per worker per hour) is readily available.
	☐
	☐
	☐
	____________________

	Shade is available for workers to take breaks during hot weather.
	☐
	☐
	☐
	____________________

	A heat acclimatization program is in place for new workers or those returning after an absence.
	☐
	☐
	☐
	____________________

	Work-rest cycles are implemented to reduce heat exposure during peak heat hours.
	☐
	☐
	☐
	____________________

	A buddy system is in place to monitor workers for signs of heat illness.
	☐
	☐
	☐
	____________________

	Workers are trained on the signs and symptoms of heat illness and how to respond.
	☐
	☐
	☐
	____________________

	Workers are encouraged to drink water frequently, even if they don't feel thirsty.
	☐
	☐
	☐
	____________________

	Workers with pre-existing medical conditions are closely monitored for heat stress.
	☐
	☐
	☐
	____________________

	Electrolyte replacement drinks are available to workers.
	☐
	☐
	☐
	____________________

	Ambient temperature and humidity are monitored to assess heat stress risk.
	☐
	☐
	☐
	____________________


Documentation & Training
	Item
	Pass
	Fail
	N/A
	Notes

	Material Safety Data Sheets (MSDS) for asphalt and other chemicals are readily available.
	☐
	☐
	☐
	____________________

	Daily equipment inspection logs are completed and maintained.
	☐
	☐
	☐
	____________________

	The traffic control plan is documented and readily available on site.
	☐
	☐
	☐
	____________________

	A competent person is designated and trained to conduct site safety inspections.
	☐
	☐
	☐
	____________________

	Workers are trained in basic first aid and CPR.
	☐
	☐
	☐
	____________________

	Equipment operators are trained and certified to operate the specific equipment they are using.
	☐
	☐
	☐
	____________________

	Workers are trained on hazard communication and chemical safety.
	☐
	☐
	☐
	____________________

	An emergency contact list is posted and readily accessible.
	☐
	☐
	☐
	____________________

	Regular safety meeting minutes are documented and available for review.
	☐
	☐
	☐
	____________________

	Incident reporting procedures are established and followed.
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
