InspectionReport
Autoclave Sterilization Safety Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Pre-Cycle Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Is the autoclave chamber free from debris, residue, and stains? (Visual inspection)
	☐
	☐
	☐
	____________________

	Inspect the door seal for cracks, tears, or deformation. Is the seal pliable and properly seated?
	☐
	☐
	☐
	____________________

	Verify the water level in the reservoir is within the recommended range as indicated by the manufacturer.
	☐
	☐
	☐
	____________________

	Is the drain screen clear of obstructions to ensure proper drainage?
	☐
	☐
	☐
	____________________

	Visually inspect temperature sensors for damage or corrosion.
	☐
	☐
	☐
	____________________

	Verify the pressure gauge is functioning correctly and reads zero when the chamber is at atmospheric pressure.
	☐
	☐
	☐
	____________________

	Confirm items are loaded according to validated procedures, ensuring proper steam penetration.
	☐
	☐
	☐
	____________________

	Verify the autoclave is equipped with a functional air removal system (e.g., vacuum pump or steam-flush pressure-pulse).
	☐
	☐
	☐
	____________________

	Confirm that the selected cycle parameters (temperature, pressure, time) are appropriate for the load being sterilized.
	☐
	☐
	☐
	____________________

	Verify that all safety interlocks (e.g., door locking mechanism) are functioning correctly.
	☐
	☐
	☐
	____________________


During-Cycle Monitoring
	Item
	Pass
	Fail
	N/A
	Notes

	Continuously monitor the pressure and temperature readings throughout the sterilization cycle. Are they within the validated range?
	☐
	☐
	☐
	____________________

	Ensure the cycle time matches the validated sterilization parameters.
	☐
	☐
	☐
	____________________

	Monitor for any alarms or error messages during the cycle. Document any occurrences.
	☐
	☐
	☐
	____________________

	If applicable, monitor steam quality indicators to ensure adequate steam purity.
	☐
	☐
	☐
	____________________

	Verify that condensate is being effectively removed from the chamber during the cycle.
	☐
	☐
	☐
	____________________

	Visually inspect the door seal for any signs of steam leakage during the cycle.
	☐
	☐
	☐
	____________________

	Monitor for excessive pressure fluctuations during the cycle, which could indicate a problem.
	☐
	☐
	☐
	____________________

	Verify that the cycle is progressing through the expected phases (e.g., heating, sterilization, drying).
	☐
	☐
	☐
	____________________


Post-Cycle Verification
	Item
	Pass
	Fail
	N/A
	Notes

	Verify that biological indicators (BIs) meet the required kill criteria after the cycle. Document results.
	☐
	☐
	☐
	____________________

	Inspect chemical indicators for the appropriate color change, indicating adequate sterilization conditions.
	☐
	☐
	☐
	____________________

	Visually inspect the load for any signs of damage or wetness.
	☐
	☐
	☐
	____________________

	Ensure the drying time is sufficient to prevent condensation on sterilized items.
	☐
	☐
	☐
	____________________

	Verify that the autoclave cycle completed successfully without any errors or interruptions.
	☐
	☐
	☐
	____________________

	Ensure all cycle parameters, BI/CI results, and operator information are accurately documented in the autoclave log.
	☐
	☐
	☐
	____________________

	Allow adequate cooling time before unloading the autoclave to prevent steam burns.
	☐
	☐
	☐
	____________________

	Confirm that unloading procedures are followed to minimize the risk of contamination.
	☐
	☐
	☐
	____________________


Maintenance and Calibration
	Item
	Pass
	Fail
	N/A
	Notes

	Verify that preventative maintenance is performed according to the manufacturer's recommendations and facility schedule.
	☐
	☐
	☐
	____________________

	Review calibration records for temperature and pressure sensors. Are they within the required tolerances?
	☐
	☐
	☐
	____________________

	Check the door seal replacement schedule. Is it within the recommended timeframe?
	☐
	☐
	☐
	____________________

	Verify that filters are replaced according to the manufacturer's recommendations.
	☐
	☐
	☐
	____________________

	Inspect the pressure relief valve for proper function and ensure it is not obstructed.
	☐
	☐
	☐
	____________________

	Verify the steam trap is functioning correctly to remove condensate from the steam lines.
	☐
	☐
	☐
	____________________

	Monitor the quality of the water used in the autoclave to prevent scale buildup and corrosion.
	☐
	☐
	☐
	____________________

	Verify that the autoclave chamber is cleaned regularly according to the facility's SOP.
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
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