InspectionReport
High-Rise Facade Cleaning Safety Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Davit Arm and Anchor Point Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Is the davit arm certified by a qualified engineer within the last 12 months? (Review certification documentation)
	☐
	☐
	☐
	____________________

	Perform a visual inspection of the davit arm for any signs of corrosion, cracks, or deformation.
	☐
	☐
	☐
	____________________

	Verify the davit arm's load rating is sufficient for the intended load, including personnel, equipment, and a safety factor of at least 5:1.
	☐
	☐
	☐
	____________________

	Inspect the davit arm's mounting points for secure attachment to the building structure. Check for loose bolts, damaged welds, or compromised structural integrity.
	☐
	☐
	☐
	____________________

	Is the anchor point certified by a qualified engineer within the last 12 months? (Review certification documentation)
	☐
	☐
	☐
	____________________

	Conduct a visual inspection of the anchor point for any signs of corrosion, cracks, or deformation.
	☐
	☐
	☐
	____________________

	Confirm the anchor point's load rating is sufficient for the intended load, including personnel, equipment, and a safety factor of at least 5:1.
	☐
	☐
	☐
	____________________

	Ensure the anchor point is readily accessible and free from obstructions that could hinder its use.
	☐
	☐
	☐
	____________________

	Verify the davit arm rotates freely and smoothly without any binding or excessive force.
	☐
	☐
	☐
	____________________

	Inspect the davit arm's locking mechanism to ensure it securely locks the arm in the desired position.
	☐
	☐
	☐
	____________________

	Verify the anchor point is located in a position that minimizes swing fall hazards.
	☐
	☐
	☐
	____________________

	Confirm the anchor point is clearly labeled with its load rating and date of last inspection.
	☐
	☐
	☐
	____________________


Rope Descent System (RDS) Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Inspect the working rope and safety line for cuts, abrasions, fraying, chemical damage, or excessive wear along their entire length.
	☐
	☐
	☐
	____________________

	Verify the rope diameter meets the manufacturer's specifications and is compatible with the descent control device.
	☐
	☐
	☐
	____________________

	Inspect rope terminations (knots, splices, swaged fittings) for proper construction and security.
	☐
	☐
	☐
	____________________

	Examine the descent control device for proper function, smooth operation, and any signs of damage or wear.
	☐
	☐
	☐
	____________________

	Verify the backup device (e.g., rope grab) is properly installed and functions correctly, arresting a fall immediately.
	☐
	☐
	☐
	____________________

	Inspect carabiners for proper locking mechanism function, gate closure, and any signs of damage or deformation. Ensure they are auto-locking and double-locking.
	☐
	☐
	☐
	____________________

	Inspect the full-body harness for cuts, abrasions, tears, or chemical damage. Verify proper fit and adjustment.
	☐
	☐
	☐
	____________________

	Ensure rope protectors are in place to prevent abrasion at edges and corners.
	☐
	☐
	☐
	____________________

	Verify the rope length is sufficient to reach the lowest intended work point with adequate slack.
	☐
	☐
	☐
	____________________

	Confirm proper rope management techniques are in place to prevent entanglement or snagging.
	☐
	☐
	☐
	____________________

	Verify all components of the RDS are compatible with each other and meet the manufacturer's specifications.
	☐
	☐
	☐
	____________________

	Review the rope log to ensure the rope has not exceeded its service life or been subjected to any damaging events.
	☐
	☐
	☐
	____________________


Public Protection Measures
	Item
	Pass
	Fail
	N/A
	Notes

	Ensure adequate barricades are in place to prevent pedestrian access to the work area below.
	☐
	☐
	☐
	____________________

	Verify warning signs are prominently displayed to alert pedestrians of overhead work.
	☐
	☐
	☐
	____________________

	Inspect debris netting for proper installation and integrity to prevent falling objects from reaching the ground.
	☐
	☐
	☐
	____________________

	Confirm a designated spotter is in place to monitor the work area and warn pedestrians of potential hazards.
	☐
	☐
	☐
	____________________

	Ensure all tools and equipment are properly tethered to prevent them from falling.
	☐
	☐
	☐
	____________________

	Verify clear communication protocols are in place between the workers and the spotter.
	☐
	☐
	☐
	____________________

	Define a clear drop zone and ensure all personnel are aware of its boundaries.
	☐
	☐
	☐
	____________________

	Assess wind conditions and suspend operations if winds exceed safe limits (typically 25 mph).
	☐
	☐
	☐
	____________________

	Review the weather forecast for any potential hazards (e.g., thunderstorms, high winds) and adjust work plans accordingly.
	☐
	☐
	☐
	____________________

	Confirm the emergency plan is in place and all personnel are familiar with its procedures.
	☐
	☐
	☐
	____________________

	Ensure a fully stocked first-aid kit is readily available on site.
	☐
	☐
	☐
	____________________

	Monitor pedestrian traffic flow and adjust barricades or spotter positioning as needed.
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Inspect hard hats for cracks, dents, or other damage. Ensure they meet ANSI Z89.1 standards.
	☐
	☐
	☐
	____________________

	Verify safety glasses or goggles are worn to protect against debris and chemical splashes. Ensure they meet ANSI Z87.1 standards.
	☐
	☐
	☐
	____________________

	Ensure appropriate gloves are worn to protect against cuts, abrasions, and chemical exposure. Check for tears or punctures.
	☐
	☐
	☐
	____________________

	Verify workers are wearing slip-resistant footwear with ankle support. Check for worn soles or damaged uppers.
	☐
	☐
	☐
	____________________

	Inspect the full-body harness for cuts, abrasions, tears, or chemical damage. Verify proper fit and adjustment.
	☐
	☐
	☐
	____________________

	Inspect the lanyard for cuts, abrasions, or damage to the snap hooks. Ensure it is properly connected to the harness and anchor point.
	☐
	☐
	☐
	____________________

	Verify all tools are properly tethered to prevent them from falling. Check the tether for damage or wear.
	☐
	☐
	☐
	____________________

	Ensure workers are wearing appropriate clothing for the weather conditions (e.g., rain gear, thermal layers).
	☐
	☐
	☐
	____________________

	Verify PPE is clean and properly maintained.
	☐
	☐
	☐
	____________________

	Ensure all PPE fits properly and is comfortable for the worker.
	☐
	☐
	☐
	____________________

	Confirm all workers have been trained on the proper use and maintenance of their PPE.
	☐
	☐
	☐
	____________________

	If required, ensure appropriate respiratory protection is worn and properly fitted. (e.g., for chemical cleaning).
	☐
	☐
	☐
	____________________


Documentation and Training
	Item
	Pass
	Fail
	N/A
	Notes

	Verify a Job Hazard Analysis (JHA) has been completed and reviewed with all workers.
	☐
	☐
	☐
	____________________

	Confirm a rescue plan is in place and all workers are trained on its procedures.
	☐
	☐
	☐
	____________________

	Verify a competent person is designated on site to oversee the work and ensure safety compliance.
	☐
	☐
	☐
	____________________

	Review training records to ensure all workers are properly trained in fall protection, rope descent systems, and hazard communication.
	☐
	☐
	☐
	____________________

	Inspect equipment inspection logs to ensure all equipment has been inspected and is in good working order.
	☐
	☐
	☐
	____________________

	Ensure Material Safety Data Sheets (MSDS) are readily available for all chemicals used on site.
	☐
	☐
	☐
	____________________

	Verify all required permits (e.g., street closure permits) are obtained and displayed.
	☐
	☐
	☐
	____________________

	Confirm a communication plan is in place to address emergencies and routine communication.
	☐
	☐
	☐
	____________________

	Verify a site-specific safety plan is in place and addresses the unique hazards of the location.
	☐
	☐
	☐
	____________________

	Ensure an emergency contact list is readily available with phone numbers for emergency services, supervisors, and building management.
	☐
	☐
	☐
	____________________

	Confirm a daily safety briefing is conducted before work begins to review hazards and safety procedures.
	☐
	☐
	☐
	____________________

	Ensure equipment manuals are available on site for reference.
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
