InspectionReport
Commercial Aquarium Dive Team Safety Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Dive Locker & Equipment Storage
	Item
	Pass
	Fail
	N/A
	Notes

	Dive locker is clean, dry, and organized to prevent equipment damage and ensure easy access. (IMCA D 023 4.1)
	☐
	☐
	☐
	____________________

	SCUBA cylinders (bailout bottles) are stored securely, preventing them from falling or being damaged. (CGA G-5.5)
	☐
	☐
	☐
	____________________

	Regulators and hoses are stored in a manner that prevents kinks, bends, or other damage. (ANSI/ACDE 03-2018 6.2.3)
	☐
	☐
	☐
	____________________

	Wet suits and dry suits are properly hung or stored to prevent compression and degradation of the neoprene. (Manufacturer's Recommendations)
	☐
	☐
	☐
	____________________

	Inventory of all dive tools (knives, shears, etc.) is complete and accounted for after each dive. (Aquarium SOP)
	☐
	☐
	☐
	____________________

	Batteries for dive lights and communication systems are stored in a dry, temperature-controlled environment. (NFPA 70)
	☐
	☐
	☐
	____________________

	First aid kit is fully stocked and readily accessible in the dive locker. Check expiration dates of all medications. (OSHA 29 CFR 1910.151)
	☐
	☐
	☐
	____________________

	Dive logbook is readily available and contains records of all dives, equipment maintenance, and incidents. (IMCA D 023 4.2)
	☐
	☐
	☐
	____________________

	Adequate supply of spare parts (o-rings, hoses, etc.) is maintained for critical dive equipment. (Aquarium SOP)
	☐
	☐
	☐
	____________________

	Cleaning and disinfection protocols are in place and followed for all dive equipment after each use. (CDC Guidelines)
	☐
	☐
	☐
	____________________


Surface-Supplied Air System
	Item
	Pass
	Fail
	N/A
	Notes

	Air compressor is operating within manufacturer's specifications, including pressure, temperature, and flow rate. (Manufacturer's Specifications)
	☐
	☐
	☐
	____________________

	Air quality is tested regularly (at least quarterly) and meets Grade E standards (or equivalent). Documentation available. (CGA G-7.1)
	☐
	☐
	☐
	____________________

	Umbilical hose is inspected for cuts, abrasions, kinks, and proper connections before each dive. (IMCA D 023 5.3)
	☐
	☐
	☐
	____________________

	Two-way communication system between diver and surface is functioning clearly and reliably. (OSHA 29 CFR 1910.426(c)(1))
	☐
	☐
	☐
	____________________

	Depth monitoring system is calibrated and functioning accurately, providing real-time depth readings to the surface. (ANSI/ACDE 03-2018 7.4.1)
	☐
	☐
	☐
	____________________

	Bailout bottle is fully charged and within hydrostatic test date. Pressure verified before each dive. (OSHA 29 CFR 1910.425(c)(5))
	☐
	☐
	☐
	____________________

	Regulator is functioning smoothly and delivering air on demand without excessive effort. (ANSI/ACDE 03-2018 6.2.2)
	☐
	☐
	☐
	____________________

	Backup air supply (e.g., pony bottle) is readily available at the surface in case of compressor failure. (Aquarium SOP)
	☐
	☐
	☐
	____________________

	Pressure gauges on the surface-supplied air system are accurate and calibrated. (ANSI/ACDE 03-2018 7.4.2)
	☐
	☐
	☐
	____________________

	Emergency shutdown procedures for the air compressor are clearly posted and understood by all personnel. (Aquarium SOP)
	☐
	☐
	☐
	____________________


Pre-Dive Procedures & Diver Briefing
	Item
	Pass
	Fail
	N/A
	Notes

	Dive plan is reviewed with all team members, including objectives, potential hazards, and emergency procedures. (OSHA 29 CFR 1910.422(b))
	☐
	☐
	☐
	____________________

	Each diver performs a thorough pre-dive equipment check, including mask, fins, BCD, regulator, and bailout bottle. (ANSI/ACDE 03-2018 8.1)
	☐
	☐
	☐
	____________________

	Buddy check is performed to verify proper equipment function and familiarity with emergency procedures. (PADI Standards)
	☐
	☐
	☐
	____________________

	Water conditions (temperature, visibility, currents) are assessed and communicated to the dive team. (Aquarium SOP)
	☐
	☐
	☐
	____________________

	Potential marine life hazards (e.g., venomous species, aggressive fish) are identified and discussed. (Aquarium SOP)
	☐
	☐
	☐
	____________________

	Locations of all filter intakes are clearly marked and communicated to the dive team. (Aquarium SOP)
	☐
	☐
	☐
	____________________

	Emergency signals (e.g., rope pulls, light signals) are reviewed and understood by all team members. (OSHA 29 CFR 1910.426(c)(2))
	☐
	☐
	☐
	____________________

	Diver's flag is properly displayed to warn boat traffic of diving operations. (USCG Regulations)
	☐
	☐
	☐
	____________________

	Surface support personnel are trained in emergency procedures and equipped to provide assistance. (OSHA 29 CFR 1910.427)
	☐
	☐
	☐
	____________________

	Clear communication protocols are established and tested between the diver, surface support, and aquarium staff. (Aquarium SOP)
	☐
	☐
	☐
	____________________


In-Water Safety & Monitoring
	Item
	Pass
	Fail
	N/A
	Notes

	Diver's location is continuously monitored from the surface. (OSHA 29 CFR 1910.427(b)(1))
	☐
	☐
	☐
	____________________

	Umbilical hose is managed to prevent entanglement or snagging. (IMCA D 023 5.3)
	☐
	☐
	☐
	____________________

	Diver's depth and bottom time are continuously monitored to prevent decompression sickness. (NOAA Diving Manual)
	☐
	☐
	☐
	____________________

	Divers maintain a safe distance from all filter intakes. (Aquarium SOP)
	☐
	☐
	☐
	____________________

	Divers avoid unnecessary contact with marine life. (Aquarium SOP)
	☐
	☐
	☐
	____________________

	Emergency ascent procedures are followed in case of equipment failure or other emergencies. (OSHA 29 CFR 1910.426(d))
	☐
	☐
	☐
	____________________

	Regular communication checks are conducted between the diver and surface support. (OSHA 29 CFR 1910.426(c)(1))
	☐
	☐
	☐
	____________________

	The buddy system is strictly adhered to at all times. (PADI Standards)
	☐
	☐
	☐
	____________________

	Decompression stops are strictly adhered to, if required. (NOAA Diving Manual)
	☐
	☐
	☐
	____________________

	Diver's air consumption is monitored to ensure adequate air supply for the duration of the dive. (Aquarium SOP)
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
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	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
