InspectionReport
High-Rise Glass Glazing & Installation Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Vacuum Lifter Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Inspect vacuum lifter pads for cuts, tears, or debris before each lift. Replace damaged pads immediately.
	☐
	☐
	☐
	____________________

	Verify vacuum lifter battery is fully charged before starting work. Ensure sufficient charge for the day's planned lifts.
	☐
	☐
	☐
	____________________

	Confirm vacuum gauge is functioning correctly and displays adequate vacuum pressure (minimum 80% of rated capacity) before lifting.
	☐
	☐
	☐
	____________________

	Test audible and visual low-vacuum alarms before each use. Ensure alarms activate at the manufacturer's specified threshold.
	☐
	☐
	☐
	____________________

	Verify the vacuum lifter's rated capacity exceeds the weight of the glass panel being lifted, with a safety factor of at least 2:1.
	☐
	☐
	☐
	____________________

	Inspect all vacuum hoses and connections for leaks or damage. Replace any compromised components immediately.
	☐
	☐
	☐
	____________________

	Review vacuum lifter maintenance records to ensure regular inspections and servicing are up-to-date.
	☐
	☐
	☐
	____________________

	Verify the emergency vacuum release mechanism is functional and easily accessible in case of power failure.
	☐
	☐
	☐
	____________________

	Confirm all operators are trained and certified in the safe operation of the specific vacuum lifter model being used.
	☐
	☐
	☐
	____________________

	Assess weather conditions (wind speed, rain) and halt glazing operations if conditions exceed the vacuum lifter's or glass panel's safe operating limits.
	☐
	☐
	☐
	____________________


Wind Load & Environmental Conditions
	Item
	Pass
	Fail
	N/A
	Notes

	Determine maximum allowable wind speed for glazing operations based on glass size, vacuum lifter capacity, and site-specific conditions. Use an anemometer to measure wind speed.
	☐
	☐
	☐
	____________________

	Monitor wind gust frequency and intensity. Suspend glazing operations if gusts exceed 75% of the maximum allowable wind speed.
	☐
	☐
	☐
	____________________

	Review updated weather forecasts at least every 4 hours to anticipate changes in wind conditions and adjust work plans accordingly.
	☐
	☐
	☐
	____________________

	Ensure glass panels are securely stored and protected from wind exposure before installation. Use appropriate bracing and tie-downs.
	☐
	☐
	☐
	____________________

	Identify and mitigate potential wind obstructions (e.g., adjacent buildings) that could create localized wind turbulence.
	☐
	☐
	☐
	____________________

	Monitor temperature extremes (high and low) that could affect vacuum lifter performance or glass panel integrity. Consult manufacturer specifications.
	☐
	☐
	☐
	____________________

	Suspend glazing operations during heavy rain or snow to prevent slippage and reduced visibility.
	☐
	☐
	☐
	____________________

	Monitor humidity levels, as high humidity can affect vacuum lifter performance. Consult manufacturer specifications.
	☐
	☐
	☐
	____________________

	Verify a site-specific wind action plan is in place and communicated to all personnel involved in glazing operations.
	☐
	☐
	☐
	____________________

	Ensure a clear emergency shutdown procedure is in place and understood by all personnel in case of sudden adverse weather conditions.
	☐
	☐
	☐
	____________________


Edge Protection & Fall Prevention
	Item
	Pass
	Fail
	N/A
	Notes

	Verify perimeter guardrails are installed and properly secured on all open edges where glazing is taking place. Ensure guardrails meet OSHA height requirements (42 inches +/- 3 inches).
	☐
	☐
	☐
	____________________

	Inspect safety nets for proper installation, adequate overlap, and sufficient clearance below. Ensure nets are free from damage or debris.
	☐
	☐
	☐
	____________________

	Ensure all glaziers are wearing properly fitted personal fall arrest systems (PFAS) with appropriate anchorage points. Inspect harnesses and lanyards for damage.
	☐
	☐
	☐
	____________________

	Verify anchorage points for PFAS are certified to withstand a minimum of 5,000 pounds per employee attached or designed by a qualified person.
	☐
	☐
	☐
	____________________

	Establish controlled access zones (CAZ) where guardrails or safety nets are not feasible. Clearly mark CAZ boundaries with warning lines or control lines.
	☐
	☐
	☐
	____________________

	Ensure warning lines are erected at least 6 feet from the edge of the roof or working surface. Verify lines are flagged every 6 feet.
	☐
	☐
	☐
	____________________

	Are 3.5-inch toe boards installed on all open sides to prevent tools and materials from falling (where applicable)?
	☐
	☐
	☐
	____________________

	Provide edge protection (e.g., edge protectors, gloves) to prevent cuts and lacerations when handling glass panels.
	☐
	☐
	☐
	____________________

	Establish and enforce a strict drop zone management plan to prevent tools and materials from falling to lower levels.
	☐
	☐
	☐
	____________________

	Maintain good housekeeping practices to prevent slips, trips, and falls. Keep walkways clear of debris and obstructions.
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Verify all personnel are wearing ANSI-approved hard hats in good condition.
	☐
	☐
	☐
	____________________

	Ensure all personnel are wearing ANSI Z87.1-approved safety glasses with side shields.
	☐
	☐
	☐
	____________________

	Confirm glaziers are wearing cut-resistant gloves when handling glass panels.
	☐
	☐
	☐
	____________________

	Ensure all personnel are wearing high-visibility clothing (Class 2 or 3) that meets ANSI 107 standards.
	☐
	☐
	☐
	____________________

	Verify all personnel are wearing steel-toed boots that meet ASTM F2413 standards.
	☐
	☐
	☐
	____________________

	Inspect fall protection harnesses for proper fit, damage, and wear. Ensure D-rings are in good condition.
	☐
	☐
	☐
	____________________

	Ensure personnel are wearing appropriate clothing for the weather conditions (e.g., rain gear, thermal layers).
	☐
	☐
	☐
	____________________

	Encourage the use of sunscreen and hats to protect against sun exposure.
	☐
	☐
	☐
	____________________

	Assess the need for respiratory protection based on site-specific conditions (e.g., dust, fumes). Provide appropriate respirators if required.
	☐
	☐
	☐
	____________________

	Verify that PPE is properly maintained, cleaned, and stored when not in use.
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
