InspectionReport
Commercial Flat Roof Fall Protection Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
I. Pre-Work Planning & Documentation
	Item
	Pass
	Fail
	N/A
	Notes

	Is a site-specific Fall Protection Plan documented and readily available? (OSHA 1926.502(h))
	☐
	☐
	☐
	____________________

	Has a Competent Person been designated to supervise fall protection measures? (OSHA 1926.502(f))
	☐
	☐
	☐
	____________________

	Was a pre-work safety briefing conducted, covering fall hazards and control measures? (OSHA 1926.20(b)(1))
	☐
	☐
	☐
	____________________

	Are inspection records available for all fall protection equipment (harnesses, lanyards, anchor points)? (ANSI Z359.11)
	☐
	☐
	☐
	____________________

	Have weather conditions (wind, rain, ice) been assessed for their impact on fall hazards? (OSHA 1926.501)
	☐
	☐
	☐
	____________________

	Is a documented rescue plan in place in case of a fall incident? (OSHA 1926.502(d)(20))
	☐
	☐
	☐
	____________________

	Are relevant MSDS/SDS sheets available for all chemicals used on the roof? (OSHA 1910.1200)
	☐
	☐
	☐
	____________________

	Are all site-specific hazards (e.g., power lines, asbestos) identified and communicated to workers?
	☐
	☐
	☐
	____________________


II. Warning Line Systems & Safety Monitors
	Item
	Pass
	Fail
	N/A
	Notes

	Are warning lines erected at least 6 feet from the roof edge? (OSHA 1926.502(f)(1)(ii))
	☐
	☐
	☐
	____________________

	Are warning lines flagged every 6 feet and capable of withstanding 16 pounds of force? (OSHA 1926.502(f)(1)(iii))
	☐
	☐
	☐
	____________________

	If mechanical equipment is used, are warning lines at least 10 feet from the edge? (OSHA 1926.502(f)(1)(ii))
	☐
	☐
	☐
	____________________

	Is the safety monitor competent and able to identify fall hazards? (OSHA 1926.502(k))
	☐
	☐
	☐
	____________________

	Can the safety monitor effectively communicate warnings to workers? (OSHA 1926.502(k))
	☐
	☐
	☐
	____________________

	Is the safety monitor free from other duties that could distract them from their safety responsibilities? (OSHA 1926.502(k))
	☐
	☐
	☐
	____________________

	Are warning lines clearly visible from all angles and in all lighting conditions?
	☐
	☐
	☐
	____________________

	Are warning lines securely anchored to prevent displacement by wind or contact?
	☐
	☐
	☐
	____________________

	Is the sag in the warning line minimal to prevent workers from tripping?
	☐
	☐
	☐
	____________________


III. Personal Fall Arrest Systems (PFAS)
	Item
	Pass
	Fail
	N/A
	Notes

	Inspect harnesses for damage (cuts, abrasions, chemical exposure) before each use. (ANSI Z359.11)
	☐
	☐
	☐
	____________________

	Inspect lanyards for frays, cuts, and proper functioning of snap hooks. (ANSI Z359.13)
	☐
	☐
	☐
	____________________

	Verify anchor points can support 5,000 lbs per worker attached. (OSHA 1926.502(d)(15))
	☐
	☐
	☐
	____________________

	Are anchor points positioned to minimize swing fall hazards? (OSHA 1926.502(d))
	☐
	☐
	☐
	____________________

	Is there adequate fall clearance below the work area to prevent ground contact? (OSHA 1926.502(d)(16))
	☐
	☐
	☐
	____________________

	Are all components of the PFAS (harness, lanyard, anchor) compatible? (ANSI Z359)
	☐
	☐
	☐
	____________________

	If using SRLs, do they retract and lock properly when tested? (ANSI Z359.14)
	☐
	☐
	☐
	____________________

	Are harnesses properly fitted to each worker? (OSHA 1926.502)
	☐
	☐
	☐
	____________________

	If using a horizontal lifeline, is it free from damage and properly tensioned?
	☐
	☐
	☐
	____________________


IV. Skylight & Roof Opening Protection
	Item
	Pass
	Fail
	N/A
	Notes

	Are all skylights protected by covers or guardrails capable of withstanding 200 lbs? (OSHA 1926.501(b)(4)(i))
	☐
	☐
	☐
	____________________

	Are skylight covers clearly marked with 'HOLE' or 'COVER' to prevent accidental stepping? (OSHA 1926.501(b)(4)(ii))
	☐
	☐
	☐
	____________________

	Are skylight covers securely fastened to prevent displacement? (OSHA 1926.501(b)(4))
	☐
	☐
	☐
	____________________

	Are all other roof openings (e.g., hatchways) guarded by railings or covers? (OSHA 1926.501(b)(4))
	☐
	☐
	☐
	____________________

	Are guardrails 42 inches (+/- 3 inches) in height with a mid-rail? (OSHA 1926.502(b)(1))
	☐
	☐
	☐
	____________________

	Can guardrails withstand 200 pounds of force in any direction? (OSHA 1926.502(b)(3))
	☐
	☐
	☐
	____________________

	Are toe boards installed where there is a risk of tools or materials falling on workers below? (OSHA 1926.502(j))
	☐
	☐
	☐
	____________________

	Are skylight covers made of durable material that will not break or crack under load?
	☐
	☐
	☐
	____________________

	Are skylight covers highly visible, especially in low-light conditions?
	☐
	☐
	☐
	____________________


V. General Site Conditions & Housekeeping
	Item
	Pass
	Fail
	N/A
	Notes

	Are walking/working surfaces free of slip, trip, and fall hazards (debris, tools, hoses)? (OSHA 1926.25(a))
	☐
	☐
	☐
	____________________

	Are materials stored in a manner that does not create a fall hazard or obstruct walkways? (OSHA 1926.250(a)(1))
	☐
	☐
	☐
	____________________

	Are materials stored at least 6 feet away from roof edges? (Best Practice)
	☐
	☐
	☐
	____________________

	Is there adequate lighting to safely perform work tasks? (OSHA 1926.56)
	☐
	☐
	☐
	____________________

	Are ladders used for access properly secured and extended 3 feet above the landing? (OSHA 1926.1053(b)(1))
	☐
	☐
	☐
	____________________

	Are ladders inspected before each use for defects? (OSHA 1926.1053(b)(15))
	☐
	☐
	☐
	____________________

	Are extension cords in good condition and properly grounded? (OSHA 1926.405)
	☐
	☐
	☐
	____________________

	Is a fire extinguisher readily available and inspected? (OSHA 1926.150(c)(1))
	☐
	☐
	☐
	____________________

	Is a first-aid kit readily available and adequately stocked? (OSHA 1926.50(c))
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
