InspectionReport
High-Rise Scaffold Handover Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Base and Foundations
	Item
	Pass
	Fail
	N/A
	Notes

	Are base plates used under all scaffold posts and are they adequately sized for the load? (OSHA 1926.451(c)(2))
	☐
	☐
	☐
	____________________

	If the scaffold is erected on soil, are mud sills used and properly sized to distribute the load? (OSHA 1926.451(c)(2))
	☐
	☐
	☐
	____________________

	Are footings level, sound, rigid, and capable of carrying the maximum intended load without settling or displacement? (OSHA 1926.451(c)(1))
	☐
	☐
	☐
	____________________

	Are all locking pins and mechanisms on adjustable base plates properly engaged and secured?
	☐
	☐
	☐
	____________________

	Assess ground conditions for signs of instability (water pooling, soft soil).
	☐
	☐
	☐
	____________________

	Verify scaffold is plumb and level within acceptable tolerances (check with a level).
	☐
	☐
	☐
	____________________

	If mobile, are caster brakes in good working order and engaged when stationary?
	☐
	☐
	☐
	____________________

	If mobile, are casters locked to prevent movement during use?
	☐
	☐
	☐
	____________________

	Confirm proper installation of diagonal bracing to prevent racking.
	☐
	☐
	☐
	____________________

	Inspect vertical standards for damage (bends, dents, corrosion).
	☐
	☐
	☐
	____________________


Scaffold Structure and Ties
	Item
	Pass
	Fail
	N/A
	Notes

	Are scaffold ties installed at the correct vertical and horizontal spacing as per the scaffold design? (OSHA 1926.451(e)(6)(i))
	☐
	☐
	☐
	____________________

	Are scaffold ties properly secured to both the scaffold and the building structure? (OSHA 1926.451(e)(6)(ii))
	☐
	☐
	☐
	____________________

	Inspect ties for any signs of damage or corrosion.
	☐
	☐
	☐
	____________________

	Verify all frame connections are properly secured with appropriate locking devices.
	☐
	☐
	☐
	____________________

	Ensure toprails are installed at the correct height (42 inches +/- 3 inches). (OSHA 1926.451(g)(4)(ii))
	☐
	☐
	☐
	____________________

	Ensure midrails are installed approximately halfway between the toprail and the platform surface. (OSHA 1926.451(g)(4)(iii))
	☐
	☐
	☐
	____________________

	Inspect guardrails for damage (bends, breaks, corrosion).
	☐
	☐
	☐
	____________________

	Are gaps between platform units and the uprights small enough to prevent falls? (OSHA 1926.451(b)(1)(i))
	☐
	☐
	☐
	____________________

	Do platform units overlap properly to prevent tripping hazards?
	☐
	☐
	☐
	____________________

	Inspect platforms for damage (cracks, rot, corrosion).
	☐
	☐
	☐
	____________________


Access and Egress
	Item
	Pass
	Fail
	N/A
	Notes

	Is safe access provided to all scaffold platforms (ladders, stair towers)? (OSHA 1926.451(e)(1))
	☐
	☐
	☐
	____________________

	Are ladders set at the correct angle (4:1 ratio)?
	☐
	☐
	☐
	____________________

	Do ladders extend at least 3 feet above the landing platform? (OSHA 1926.1053(b)(1))
	☐
	☐
	☐
	____________________

	Are ladders secured to prevent displacement?
	☐
	☐
	☐
	____________________

	If stair towers are used, are they properly constructed and secured?
	☐
	☐
	☐
	____________________

	Are stair railings installed on stair towers and in good condition?
	☐
	☐
	☐
	____________________

	Is access to and from the scaffold free from obstructions?
	☐
	☐
	☐
	____________________

	Are emergency egress routes clearly identified and unobstructed?
	☐
	☐
	☐
	____________________

	Inspect ladder rungs for damage, missing rungs, or slippery conditions.
	☐
	☐
	☐
	____________________

	Ensure ladders are placed on stable and level surfaces.
	☐
	☐
	☐
	____________________


Fall Protection
	Item
	Pass
	Fail
	N/A
	Notes

	Are all workers using appropriate personal fall arrest systems (PFAS) when required? (OSHA 1926.451(g)(1))
	☐
	☐
	☐
	____________________

	Inspect harnesses for damage, wear, and proper fit.
	☐
	☐
	☐
	____________________

	Inspect lanyards for cuts, abrasions, and proper functioning of snap hooks.
	☐
	☐
	☐
	____________________

	Are anchorage points adequate and properly rated for fall arrest? (OSHA 1926.502(d)(15))
	☐
	☐
	☐
	____________________

	Is there sufficient fall clearance below the work platform to prevent striking a lower level?
	☐
	☐
	☐
	____________________

	Are debris nets installed and properly maintained to catch falling objects?
	☐
	☐
	☐
	____________________

	Are 3.5-inch toe boards installed on all open sides and ends of the platform? (OSHA 1926.451(h)(2))
	☐
	☐
	☐
	____________________

	Inspect toe boards for damage or missing sections.
	☐
	☐
	☐
	____________________

	Are controlled access zones properly established and enforced?
	☐
	☐
	☐
	____________________

	Are warning lines used correctly and at the appropriate distance from the edge?
	☐
	☐
	☐
	____________________


Documentation and Tagging
	Item
	Pass
	Fail
	N/A
	Notes

	Is a scaffold design available and does it match the erected scaffold? (OSHA 1926.451(d)(1))
	☐
	☐
	☐
	____________________

	Was the scaffold erected under the supervision of a Competent Person? (OSHA 1926.451(f)(7))
	☐
	☐
	☐
	____________________

	Is a valid inspection tag attached to the scaffold, indicating it is safe for use? (OSHA 1926.451(f)(3))
	☐
	☐
	☐
	____________________

	Verify the inspection tag has not expired.
	☐
	☐
	☐
	____________________

	If a Red Tag is present, ensure the scaffold is not in use and the deficiencies are being addressed.
	☐
	☐
	☐
	____________________

	Is the maximum intended load capacity clearly posted on the scaffold? (OSHA 1926.451(f)(8))
	☐
	☐
	☐
	____________________

	Are any modifications to the scaffold approved by a Competent Person and documented?
	☐
	☐
	☐
	____________________

	Verify that workers using the scaffold have received proper training. (OSHA 1926.454)
	☐
	☐
	☐
	____________________

	Are daily scaffold inspection logs being maintained?
	☐
	☐
	☐
	____________________

	Confirm that all handover documentation is complete and accurate.
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
