InspectionReport
Concrete Boom Pump Truck Outrigger Setup Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Mobile Equipment Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Visually inspect outrigger arms and pads for cracks, bends, or other damage before each use. (OSHA 1926.1407(a))
	☐
	☐
	☐
	____________________

	Inspect hydraulic hoses and fittings for leaks. Repair or replace any leaking components before operation. (ANSI A10.3-2022 Sec. 6.2.1)
	☐
	☐
	☐
	____________________

	Verify that outrigger extension locking mechanisms are functioning correctly and securely lock the outrigger arms in the extended position. (BS EN 12001:2012+A1:2017 Clause 5.3.2.1)
	☐
	☐
	☐
	____________________

	Inspect tires for proper inflation and any signs of damage (cuts, bulges, or excessive wear). (OSHA 1926.600)
	☐
	☐
	☐
	____________________

	Test the horn to ensure it is functioning properly. (OSHA 1926.602(a)(9)(i))
	☐
	☐
	☐
	____________________

	Verify that the backup alarm is audible and functioning correctly when the pump is in reverse. (OSHA 1926.602(a)(9)(ii))
	☐
	☐
	☐
	____________________

	Confirm the emergency shut-off switch is easily accessible and functioning correctly. (ANSI A10.3-2022 Sec. 6.3.2)
	☐
	☐
	☐
	____________________

	Check engine oil, hydraulic fluid, and coolant levels. Top off as needed. (Manufacturer's Recommendations)
	☐
	☐
	☐
	____________________

	Ensure adequate fuel level for the duration of the concrete pour. (Best Practice)
	☐
	☐
	☐
	____________________

	Verify windshield wipers are functioning and the windshield is clean for optimal visibility. (OSHA 1926.601(b)(5))
	☐
	☐
	☐
	____________________


Site Conditions & Outrigger Setup
	Item
	Pass
	Fail
	N/A
	Notes

	Assess soil bearing capacity. Ensure soil is compacted and capable of supporting the pump truck's weight plus the weight of the concrete and boom. (ANSI A10.3-2022 Sec. 5.4.1)
	☐
	☐
	☐
	____________________

	Use appropriately sized outrigger pads/dunnage to distribute the load over a sufficient area. Pad size must be adequate for the soil conditions and pump weight. (OSHA 1926.1405(k)(1))
	☐
	☐
	☐
	____________________

	Outrigger pads/dunnage must be constructed of materials capable of supporting the load without deformation or failure (e.g., hardwood timbers, engineered composite pads). (Best Practice)
	☐
	☐
	☐
	____________________

	Ensure the pump truck is level after setting the outriggers. Use a level to verify. (ANSI A10.3-2022 Sec. 5.4.2)
	☐
	☐
	☐
	____________________

	Inspect for underground utilities (gas, water, electric) before setting outriggers. Call 811 before digging. (OSHA 1926.651(b)(2))
	☐
	☐
	☐
	____________________

	Identify and avoid overhead obstructions such as power lines, trees, and structures. (OSHA 1926.1408(a))
	☐
	☐
	☐
	____________________

	Maintain minimum clearance distances from overhead power lines as specified by OSHA 1926.1408. Document clearance distance. (OSHA 1926.1408(c))
	☐
	☐
	☐
	____________________

	Assess ground slope. Do not set up on excessively sloped surfaces. (Manufacturer's Recommendations)
	☐
	☐
	☐
	____________________

	Implement adequate traffic control measures (cones, barricades, flaggers) to protect the pump truck and personnel from vehicle traffic. (MUTCD Standards)
	☐
	☐
	☐
	____________________

	Establish pedestrian barriers to prevent unauthorized access to the work area. (Best Practice)
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Ensure all personnel in the work area are wearing hard hats that meet ANSI Z89.1 standards. (OSHA 1926.100(a))
	☐
	☐
	☐
	____________________

	Ensure all personnel are wearing safety glasses with side shields that meet ANSI Z87.1 standards. (OSHA 1926.102(a)(1))
	☐
	☐
	☐
	____________________

	Ensure all personnel are wearing steel-toe boots that meet ASTM F2413 standards. (OSHA 1926.96(b))
	☐
	☐
	☐
	____________________

	Ensure all personnel are wearing high-visibility clothing (vest or shirt) that meets ANSI/ISEA 107 standards. (OSHA 1926.201(a)(1))
	☐
	☐
	☐
	____________________

	Ensure personnel are wearing appropriate gloves for the task (e.g., leather gloves for handling equipment, rubber gloves for handling wet concrete). (Best Practice)
	☐
	☐
	☐
	____________________

	Assess noise levels. Provide and ensure the use of hearing protection if noise levels exceed 85 dBA. (OSHA 1926.52(b))
	☐
	☐
	☐
	____________________

	Assess air quality. Provide and ensure the use of respiratory protection if dust or other airborne contaminants are present. (OSHA 1910.134)
	☐
	☐
	☐
	____________________

	Ensure a readily available eyewash station is accessible in case of concrete splash. (OSHA 1926.50(c))
	☐
	☐
	☐
	____________________


Operational Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Conduct a pre-pour meeting to discuss the pour plan, potential hazards, and emergency procedures. (Best Practice)
	☐
	☐
	☐
	____________________

	Verify that the boom operator has a clear view of the work area and can safely operate the boom without contacting obstructions. (ANSI A10.3-2022 Sec. 7.2.1)
	☐
	☐
	☐
	____________________

	Ensure personnel are trained on proper hose handling procedures to prevent hose whip injuries. (Best Practice)
	☐
	☐
	☐
	____________________

	Use hose restraints (e.g., safety chains, straps) to prevent uncontrolled hose movement in case of a coupling failure. (Best Practice)
	☐
	☐
	☐
	____________________

	Establish clear communication signals between the boom operator and the nozzleman. (ANSI A10.3-2022 Sec. 7.3.2)
	☐
	☐
	☐
	____________________

	Ensure the boom tip is clearly visible to the operator at all times. Use spotters if necessary. (Best Practice)
	☐
	☐
	☐
	____________________

	Monitor wind conditions. Cease operations if wind speeds exceed the pump manufacturer's recommendations. (Manufacturer's Recommendations)
	☐
	☐
	☐
	____________________

	Inspect the concrete hose for wear, kinks, or damage before each use. Replace damaged hoses immediately. (Best Practice)
	☐
	☐
	☐
	____________________

	Ensure the nozzleman is positioned safely and has a clear escape route in case of an emergency. (Best Practice)
	☐
	☐
	☐
	____________________


Documentation & Training
	Item
	Pass
	Fail
	N/A
	Notes

	Verify that the boom pump operator is certified and trained to operate the specific type of pump being used. (ANSI A10.3-2022 Sec. 4.2.1)
	☐
	☐
	☐
	____________________

	Review the daily inspection log to ensure that the pump has been inspected and is in good working order. (OSHA 1926.1412)
	☐
	☐
	☐
	____________________

	Confirm a site-specific hazard assessment has been conducted and documented. (OSHA 1926.20(b)(1))
	☐
	☐
	☐
	____________________

	Document the outrigger setup, including pad size, soil conditions, and power line clearance distances. (Best Practice)
	☐
	☐
	☐
	____________________

	Verify that all personnel involved in the concrete pour have received adequate training on the hazards and safe work practices. (OSHA 1926.21(b)(2))
	☐
	☐
	☐
	____________________

	Ensure that the pump truck's load charts are readily available and legible. (OSHA 1926.1417)
	☐
	☐
	☐
	____________________

	Review maintenance records to ensure the pump has been properly maintained according to the manufacturer's recommendations. (Best Practice)
	☐
	☐
	☐
	____________________

	Ensure emergency contact information is readily available on site. (Best Practice)
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
