InspectionReport
Grain Silo Entry Safety Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Pre-Entry Permitting & LOTO
	Item
	Pass
	Fail
	N/A
	Notes

	Entry permit is completed, signed, and dated by authorized personnel before entry. (OSHA 1910.146(e))
	☐
	☐
	☐
	____________________

	Sweep auger and all mechanical equipment within the silo are completely locked out and tagged out. (OSHA 1910.272(g)(1)(i))
	☐
	☐
	☐
	____________________

	Electrical disconnects for all equipment are locked and tagged out at the main panel. (NFPA 70E)
	☐
	☐
	☐
	____________________

	Atmospheric testing for oxygen levels, combustible gases, and toxic substances is completed and documented within the permit. (OSHA 1910.146(d)(5))
	☐
	☐
	☐
	____________________

	Communication system (two-way radio or hard-wired system) between entrant and attendant is tested and functional. (OSHA 1910.146(i))
	☐
	☐
	☐
	____________________

	A detailed rescue plan is documented and readily available, including contact information for emergency services. (OSHA 1910.146(d)(9))
	☐
	☐
	☐
	____________________

	Entry permit is posted at the entry point of the grain silo. (OSHA 1910.146(e)(2))
	☐
	☐
	☐
	____________________

	Entrant and attendant have been briefed on the hazards, entry procedures, and emergency procedures. (OSHA 1910.146(h))
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Full-body harness fits correctly and is inspected for damage (tears, cuts, corrosion) before each use. (ANSI Z359.11)
	☐
	☐
	☐
	____________________

	Lifeline is in good condition, free from cuts, abrasions, and chemical damage. (ANSI Z359.15)
	☐
	☐
	☐
	____________________

	Respirator (if required) is properly fit-tested and the user is trained on its use and limitations. (OSHA 1910.134)
	☐
	☐
	☐
	____________________

	Appropriate dust mask (N95 or higher) is available and worn to minimize dust inhalation. (NIOSH Recommendations)
	☐
	☐
	☐
	____________________

	Safety glasses or goggles are worn to protect eyes from dust and debris. (ANSI Z87.1)
	☐
	☐
	☐
	____________________

	Appropriate footwear (steel-toed boots) is worn to protect feet from injury. (ANSI Z41)
	☐
	☐
	☐
	____________________

	Clothing is close-fitting to prevent entanglement with equipment or grain. (General Safety Practice)
	☐
	☐
	☐
	____________________

	Hearing protection is available and used if noise levels exceed 85 dBA. (OSHA 1910.95)
	☐
	☐
	☐
	____________________


Silo Condition & Environment
	Item
	Pass
	Fail
	N/A
	Notes

	Grain level is assessed to determine the extent of bridging or compaction. (Visual Inspection)
	☐
	☐
	☐
	____________________

	Signs of bridging (uneven surfaces, voids) are identified and addressed before entry. (Visual Inspection)
	☐
	☐
	☐
	____________________

	Dust accumulation on surfaces is assessed and controlled before and during entry. (NFPA 61)
	☐
	☐
	☐
	____________________

	Ventilation is adequate to minimize dust concentration and maintain breathable air. (ACGIH Recommendations)
	☐
	☐
	☐
	____________________

	Lighting is sufficient to provide clear visibility inside the silo. (OSHA 1926.56)
	☐
	☐
	☐
	____________________

	Temperature and humidity are monitored to prevent heat stress or other adverse conditions. (NIOSH Recommendations)
	☐
	☐
	☐
	____________________

	Entry point is clear of obstructions and provides safe access. (General Safety Practice)
	☐
	☐
	☐
	____________________

	Any internal obstructions (ladders, supports) are identified and accounted for in the entry plan. (Visual Inspection)
	☐
	☐
	☐
	____________________

	Grain condition (moisture, mold, foreign material) is assessed to identify potential hazards. (Visual Inspection)
	☐
	☐
	☐
	____________________


Fall Protection & Rescue Equipment
	Item
	Pass
	Fail
	N/A
	Notes

	Anchorage point for lifeline is rated for at least 5,000 lbs per person attached. (OSHA 1926.502(d)(15))
	☐
	☐
	☐
	____________________

	Lifeline is securely attached to the harness and the anchorage point. (ANSI Z359.15)
	☐
	☐
	☐
	____________________

	Retrieval system (winch or tripod) is available and in good working order for emergency extraction. (OSHA 1910.146(k)(3))
	☐
	☐
	☐
	____________________

	Rescue team is trained in grain engulfment rescue techniques and equipment operation. (OSHA 1910.146(k))
	☐
	☐
	☐
	____________________

	Rescue equipment (harnesses, ropes, cutting tools) is inspected before each use. (Manufacturer Recommendations)
	☐
	☐
	☐
	____________________

	Confined space monitor is present and continuously monitoring atmospheric conditions. (OSHA 1910.146(i))
	☐
	☐
	☐
	____________________

	First-aid kit is readily available and stocked with necessary supplies. (ANSI Z308.1)
	☐
	☐
	☐
	____________________

	A tagline is used to control the movement of the entrant within the silo. (Best Practice)
	☐
	☐
	☐
	____________________

	Cutting tools (e.g., grain rescue tubes) are available for creating a barrier around the engulfed person. (Grain Handling Safety Coalition Recommendations)
	☐
	☐
	☐
	____________________


Combustible Dust Control
	Item
	Pass
	Fail
	N/A
	Notes

	All potential ignition sources (open flames, sparks, hot surfaces) are removed from the silo area. (NFPA 61)
	☐
	☐
	☐
	____________________

	Measures are in place to control static electricity (grounding, bonding). (NFPA 77)
	☐
	☐
	☐
	____________________

	Housekeeping procedures are followed to minimize dust accumulation on surfaces. (NFPA 652)
	☐
	☐
	☐
	____________________

	Dust collection system (if present) is functional and properly maintained. (NFPA 652)
	☐
	☐
	☐
	____________________

	Explosion venting (if present) is clear of obstructions. (NFPA 68)
	☐
	☐
	☐
	____________________

	Hot work permit is required for any activities that could generate sparks or heat. (OSHA 1910.252)
	☐
	☐
	☐
	____________________

	Electrical equipment is rated for use in a Class II, Division 1 or 2 environment. (NEC Article 500)
	☐
	☐
	☐
	____________________

	No smoking policy is strictly enforced in and around the grain silo. (General Safety Practice)
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
