InspectionReport
Crane Pre-Operation Daily Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
Jurisdiction: Adaptable. Covers OSHA 29 CFR 1910.179 (US overhead and gantry cranes) and UK HSE LOLER 1998. Adaptable to other jurisdictions with crane regulations. Apply only the section and thresholds for the governing jurisdiction; do not combine US and UK requirements as if they were one code.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Inspection header
	Field
	Entry

	Crane type (overhead / gantry / jib)
	________________________________________________

	Crane ID / serial number
	________________________________________________

	Operator / inspector name
	________________________________________________

	Date and shift
	________________________________________________


Daily visual inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Fluid systems: no deterioration or leakage in pneumatic / hydraulic lines, tanks, valves, drain pumps
	☐
	☐
	☐
	____________________

	General condition: no loose, broken, or severely rusted parts on bridge, runway, hoist, or trolley
	☐
	☐
	☐
	____________________

	Rated capacity markings: maximum rated load clearly painted or plated on crane structure and individual hoist blocks
	☐
	☐
	☐
	____________________

	Work area: crane travel path of obstacles and personnel; warning devices / horns audible over ambient noise
	☐
	☐
	☐
	____________________


Functional testing
	Item
	Pass
	Fail
	N/A
	Notes

	Motion controls: pendant or radio controls; buttons move smoothly, don't stick, return to neutral 'off' when released
	☐
	☐
	☐
	____________________

	Brake testing: lift test load a few inches; load holds without drifting downward
	☐
	☐
	☐
	____________________

	Upper limit switch: tried out under no load; block 'inched' into limit or run in at slow speed; switch operates properly
	☐
	☐
	☐
	____________________


Wire ropes, chains, and below-the-hook devices
	Item
	Pass
	Fail
	N/A
	Notes

	Wire rope: entire visible length inspected for broken wires, severe kinking, bird-caging, twisting, diameter reduction; properly spooled in drum grooves
	☐
	☐
	☐
	____________________

	Hoist chains: no distorted links, gouges, excessive wear, or stretching beyond manufacturer tolerances
	☐
	☐
	☐
	____________________

	Slings and shackles: tags present on synthetic slings; no cuts, chemical burns, or melted fibers
	☐
	☐
	☐
	____________________


Hook inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Throat opening wear: ≤ 10% of original dimension
	☐
	☐
	☐
	____________________

	Hook twist: ≤ 10 degrees from original unbent plane
	☐
	☐
	☐
	____________________

	Safety latch: present, not bent, springs closed
	☐
	☐
	☐
	____________________

	Hardware: hook nut not loose; hook swivels freely
	☐
	☐
	☐
	____________________


Defect action and recordkeeping
	Item
	Pass
	Fail
	N/A
	Notes

	Deficiency constitutes safety hazard: Yes / No
	☐
	☐
	☐
	____________________

	Crane locked out and tagged out of service: Yes / No
	☐
	☐
	☐
	____________________

	Appointed person / qualified technician notified
	☐
	☐
	☐
	____________________

	Monthly inspection of hooks and hoist equipment: documented (signed, dated)
	☐
	☐
	☐
	____________________

	Inspector signature
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
References consulted
OSHA 29 CFR 1910.179 – Overhead and gantry cranes
UK HSE – LOLER 1998 (Lifting Operations and Lifting Equipment Regulations)
ASME B30.2 – Overhead and gantry cranes
OSHA 1910.179(n)(4)(i) – Upper limit switch testing
Verify the current edition and local adoption before use.
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
