InspectionReport
Data Center Electrical Safety Walk Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
LOTO (Lockout/Tagout) Compliance
	Item
	Pass
	Fail
	N/A
	Notes

	Is a written LOTO procedure readily available and specific to the equipment being worked on?
	☐
	☐
	☐
	____________________

	Are all authorized employees trained in LOTO procedures and can demonstrate competency?
	☐
	☐
	☐
	____________________

	Are LOTO devices (locks and tags) properly applied and clearly identified with the employee's name?
	☐
	☐
	☐
	____________________

	Is energy isolation verified before starting work (e.g., voltage testing after lockout)?
	☐
	☐
	☐
	____________________

	Are electrical panels clearly labeled with voltage and LOTO requirements?
	☐
	☐
	☐
	____________________

	For group LOTO, is a group lockout box used and properly managed?
	☐
	☐
	☐
	____________________

	Has a periodic inspection of the LOTO procedure been conducted within the last 12 months?
	☐
	☐
	☐
	____________________

	Is there a documented procedure for the safe removal of LOTO devices?
	☐
	☐
	☐
	____________________

	Are LOTO locks and tags in good condition and specifically designed for LOTO purposes?
	☐
	☐
	☐
	____________________

	Are all potential sources of hazardous energy (electrical, mechanical, pneumatic, etc.) properly controlled?
	☐
	☐
	☐
	____________________


Arc Flash Hazard Assessment & PPE
	Item
	Pass
	Fail
	N/A
	Notes

	Is a current arc flash hazard assessment available for the equipment being worked on (dated within the last 5 years)?
	☐
	☐
	☐
	____________________

	Are arc flash warning labels present and legible on all electrical equipment?
	☐
	☐
	☐
	____________________

	Is appropriate arc-rated PPE (clothing, face shield, gloves) available and in good condition?
	☐
	☐
	☐
	____________________

	Is the arc rating of the PPE sufficient for the calculated incident energy level?
	☐
	☐
	☐
	____________________

	Are workers aware of the arc flash boundary and approach distances?
	☐
	☐
	☐
	____________________

	Is a Qualified Person present and supervising the work?
	☐
	☐
	☐
	____________________

	Are insulated tools rated for the voltage being worked on?
	☐
	☐
	☐
	____________________

	Is the multimeter CAT III or CAT IV rated and in good working order?
	☐
	☐
	☐
	____________________

	Are unqualified persons kept outside the restricted approach boundary?
	☐
	☐
	☐
	____________________

	Is appropriate head protection (hard hat) being worn?
	☐
	☐
	☐
	____________________


Temporary Power & Grounding
	Item
	Pass
	Fail
	N/A
	Notes

	Are all temporary power circuits protected by Ground Fault Circuit Interrupters (GFCIs)?
	☐
	☐
	☐
	____________________

	Are temporary power cords free from damage (cuts, abrasions, exposed conductors)?
	☐
	☐
	☐
	____________________

	Are temporary power cords rated for the environment (e.g., wet location)?
	☐
	☐
	☐
	____________________

	Are temporary power cords properly secured to prevent tripping hazards?
	☐
	☐
	☐
	____________________

	Is all temporary electrical equipment properly grounded?
	☐
	☐
	☐
	____________________

	Is there clear access to temporary power distribution panels?
	☐
	☐
	☐
	____________________

	Are temporary power circuits protected by appropriate overcurrent protection (fuses or circuit breakers)?
	☐
	☐
	☐
	____________________

	Are temporary power connections weatherproof and protected from the elements?
	☐
	☐
	☐
	____________________

	Are extension cords used appropriately (not daisy-chained, not used as permanent wiring)?
	☐
	☐
	☐
	____________________

	Are temporary power systems inspected regularly?
	☐
	☐
	☐
	____________________


General Electrical Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Is there adequate working clearance (3 feet) in front of electrical panels?
	☐
	☐
	☐
	____________________

	Are all electrical panel covers in place and securely fastened?
	☐
	☐
	☐
	____________________

	Is any damaged electrical equipment (e.g., cracked enclosures, loose wiring) taken out of service?
	☐
	☐
	☐
	____________________

	Are cables and wiring properly managed to prevent tripping hazards and damage?
	☐
	☐
	☐
	____________________

	Are conduits and raceways properly installed and supported?
	☐
	☐
	☐
	____________________

	Are electrical components protected from moisture, dust, and other environmental hazards?
	☐
	☐
	☐
	____________________

	Are appropriate fire extinguishers (Class C) readily available near electrical equipment?
	☐
	☐
	☐
	____________________

	Is the area around electrical equipment kept clean and free from obstructions?
	☐
	☐
	☐
	____________________

	Are regular electrical inspections conducted and documented?
	☐
	☐
	☐
	____________________

	Are extension cords used only for temporary connections and not as permanent wiring?
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
