InspectionReport
Urban Building Demolition & Shoring Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Shoring System Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Verify shoring system load capacity matches or exceeds calculated loads from engineering survey (documented calculations available on site).
	☐
	☐
	☐
	____________________

	Inspect all shoring members (posts, beams, bracing) for damage (cracks, bends, corrosion) before installation and daily. Replace damaged members immediately.
	☐
	☐
	☐
	____________________

	Confirm vertical alignment of shoring posts using a plumb bob or laser level. Maximum allowable deviation: +/- 1/4 inch per 10 feet of height.
	☐
	☐
	☐
	____________________

	Ensure shoring baseplates are in full and level contact with the supporting surface. Use shims as needed to achieve full contact.
	☐
	☐
	☐
	____________________

	Check tightness of all shoring wedges and connections. Retighten as needed to maintain proper load transfer. Document wedge torque values.
	☐
	☐
	☐
	____________________

	Verify splice connections in shoring members are properly installed and tightened according to manufacturer's specifications. Inspect for slippage or loosening.
	☐
	☐
	☐
	____________________

	Monitor ground settlement around shoring footings daily. Maximum allowable settlement: 1/8 inch. Implement corrective action if settlement exceeds this limit.
	☐
	☐
	☐
	____________________

	Confirm engineering survey of shoring system is conducted daily, prior to commencement of demolition activities. Document survey results.
	☐
	☐
	☐
	____________________

	Inspect shoring system for weather-related damage (corrosion, water accumulation). Implement measures to protect shoring from weather exposure.
	☐
	☐
	☐
	____________________

	Ensure safe access and egress are maintained around the shoring system. Clear pathways of obstructions and debris.
	☐
	☐
	☐
	____________________


Demolition Sequencing & Pre-Weakening
	Item
	Pass
	Fail
	N/A
	Notes

	Verify demolition sequence adheres strictly to the approved demolition plan and engineering survey recommendations. Document any deviations.
	☐
	☐
	☐
	____________________

	Confirm load-bearing walls are clearly identified and marked on site plans and in the field before any pre-weakening or demolition occurs.
	☐
	☐
	☐
	____________________

	Ensure pre-weakening operations (e.g., controlled cuts) are performed under direct supervision of a qualified structural engineer.
	☐
	☐
	☐
	____________________

	Verify depth and extent of pre-weakening cuts are within specified limits outlined in the demolition plan and engineering calculations.
	☐
	☐
	☐
	____________________

	Monitor adjacent structures for signs of distress (cracks, settlement) during demolition activities. Implement corrective action if necessary.
	☐
	☐
	☐
	____________________

	Establish and maintain a clearly defined demolition zone with restricted access. Use barricades, signage, and spotters to prevent unauthorized entry.
	☐
	☐
	☐
	____________________

	Ensure material removal path is clear of obstructions and adequately supported. Inspect debris chutes for damage and proper installation.
	☐
	☐
	☐
	____________________

	Inspect debris chute connections, supports, and discharge point daily. Ensure chute is properly secured and prevents uncontrolled debris release.
	☐
	☐
	☐
	____________________

	Verify dust control measures (water suppression, enclosures) are in place and effectively minimizing dust emissions. Monitor air quality.
	☐
	☐
	☐
	____________________

	Implement vibration monitoring program if demolition activities may impact adjacent structures. Compare readings to acceptable limits.
	☐
	☐
	☐
	____________________


Mobile Equipment & Heavy Machinery
	Item
	Pass
	Fail
	N/A
	Notes

	Conduct daily inspection of all mobile equipment (excavators, loaders, cranes) before operation. Document inspection results.
	☐
	☐
	☐
	____________________

	Verify all equipment operators are properly trained and certified to operate the specific equipment being used. Maintain records of certifications.
	☐
	☐
	☐
	____________________

	Ensure load charts are readily available and legible for all cranes and lifting equipment. Operators must understand and adhere to load limits.
	☐
	☐
	☐
	____________________

	Identify and mitigate proximity hazards (overhead power lines, underground utilities) before operating mobile equipment. Maintain safe clearance distances.
	☐
	☐
	☐
	____________________

	Verify backup alarms are functioning properly on all mobile equipment. Repair or replace alarms immediately if defective.
	☐
	☐
	☐
	____________________

	Ensure all mobile equipment is equipped with rollover protection (ROPS) and seatbelts. Operators must wear seatbelts at all times.
	☐
	☐
	☐
	____________________

	Establish and maintain clear travel paths for mobile equipment. Minimize congestion and potential for collisions.
	☐
	☐
	☐
	____________________

	Implement safe refueling procedures for mobile equipment. Prohibit smoking and open flames during refueling. Use spill containment measures.
	☐
	☐
	☐
	____________________

	Verify parking brakes are engaged when mobile equipment is parked on slopes or uneven surfaces.
	☐
	☐
	☐
	____________________

	Test the horn on all mobile equipment daily to ensure it is functioning correctly.
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Ensure all personnel on site are wearing properly fitted hard hats that meet ANSI Z89.1 standards.
	☐
	☐
	☐
	____________________

	Verify appropriate eye protection (safety glasses, goggles, face shields) is worn based on the task being performed (e.g., cutting, grinding, demolition).
	☐
	☐
	☐
	____________________

	Ensure hearing protection (earplugs, earmuffs) is worn in areas where noise levels exceed 85 dBA. Conduct noise monitoring to determine exposure levels.
	☐
	☐
	☐
	____________________

	Verify appropriate hand protection (gloves) is worn based on the task being performed (e.g., handling debris, operating equipment).
	☐
	☐
	☐
	____________________

	Ensure all personnel are wearing safety shoes or boots that meet ANSI Z41 standards.
	☐
	☐
	☐
	____________________

	Verify all personnel working near mobile equipment or in traffic areas are wearing high-visibility clothing (vests, jackets) that meet ANSI 107 standards.
	☐
	☐
	☐
	____________________

	If respiratory hazards are present (dust, fumes), ensure a respiratory protection program is in place, including fit testing, medical evaluations, and proper respirator selection.
	☐
	☐
	☐
	____________________

	Inspect all PPE for damage or defects before each use. Replace damaged PPE immediately. Maintain PPE in good working condition.
	☐
	☐
	☐
	____________________

	Verify all personnel have received training on the proper use, care, and maintenance of required PPE.
	☐
	☐
	☐
	____________________

	Inspect fall protection harnesses daily for rips, tears, fraying, or other damage before each use.
	☐
	☐
	☐
	____________________


Documentation & Communication
	Item
	Pass
	Fail
	N/A
	Notes

	Verify the approved demolition plan, including engineering calculations and shoring design, is readily available on site.
	☐
	☐
	☐
	____________________

	Confirm daily engineering survey reports are completed and readily available for review. Reports must document shoring system condition and any observed deviations.
	☐
	☐
	☐
	____________________

	Verify a pre-demolition survey was conducted to identify potential hazards (asbestos, lead paint, utilities) and documented.
	☐
	☐
	☐
	____________________

	Confirm a competent person has been designated and is present on site to oversee demolition activities and ensure compliance with safety regulations.
	☐
	☐
	☐
	____________________

	Ensure emergency contact information (fire, police, ambulance, hospital) is readily available and posted in a conspicuous location.
	☐
	☐
	☐
	____________________

	Conduct daily toolbox talks to discuss specific hazards and safety procedures for the day's activities. Document attendance and topics covered.
	☐
	☐
	☐
	____________________

	Maintain a log of all personnel entering and exiting the demolition site. Restrict access to authorized personnel only.
	☐
	☐
	☐
	____________________

	Ensure a hazard communication program is in place, including SDSs for all hazardous materials used on site. Train employees on hazard recognition and safe handling procedures.
	☐
	☐
	☐
	____________________

	Maintain a detailed log of all shoring inspections, including dates, times, findings, and corrective actions taken.
	☐
	☐
	☐
	____________________

	Ensure incident reporting procedures are clearly defined and understood by all personnel. Investigate all incidents and implement corrective actions to prevent recurrence.
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
