InspectionReport
Elevator Shaft Installation & Fall Protection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Hoistway Barricade Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Are hoistway openings barricaded with a minimum 42-inch high guardrail system, including mid-rail and toe board?
	☐
	☐
	☐
	____________________

	Are barricade materials (wood, metal, etc.) structurally sound and capable of withstanding a 200-pound force in any direction?
	☐
	☐
	☐
	____________________

	Are barricades securely attached to the hoistway structure to prevent accidental displacement?
	☐
	☐
	☐
	____________________

	Are warning signs (e.g., 'Danger - Open Hoistway') clearly posted at each barricaded opening?
	☐
	☐
	☐
	____________________

	Do barricades allow for necessary access while preventing accidental falls into the hoistway?
	☐
	☐
	☐
	____________________

	Are 3.5-inch toe boards installed on all open sides of the hoistway to prevent tools and materials from falling?
	☐
	☐
	☐
	____________________

	Is a daily inspection of all hoistway barricades conducted and documented?
	☐
	☐
	☐
	____________________

	Are all barricades a minimum of 42 inches in height, with a midrail positioned halfway between the top rail and the walking/working surface?
	☐
	☐
	☐
	____________________

	Are barricades free from damage, deterioration, or any condition that could compromise their structural integrity?
	☐
	☐
	☐
	____________________

	Is adequate lighting (minimum 10 foot-candles) provided at all hoistway entrances and working areas?
	☐
	☐
	☐
	____________________


Fall Protection Systems (Personal)
	Item
	Pass
	Fail
	N/A
	Notes

	Are personal fall arrest systems (PFAS) inspected daily for damage, wear, and proper fit by a competent person?
	☐
	☐
	☐
	____________________

	Are anchor points for PFAS capable of supporting at least 5,000 pounds per employee attached?
	☐
	☐
	☐
	____________________

	Are tie-off points located above the worker's D-ring to minimize free-fall distance?
	☐
	☐
	☐
	____________________

	Are lanyards free from cuts, abrasions, chemical damage, and other signs of deterioration?
	☐
	☐
	☐
	____________________

	Do self-retracting lifelines (SRLs) function properly, with smooth extension and retraction?
	☐
	☐
	☐
	____________________

	Is there adequate fall clearance below the worker to prevent contact with lower levels or obstructions?
	☐
	☐
	☐
	____________________

	Is a rescue plan in place and readily available in case of a fall?
	☐
	☐
	☐
	____________________

	Is the full body harness compatible with the lanyard and anchorage connector being used?
	☐
	☐
	☐
	____________________

	Have all employees working at height received documented fall protection training?
	☐
	☐
	☐
	____________________

	Are car top railings in place and properly secured when performing car top inspections?
	☐
	☐
	☐
	____________________


Overhead Protection & Housekeeping
	Item
	Pass
	Fail
	N/A
	Notes

	Is overhead protection (e.g., netting, planking) in place to prevent tools and materials from falling into the hoistway?
	☐
	☐
	☐
	____________________

	Is the hoistway free from accumulated debris, tools, and materials that could create a hazard?
	☐
	☐
	☐
	____________________

	Are tools used at height tethered to prevent them from falling?
	☐
	☐
	☐
	____________________

	Are materials stored at least 6 feet away from the hoistway edge?
	☐
	☐
	☐
	____________________

	Are warning signs posted below the hoistway indicating potential falling object hazards?
	☐
	☐
	☐
	____________________

	If a false car is in use, is it inspected daily for structural integrity and proper operation?
	☐
	☐
	☐
	____________________

	Is adequate lighting provided below the hoistway to identify potential falling objects?
	☐
	☐
	☐
	____________________

	Is a reliable communication system (e.g., radios) in place between workers in the hoistway and those on other levels?
	☐
	☐
	☐
	____________________

	Is an emergency stop device readily accessible within the hoistway?
	☐
	☐
	☐
	____________________

	Is a fire extinguisher (minimum 2A:10BC rating) readily accessible near the hoistway?
	☐
	☐
	☐
	____________________


Electrical Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Are all electrical tools and equipment used in or near the hoistway GFCI protected?
	☐
	☐
	☐
	____________________

	Are extension cords free from damage, splices, and improper use?
	☐
	☐
	☐
	____________________

	Are electrical panels and disconnects readily accessible and clearly labeled?
	☐
	☐
	☐
	____________________

	Is a lockout/tagout procedure in place and followed for all electrical work?
	☐
	☐
	☐
	____________________

	Are all electrical tools and equipment properly grounded?
	☐
	☐
	☐
	____________________

	Are overhead power lines identified and are safe clearance distances maintained?
	☐
	☐
	☐
	____________________

	Is temporary wiring installed according to code requirements?
	☐
	☐
	☐
	____________________

	Is all electrical work performed by a qualified electrician?
	☐
	☐
	☐
	____________________

	Are electrical enclosures weatherproof when exposed to the elements?
	☐
	☐
	☐
	____________________

	Has an arc flash hazard assessment been conducted, and are appropriate PPE requirements being followed?
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
