InspectionReport
Equipment Inspection Checklist ()
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
Jurisdiction: Adaptable. Covers OSHA (US), ANSI, and ASME standards. Adaptable to other jurisdictions with equivalent work equipment regulations. Apply only the section and thresholds for the governing jurisdiction; do not combine US and UK requirements as if they were one code.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Equipment and inspection header
	Field
	Entry

	Equipment type and model
	________________________________________________

	Equipment ID / serial number
	________________________________________________

	Operator / inspector name
	________________________________________________

	Date and shift
	________________________________________________

	Inspection type (pre-use / operational / periodic)
	________________________________________________


Pre-use walkaround
	Item
	Pass
	Fail
	N/A
	Notes

	Fluid leaks (hydraulic, engine oil, coolant, fuel)
	☐
	☐
	☐
	____________________

	Damaged hoses and fittings
	☐
	☐
	☐
	____________________

	Worn tires or tracks
	☐
	☐
	☐
	____________________

	Cracked frames or structural components
	☐
	☐
	☐
	____________________

	Missing or damaged guards
	☐
	☐
	☐
	____________________

	Damaged lights and reflectors
	☐
	☐
	☐
	____________________

	Loose or missing fasteners
	☐
	☐
	☐
	____________________

	Operator visibility (cracked glass, dirty windows)
	☐
	☐
	☐
	____________________


Safety equipment
	Item
	Pass
	Fail
	N/A
	Notes

	Seat belts: functional
	☐
	☐
	☐
	____________________

	ROPS / FOPS: intact, no cracks or unauthorized welds
	☐
	☐
	☐
	____________________

	Emergency stops: functional
	☐
	☐
	☐
	____________________

	Operator presence system: functional
	☐
	☐
	☐
	____________________

	Fire extinguisher: present and charged
	☐
	☐
	☐
	____________________

	Backup camera (if fitted): functional
	☐
	☐
	☐
	____________________


Operational test
	Item
	Pass
	Fail
	N/A
	Notes

	Gauges and warning lights: operational
	☐
	☐
	☐
	____________________

	Horn and backup alarm: functional and audible
	☐
	☐
	☐
	____________________

	Steering: responsive, no binding
	☐
	☐
	☐
	____________________

	Brakes: service, parking, emergency stop all functional
	☐
	☐
	☐
	____________________

	Throttle response: smooth
	☐
	☐
	☐
	____________________

	Hydraulic functions: smooth, no jerking
	☐
	☐
	☐
	____________________

	Lifting mechanisms and attachments: full range of motion
	☐
	☐
	☐
	____________________


Periodic maintenance items
	Item
	Pass
	Fail
	N/A
	Notes

	Fluid levels: engine oil, hydraulic, coolant, fuel
	☐
	☐
	☐
	____________________

	Filter condition indicators
	☐
	☐
	☐
	____________________

	Belt tension
	☐
	☐
	☐
	____________________

	Battery terminals and charge
	☐
	☐
	☐
	____________________

	Tire pressure and tread depth
	☐
	☐
	☐
	____________________

	Lubrication points
	☐
	☐
	☐
	____________________


Defect tracking
	Item
	Pass
	Fail
	N/A
	Notes

	Defect description
	☐
	☐
	☐
	____________________

	Pass / Fail rating
	☐
	☐
	☐
	____________________

	Corrective action required
	☐
	☐
	☐
	____________________

	Equipment status (in service / out of service)
	☐
	☐
	☐
	____________________

	Inspector signature
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
References consulted
OSHA 29 CFR 1910.178 – Powered industrial trucks
OSHA 29 CFR 1926.1400 – Cranes and derricks
OSHA 29 CFR 1910.67 and 1926.453 – Aerial lifts
ASME B30.5 – Mobile and locomotive cranes
ANSI A92 – Aerial work platforms
Verify the current edition and local adoption before use.
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
