InspectionReport
Temporary Bleacher & Grandstand Safety Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Structural Integrity
	Item
	Pass
	Fail
	N/A
	Notes

	Verify that the foundation or ground supporting the grandstand is level, stable, and capable of bearing the anticipated load. Check for signs of settlement or erosion.
	☐
	☐
	☐
	____________________

	Inspect all frame connections (bolts, welds, pins) for tightness, corrosion, and damage. Ensure all locking mechanisms are properly engaged.
	☐
	☐
	☐
	____________________

	Confirm that all required support bracing (cross-bracing, diagonal bracing) is in place and properly secured. Check for bent, damaged, or missing braces.
	☐
	☐
	☐
	____________________

	Examine all planking (seating and walkways) for cracks, splits, rot, or other damage. Replace any damaged planks immediately.
	☐
	☐
	☐
	____________________

	Verify that all planking is securely fastened to the frame to prevent movement or displacement. Check for proper spacing between planks.
	☐
	☐
	☐
	____________________

	Confirm that the grandstand's load capacity is clearly posted and not exceeded. Ensure event staff are aware of the load limits.
	☐
	☐
	☐
	____________________

	Measure aisle widths to ensure they meet minimum code requirements for safe egress. Clear aisles of any obstructions.
	☐
	☐
	☐
	____________________

	Verify that all egress pathways are clear, well-lit, and free from obstructions. Ensure adequate signage is in place to guide occupants to exits.
	☐
	☐
	☐
	____________________

	Inspect all metal components (bolts, connectors, etc.) for signs of corrosion. Replace corroded hardware immediately.
	☐
	☐
	☐
	____________________

	Monitor for any signs of settling or shifting of the structure during and after setup. Re-level and stabilize as needed.
	☐
	☐
	☐
	____________________


Guardrails and Fall Protection
	Item
	Pass
	Fail
	N/A
	Notes

	Measure guardrail height to ensure it meets minimum code requirements (typically 42 inches).
	☐
	☐
	☐
	____________________

	Verify that guardrails are capable of withstanding the required load (typically 200 pounds). Test for stability and rigidity.
	☐
	☐
	☐
	____________________

	Confirm that midrails are installed between the top rail and the walking surface to prevent falls. Spacing should not exceed 19 inches.
	☐
	☐
	☐
	____________________

	Ensure that toe boards (minimum 4 inches high) are installed where there is a risk of objects falling onto people below.
	☐
	☐
	☐
	____________________

	Inspect stair railings for proper height, strength, and secure attachment. Ensure handrails are continuous and graspable.
	☐
	☐
	☐
	____________________

	Measure gaps in guardrails and stair railings to ensure they do not exceed code limits (typically 4 inches).
	☐
	☐
	☐
	____________________

	If required, verify that fall arrest systems (harnesses, lanyards, anchor points) are in good condition and properly inspected. Ensure users are trained in their use.
	☐
	☐
	☐
	____________________

	Confirm that perimeter barriers are in place to prevent unauthorized access to the grandstand structure.
	☐
	☐
	☐
	____________________

	Ensure handrails extend beyond the top and bottom risers of stairways as required by code.
	☐
	☐
	☐
	____________________

	Verify the guardrail design prevents easy climbing by children (e.g., no horizontal rails spaced closely together).
	☐
	☐
	☐
	____________________


Egress and Emergency Preparedness
	Item
	Pass
	Fail
	N/A
	Notes

	Verify that exit signs are clearly visible, properly illuminated, and indicate the direction of egress.
	☐
	☐
	☐
	____________________

	Confirm that emergency lighting is functional and provides adequate illumination in the event of a power outage.
	☐
	☐
	☐
	____________________

	Ensure that fire extinguishers are readily accessible, properly charged, and inspected. Verify that personnel are trained in their use.
	☐
	☐
	☐
	____________________

	Review the emergency evacuation plan with event staff. Ensure everyone knows the evacuation routes and procedures.
	☐
	☐
	☐
	____________________

	Confirm that first aid supplies and trained personnel are available on-site.
	☐
	☐
	☐
	____________________

	Verify that communication systems (radios, public address system) are functional and can be used to communicate emergency information.
	☐
	☐
	☐
	____________________

	Assess crowd management procedures to ensure orderly entry, seating, and egress. Identify potential bottlenecks and develop strategies to mitigate them.
	☐
	☐
	☐
	____________________

	Verify that accessible routes are provided for individuals with disabilities, in accordance with ADA requirements.
	☐
	☐
	☐
	____________________

	Ensure all exit doors are equipped with panic hardware that allows for easy egress in an emergency.
	☐
	☐
	☐
	____________________

	Identify and clearly mark designated muster points for evacuation.
	☐
	☐
	☐
	____________________


Daily Hardware Checks
	Item
	Pass
	Fail
	N/A
	Notes

	Visually inspect and spot-check the tightness of critical bolts and fasteners, especially in high-stress areas.
	☐
	☐
	☐
	____________________

	Verify that plank supports are securely in place and show no signs of bending or cracking.
	☐
	☐
	☐
	____________________

	Inspect guardrail connections for looseness or damage. Ensure all locking pins or mechanisms are engaged.
	☐
	☐
	☐
	____________________

	Confirm that all access points (stairs, ramps) are clear of debris and in good repair.
	☐
	☐
	☐
	____________________

	Assess the impact of weather conditions (wind, rain) on the stability of the grandstand. Take appropriate action if necessary.
	☐
	☐
	☐
	____________________

	Re-inspect the ground conditions around the base of the structure for any signs of erosion or settling.
	☐
	☐
	☐
	____________________

	Ensure all safety signage (load limits, exit signs) are clearly visible and legible.
	☐
	☐
	☐
	____________________

	Verify that all lighting systems are functioning properly, including emergency lighting.
	☐
	☐
	☐
	____________________

	Inspect for any signs of vandalism or tampering with the structure.
	☐
	☐
	☐
	____________________

	Maintain an inventory of spare hardware (bolts, pins, etc.) for quick repairs.
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
