InspectionReport
Fire Extinguisher Inspection Checklist ()
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
Jurisdiction: US. NFPA 10 is the US standard for portable fire extinguishers. The checklist covers monthly visual checks and annual maintenance per NFPA 10.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Unit identification
	Field
	Entry

	Extinguisher ID number
	________________________________________________

	Location (building, floor, room)
	________________________________________________

	Type (ABC, CO2, Class K, etc.)
	________________________________________________

	Size / rating
	________________________________________________

	Manufacturer
	________________________________________________


Monthly visual inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Accessible and unobstructed
	☐
	☐
	☐
	____________________

	Operating instructions legible
	☐
	☐
	☐
	____________________

	Safety seal intact
	☐
	☐
	☐
	____________________

	Pin in place
	☐
	☐
	☐
	____________________

	Gauge in operable range (green zone)
	☐
	☐
	☐
	____________________

	No visible damage to cylinder
	☐
	☐
	☐
	____________________

	Pressure gauge readable
	☐
	☐
	☐
	____________________

	Nozzle not blocked
	☐
	☐
	☐
	____________________

	Hose intact (no cracks or dry rot)
	☐
	☐
	☐
	____________________

	No corrosion or leakage
	☐
	☐
	☐
	____________________

	Mounting bracket secure
	☐
	☐
	☐
	____________________

	Tamper seal present
	☐
	☐
	☐
	____________________


Annual maintenance check
	Item
	Pass
	Fail
	N/A
	Notes

	Date of last maintenance
	☐
	☐
	☐
	____________________

	Maintenance tag present and dated
	☐
	☐
	☐
	____________________

	Weight check (CO2 and non-gauge types)
	☐
	☐
	☐
	____________________

	Internal inspection (by certified technician)
	☐
	☐
	☐
	____________________

	Recharge date (if applicable)
	☐
	☐
	☐
	____________________

	Hydrostatic test date
	☐
	☐
	☐
	____________________


Hydrostatic testing schedule
	Item
	Pass
	Fail
	N/A
	Notes

	Stored-pressure water and loaded stream: every 5 years
	☐
	☐
	☐
	____________________

	Cartridge-operated water and loaded stream: every 5 years
	☐
	☐
	☐
	____________________

	Carbon dioxide: every 5 years
	☐
	☐
	☐
	____________________

	Wet chemical (Class K): every 5 years
	☐
	☐
	☐
	____________________

	Dry chemical and dry powder: every 12 years
	☐
	☐
	☐
	____________________

	Halon and clean agents: every 5 years
	☐
	☐
	☐
	____________________


Defect resolution
	Item
	Pass
	Fail
	N/A
	Notes

	Defect description (if any)
	☐
	☐
	☐
	____________________

	Action taken (repair / replace / remove from service)
	☐
	☐
	☐
	____________________

	Replacement unit installed
	☐
	☐
	☐
	____________________

	Inspector initials and date
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
References consulted
NFPA 10: Standard for Portable Fire Extinguishers (2022)
OSHA 29 CFR 1910.157 – Fire extinguishers
NFPA 10 §7.2 – Inspection and maintenance
Verify the current edition and local adoption before use.
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
