InspectionReport
Forklift Battery Charging & Change-out Safety Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Battery Charging Area - Site Conditions
	Item
	Pass
	Fail
	N/A
	Notes

	Is the battery charging area equipped with adequate ventilation to prevent hydrogen gas accumulation (e.g., mechanical exhaust system)?
	☐
	☐
	☐
	____________________

	Is a hydrogen gas detector present and calibrated to alarm at or below 1% (25% LEL) hydrogen concentration?
	☐
	☐
	☐
	____________________

	Is an eyewash station located within 10 seconds (or 100 feet) of the battery charging area, on the same level, with unobstructed access?
	☐
	☐
	☐
	____________________

	Is the eyewash station flushing freely with potable water for a minimum of 15 minutes, and is the water tepid (60-100°F)?
	☐
	☐
	☐
	____________________

	Is an acid spill kit readily available and fully stocked with neutralizing agents, PPE, and disposal bags?
	☐
	☐
	☐
	____________________

	Are 'No Smoking' signs clearly posted within 50 feet of the battery charging area?
	☐
	☐
	☐
	____________________

	Is a Class C fire extinguisher (suitable for electrical fires) readily accessible and fully charged?
	☐
	☐
	☐
	____________________

	Is the floor in the battery charging area acid-resistant and free from cracks or damage that could trap spilled acid?
	☐
	☐
	☐
	____________________

	Is there adequate lighting (minimum 50 foot-candles) in the battery charging area to safely perform tasks?
	☐
	☐
	☐
	____________________

	Are spare batteries stored on designated racks or pallets, preventing direct contact with the floor?
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Are acid-resistant aprons available and in good condition for all personnel handling batteries?
	☐
	☐
	☐
	____________________

	Are acid-resistant gloves (nitrile or neoprene) available and in good condition for all personnel handling batteries?
	☐
	☐
	☐
	____________________

	Are full-face shields or safety glasses with side shields available and in good condition for all personnel handling batteries?
	☐
	☐
	☐
	____________________

	Is PPE inspected before each use for tears, punctures, or other damage?
	☐
	☐
	☐
	____________________

	Have all personnel been trained on the proper use, maintenance, and disposal of PPE?
	☐
	☐
	☐
	____________________

	Are safety shoes with steel toe protection worn by all personnel handling batteries?
	☐
	☐
	☐
	____________________

	Is there a written eye protection policy enforced in the battery charging area?
	☐
	☐
	☐
	____________________

	Is there a designated area for storing PPE when not in use, away from potential contamination?
	☐
	☐
	☐
	____________________

	Are procedures in place for cleaning and decontaminating PPE after each use?
	☐
	☐
	☐
	____________________


Battery Handling Equipment
	Item
	Pass
	Fail
	N/A
	Notes

	Is the battery extractor (if used) in good working order, with all safety features functioning correctly?
	☐
	☐
	☐
	____________________

	Is the battery extractor rated for the weight of the batteries being handled?
	☐
	☐
	☐
	____________________

	Is the battery extractor inspected daily for damage, wear, or missing parts?
	☐
	☐
	☐
	____________________

	If a hoist is used, is the chain or strap inspected for wear, damage, or deformation before each use?
	☐
	☐
	☐
	____________________

	If a hoist is used, is it rated for the weight of the batteries being handled, with a clear load rating visible?
	☐
	☐
	☐
	____________________

	If a pallet jack is used, are the wheels and lifting mechanism in good working order?
	☐
	☐
	☐
	____________________

	Are lifting slings (if used) inspected for cuts, abrasions, or chemical damage before each use?
	☐
	☐
	☐
	____________________

	Have all personnel been trained on the safe operation of the battery handling equipment?
	☐
	☐
	☐
	____________________

	Is there a documented maintenance schedule for the battery handling equipment?
	☐
	☐
	☐
	____________________


Battery Charging Procedures
	Item
	Pass
	Fail
	N/A
	Notes

	Is the battery charger voltage compatible with the battery being charged?
	☐
	☐
	☐
	____________________

	Is the battery charger free from damage, with all cables and connectors in good condition?
	☐
	☐
	☐
	____________________

	Are all battery cables and connectors properly insulated and free from exposed wires?
	☐
	☐
	☐
	____________________

	Are all battery vent caps in place and functioning correctly?
	☐
	☐
	☐
	____________________

	Is the area around the battery charger clear of obstructions and flammable materials?
	☐
	☐
	☐
	____________________

	Are battery connections clean and tight, preventing arcing or sparking?
	☐
	☐
	☐
	____________________

	Is the battery charging process monitored to prevent overcharging or overheating?
	☐
	☐
	☐
	____________________

	Is the electrolyte level in the battery checked regularly and maintained at the proper level with distilled water?
	☐
	☐
	☐
	____________________

	Is the battery temperature monitored during charging to prevent overheating?
	☐
	☐
	☐
	____________________

	Are the charger's operating instructions readily available and followed?
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
