InspectionReport
Forklift Pre-Operation Inspection Report
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
Jurisdiction: US. OSHA 29 CFR 1910.178 is the US standard for powered industrial trucks. Adaptable to other jurisdictions with equivalent forklift regulations.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Inspection header
	Field
	Entry

	Forklift type and model
	________________________________________________

	Forklift ID / serial number
	________________________________________________

	Operator name
	________________________________________________

	Date and shift
	________________________________________________


5-Point visual checklist (engine off)
	Item
	Pass
	Fail
	N/A
	Notes

	Tires and wheels: no chunking, missing rubber, proper inflation; lug nuts tight
	☐
	☐
	☐
	____________________

	Forks and mast: no cracks in fork heels; mast chains equally tensioned, no stretching or rust
	☐
	☐
	☐
	____________________

	Fluid levels: engine oil, hydraulic fluid, coolant, brake fluid; no fresh fluid drips on floor
	☐
	☐
	☐
	____________________

	Safety guards: overhead guard firmly attached; load backrest extension in place
	☐
	☐
	☐
	____________________

	Decals and nameplate: data capacity plate legible; safety warning decals present and legible
	☐
	☐
	☐
	____________________


4-Point operational checklist (engine on)
	Item
	Pass
	Fail
	N/A
	Notes

	Brakes: foot brake and parking brake functional; pedal not spongy; parking brake holds on incline
	☐
	☐
	☐
	____________________

	Steering: turns fully left and right; no grinding noises; no excessive play in column
	☐
	☐
	☐
	____________________

	Hydraulics: forks raise and lower to full limits; mast tilts fully forward and back; movement smooth, not jerky
	☐
	☐
	☐
	____________________

	Safety alarms: horn loud enough over warehouse noise; backup alarm and flashing strobe light functional
	☐
	☐
	☐
	____________________


Defective forklift handling
	Item
	Pass
	Fail
	N/A
	Notes

	Forklift parked in designated out-of-service area
	☐
	☐
	☐
	____________________

	Key removed
	☐
	☐
	☐
	____________________

	'Do Not Operate' tag placed on steering wheel
	☐
	☐
	☐
	____________________

	Inspection report submitted to maintenance supervisor
	☐
	☐
	☐
	____________________

	Operator signature
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
References consulted
OSHA 29 CFR 1910.178(q)(7) – Examination before service
OSHA 29 CFR 1910.178(p)(1) – Defective trucks out of service
ANSI/ITSDF B56.1 – Safety standard for low-level and high-level loaders
OSHA – Powered industrial trucks eTool
Verify the current edition and local adoption before use.
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
