InspectionReport
Heavy Equipment Daily Pre-Shift Inspection Template
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
Jurisdiction: US. OSHA 29 CFR 1926.601 and 1926.602 are US construction standards. Adaptable to other jurisdictions with equivalent heavy equipment regulations.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Inspection header
	Field
	Entry

	Equipment type (excavator / backhoe / bulldozer / wheel loader / articulated truck)
	________________________________________________

	Equipment ID / serial number
	________________________________________________

	Operator name
	________________________________________________

	Date and shift
	________________________________________________


5-Point visual walkaround (engine off)
	Item
	Pass
	Fail
	N/A
	Notes

	Ground Engaging Tools (bucket teeth, cutting edges, rippers): missing bolts, excessive wear
	☐
	☐
	☐
	____________________

	Undercarriage and tires: track tension, missing pads, tire pressure, deep sidewall cuts
	☐
	☐
	☐
	____________________

	Hydraulic system: puddles under machine, cylinder abrasions, hose leaks or crimps
	☐
	☐
	☐
	____________________

	ROPS and safety structures: no cracks or unauthorized welds
	☐
	☐
	☐
	____________________

	Visibility aids: windows clean, mirrors intact, backup cameras functional
	☐
	☐
	☐
	____________________


4-Point operational test (engine on)
	Item
	Pass
	Fail
	N/A
	Notes

	Braking and steering: service brakes, parking brake, emergency stop; steering turns fully and smoothly
	☐
	☐
	☐
	____________________

	Safety alarms and horns: horn sounds, backup alarm automatic and audible over site noise
	☐
	☐
	☐
	____________________

	Operating controls: boom up/down, bucket curl, blade angle – responsive, not sluggish or jerky
	☐
	☐
	☐
	____________________

	Seat belts: latches securely and retracts properly
	☐
	☐
	☐
	____________________


Equipment-specific focus
	Item
	Pass
	Fail
	N/A
	Notes

	Excavators / backhoes: boom cylinders, bucket teeth, swing gear lubrication
	☐
	☐
	☐
	____________________

	Bulldozers / graders: blade condition, track tension, ripper shanks
	☐
	☐
	☐
	____________________

	Wheel loaders: tire pressure/condition, articulation joint play
	☐
	☐
	☐
	____________________

	Articulated trucks: dump bed hydraulics, tailgate function, air brakes
	☐
	☐
	☐
	____________________


Defective machinery handling
	Item
	Pass
	Fail
	N/A
	Notes

	Engine turned off, key removed
	☐
	☐
	☐
	____________________

	'Do Not Operate' tag attached
	☐
	☐
	☐
	____________________

	Site superintendent / lead mechanic notified
	☐
	☐
	☐
	____________________

	Operator signature
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
References consulted
OSHA 29 CFR 1926.601 – Motor vehicles
OSHA 29 CFR 1926.602 – Material handling equipment
OSHA 1926.601(b)(14) – Daily inspection requirement
Verify the current edition and local adoption before use.
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
