InspectionReport
Critical Heavy Lift Rigging Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Sling Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Verify each sling has a legible sling tag indicating its rated capacity, sling angle, and serial number. (ASME B30.9)
	☐
	☐
	☐
	____________________

	Confirm sling material is compatible with the load and environmental conditions (e.g., temperature, chemicals). (ASME B30.9)
	☐
	☐
	☐
	____________________

	Inspect slings for cuts, abrasions, and other damage that could compromise their strength. (ASME B30.9)
	☐
	☐
	☐
	____________________

	Examine wire rope slings for kinks, crushing, bird caging, or other distortions. (ASME B30.9)
	☐
	☐
	☐
	____________________

	Check synthetic slings for chemical damage, burns, or melting. (ASME B30.9)
	☐
	☐
	☐
	____________________

	Verify sling end fittings (e.g., eyes, hooks) are properly attached and free from cracks or deformation. (ASME B30.9)
	☐
	☐
	☐
	____________________

	Measure sling stretch/elongation. Remove from service if exceeding manufacturer's recommendations. (ASME B30.9)
	☐
	☐
	☐
	____________________

	Ensure all sling hardware (shackles, hooks) are of the correct size and rated capacity for the sling. (ASME B30.10)
	☐
	☐
	☐
	____________________

	Verify slings are stored properly, protected from damage, moisture, and extreme temperatures. (ASME B30.9)
	☐
	☐
	☐
	____________________

	Confirm slings are inspected regularly (daily before use) and documented. (ASME B30.9)
	☐
	☐
	☐
	____________________


Shackle Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Verify each shackle has a legible WLL (Working Load Limit) stamped on the body. (ASME B30.26)
	☐
	☐
	☐
	____________________

	Confirm the correct type of shackle pin is used (e.g., screw pin, bolt-type with nut and cotter pin). (ASME B30.26)
	☐
	☐
	☐
	____________________

	Ensure the shackle pin is fully engaged and properly secured. (ASME B30.26)
	☐
	☐
	☐
	____________________

	Inspect shackle body for deformation, cracks, or wear. (ASME B30.26)
	☐
	☐
	☐
	____________________

	Verify the shackle pin is straight and not bent or damaged. (ASME B30.26)
	☐
	☐
	☐
	____________________

	Check shackle threads for damage or corrosion. (ASME B30.26)
	☐
	☐
	☐
	____________________

	Ensure the shackle is loaded correctly, avoiding side loading or three-point loading. (ASME B30.26)
	☐
	☐
	☐
	____________________

	Verify shackles are properly sized for the mating hardware (e.g., sling eyes, lifting lugs). (ASME B30.26)
	☐
	☐
	☐
	____________________

	Inspect shackles for excessive corrosion that could reduce their strength. (ASME B30.26)
	☐
	☐
	☐
	____________________

	Confirm shackles are from a reputable manufacturer and meet recognized standards. (ASME B30.26)
	☐
	☐
	☐
	____________________


Spreader Bar Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Verify the spreader bar has a legible WLL (Working Load Limit) clearly marked. (ASME B30.20)
	☐
	☐
	☐
	____________________

	Confirm the spreader bar design is appropriate for the lift (e.g., adjustable, fixed length). (ASME B30.20)
	☐
	☐
	☐
	____________________

	Inspect the spreader bar for any signs of bending, buckling, or deformation. (ASME B30.20)
	☐
	☐
	☐
	____________________

	Examine all welds on the spreader bar for cracks, porosity, or other defects. (AWS D1.1)
	☐
	☐
	☐
	____________________

	Verify the end connections (e.g., lifting lugs, padeyes) are securely attached and free from damage. (ASME B30.20)
	☐
	☐
	☐
	____________________

	Ensure all hardware used with the spreader bar (e.g., shackles, slings) are compatible and properly rated. (ASME B30.20)
	☐
	☐
	☐
	____________________

	If adjustable, verify the adjustment mechanism is functioning correctly and securely locked in place. (ASME B30.20)
	☐
	☐
	☐
	____________________

	Confirm the load is evenly distributed across the spreader bar. (ASME B30.20)
	☐
	☐
	☐
	____________________

	Inspect the spreader bar for adequate corrosion protection (e.g., paint, galvanizing). (ASME B30.20)
	☐
	☐
	☐
	____________________

	Verify the spreader bar has documentation including load charts and inspection records. (ASME B30.20)
	☐
	☐
	☐
	____________________


Load & Lift Planning
	Item
	Pass
	Fail
	N/A
	Notes

	Verify the load weight is accurately determined and documented. (OSHA 1926.753)
	☐
	☐
	☐
	____________________

	Confirm the center of gravity (CG) of the load has been accurately calculated and marked. (ASME B30.9)
	☐
	☐
	☐
	____________________

	Ensure a detailed rigging plan is available and understood by all personnel involved in the lift. (OSHA 1926.753)
	☐
	☐
	☐
	____________________

	Verify the lift radius is clear of obstructions and personnel. (OSHA 1926.753)
	☐
	☐
	☐
	____________________

	Assess environmental conditions (wind speed, temperature) and adjust the lift plan accordingly. (ASME B30.5)
	☐
	☐
	☐
	____________________

	Confirm the crane is properly leveled and supported. (OSHA 1926.1402)
	☐
	☐
	☐
	____________________

	Establish a clear communication protocol between the crane operator, rigger, and signal person. (OSHA 1926.753)
	☐
	☐
	☐
	____________________

	Verify all personnel involved in the lift are qualified and trained for their respective roles. (OSHA 1926.753)
	☐
	☐
	☐
	____________________

	Confirm emergency procedures are in place and understood by all personnel. (OSHA 1926.753)
	☐
	☐
	☐
	____________________

	Assess the ground bearing capacity and ensure it is adequate to support the crane and load. (OSHA 1926.1402)
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
