InspectionReport
Home Safety Checklist - Residential Hazard & Fire Safety Check
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Fire Alarm & Detection
	Item
	Pass
	Fail
	N/A
	Notes

	Smoke alarms installed on every level of the home, outside each sleeping area, and inside each bedroom, as required by NFPA 71.
	☐
	☐
	☐
	____________________

	Each smoke alarm is within its 10-year service life (check the manufacture date on the back). Replace any unit older than 10 years.
	☐
	☐
	☐
	____________________

	Press the test button on every smoke alarm. The alarm should sound clearly. Replace any unit that does not activate.
	☐
	☐
	☐
	____________________

	Carbon monoxide (CO) alarms installed on every level of the home, outside each sleeping area, as required by NFPA 1.
	☐
	☐
	☐
	____________________

	Press the test button on every CO alarm. The alarm should sound. Replace any unit that does not activate or is past its service life.
	☐
	☐
	☐
	____________________

	Battery-powered alarms have fresh batteries. Replace batteries at least twice a year and whenever the low-battery chirp sounds.
	☐
	☐
	☐
	____________________


Electrical Safety
	Item
	Pass
	Fail
	N/A
	Notes

	The electrical service panel cover is in place, undamaged, and not obstructed. Keep at least 36 inches of clear working space in front of the panel.
	☐
	☐
	☐
	____________________

	Every circuit breaker is labeled so you can identify what it controls. Unlabeled breakers make it hard to isolate a circuit safely.
	☐
	☐
	☐
	____________________

	GFCI (ground-fault circuit interrupter) outlets are installed in kitchens, bathrooms, garages, basements, and outdoors. Test the GFCI button; the outlet should cut power.
	☐
	☐
	☐
	____________________

	AFCI (arc-fault circuit interrupter) protection is present on bedroom and living-area circuits, as required by the National Electrical Code for most residential wiring.
	☐
	☐
	☐
	____________________

	Extension cords and appliance cords are not cut, frayed, or overloaded. Do not use damaged cords. Replace any cord with exposed wiring.
	☐
	☐
	☐
	____________________

	Portable space heaters are at least 3 feet away from curtains, bedding, furniture, and other combustibles. Heaters are turned off when leaving the room or going to sleep.
	☐
	☐
	☐
	____________________


Gas & Water Heaters
	Item
	Pass
	Fail
	N/A
	Notes

	No gas odor near the gas meter, furnace, water heater, or gas appliances. If you smell gas, leave the home and call the gas company or 911 from outside.
	☐
	☐
	☐
	____________________

	The gas shutoff valve is accessible, labeled, and in the ON position when the appliance is in use. Know where it is before you need it.
	☐
	☐
	☐
	____________________

	The water heater temperature and pressure (T&P) relief valve is not capped, blocked, or painted over. The discharge pipe runs to a safe location (floor drain or within 6 feet of a floor).
	☐
	☐
	☐
	____________________

	The water heater is within its expected service life (typically 8-12 years for a tank unit). Older units are more likely to leak or fail.
	☐
	☐
	☐
	____________________


Water, Drainage & Mold
	Item
	Pass
	Fail
	N/A
	Notes

	No active leaks at faucets, shower valves, toilet bases, water heater connections, or under sinks. Fix drips promptly to prevent water damage and mold.
	☐
	☐
	☐
	____________________

	Ground around the foundation slopes away from the house so rainwater does not collect against the walls. Check for standing water after heavy rain.
	☐
	☐
	☐
	____________________

	No visible mold, water stains, or musty odor in bathrooms, kitchens, basements, or around windows. Persistent moisture is a mold risk.
	☐
	☐
	☐
	____________________

	Crawlspace or basement is dry and ventilated. Check for condensation on pipes, joists, or foundation walls, which indicates a moisture problem.
	☐
	☐
	☐
	____________________


Falls & Physical Hazards
	Item
	Pass
	Fail
	N/A
	Notes

	Stair handrails are secure and continuous on at least one side of every flight. Check that rails do not wobble when you apply pressure.
	☐
	☐
	☐
	____________________

	Carpet on stairs is not curled, loose, or worn through. Loose stair carpet is a trip and fall hazard, especially for children and older adults.
	☐
	☐
	☐
	____________________

	Bathtubs and shower floors have non-slip surfaces or mats. Check that mats are clean, not mildewed, and do not shift when wet.
	☐
	☐
	☐
	____________________

	Walking surfaces in hallways, kitchens, and entryways are clear of clutter, cords, and loose rugs. Rugs that must stay in place should have a non-slip pad.
	☐
	☐
	☐
	____________________

	Lighting is adequate in hallways, stairways, kitchens, and bathrooms. Replace burnt-out bulbs. Consider motion-sensor lights for nighttime paths.
	☐
	☐
	☐
	____________________


Fire Escape & Preparedness
	Item
	Pass
	Fail
	N/A
	Notes

	Every bedroom has at least two ways to exit (a door and a window that opens). Windows are not painted shut or blocked by furniture.
	☐
	☐
	☐
	____________________

	A written or posted fire escape plan exists for the household. Every occupant knows the two exit routes from each room and the meeting point outside.
	☐
	☐
	☐
	____________________

	A rated fire extinguisher (at least 2A:10B:C) is available in the kitchen or near the stove. The pin is in place, the gauge is in the green, and the unit is within its service life.
	☐
	☐
	☐
	____________________

	Smoke alarms are tested monthly (press the test button) and batteries are replaced at least twice a year. This is a household habit, not a one-time task.
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
