InspectionReport
Industrial Sandblasting & Surface Prep Safety Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Respiratory Protection & Air Quality
	Item
	Pass
	Fail
	N/A
	Notes

	Is current fit test documentation (within 12 months) available for each abrasive blasting operator using a supplied air respirator? (OSHA 1910.134(f))
	☐
	☐
	☐
	____________________

	Inspect Supplied Air Respirator (SAR) hoses for cuts, kinks, abrasions, and secure connections before each shift. (ANSI Z9.4)
	☐
	☐
	☐
	____________________

	Verify air compressor maintenance records are up-to-date, including filter changes and inspections. (Manufacturer's Recommendations)
	☐
	☐
	☐
	____________________

	Has the supplied air been tested within the last 6 months for contaminants (oil, water, carbon monoxide) and is the air Grade D or better? (OSHA 1910.134(i)(1)(ii))
	☐
	☐
	☐
	____________________

	Is a continuous carbon monoxide (CO) monitor with audible alarm functioning correctly and positioned to detect CO in the supplied air? (OSHA 1926.57(g)(1)(i))
	☐
	☐
	☐
	____________________

	Are respirators cleaned and disinfected after each use, and properly stored to prevent damage and contamination? (OSHA 1910.134(h)(1))
	☐
	☐
	☐
	____________________

	Is the air pressure at the respirator sufficient to meet the manufacturer's specifications and the operator's needs? (Check with a pressure gauge at the respirator).
	☐
	☐
	☐
	____________________

	Is there a backup air supply available in case of primary compressor failure? (Recommended Best Practice)
	☐
	☐
	☐
	____________________

	Inspect air-line filters for condition and ensure they are appropriate for removing oil, water, and particulates. (Manufacturer's Specifications)
	☐
	☐
	☐
	____________________

	Check the respirator exhalation valve for proper function and cleanliness. (OSHA 1910.134)
	☐
	☐
	☐
	____________________


Abrasive Blasting Equipment & Controls
	Item
	Pass
	Fail
	N/A
	Notes

	Verify the deadman switch is functioning correctly: nozzle stops immediately when the handle is released. (OSHA 1926.57(c)(1))
	☐
	☐
	☐
	____________________

	Inspect blast hose for cuts, bulges, abrasions, and secure couplings before each shift. (OSHA 1926.302(b)(4))
	☐
	☐
	☐
	____________________

	Check nozzle for wear and proper size. Replace if worn beyond manufacturer's specifications. (Manufacturer's Recommendations)
	☐
	☐
	☐
	____________________

	Ensure the abrasive blasting pot is equipped with a functional pressure relief valve. (ASME Boiler and Pressure Vessel Code)
	☐
	☐
	☐
	____________________

	Are hose whip checks installed and properly secured on all blast hoses to prevent whipping in case of coupling failure? (Recommended Best Practice)
	☐
	☐
	☐
	____________________

	If using a remote control system, verify it is functioning correctly and properly grounded. (OSHA 1926.302)
	☐
	☐
	☐
	____________________

	Verify the abrasive being used is the correct type for the application and does not contain free silica above permissible limits if silica is prohibited. (SDS Review)
	☐
	☐
	☐
	____________________

	Inspect the blast pot for leaks, corrosion, and structural integrity. (Manufacturer's Recommendations)
	☐
	☐
	☐
	____________________

	Confirm the blast pressure is set according to the manufacturer's recommendations and the specific task requirements. (Manufacturer's Recommendations)
	☐
	☐
	☐
	____________________

	Verify grounding continuity between the blast pot, nozzle, and workpiece to prevent static discharge. (NFPA 77)
	☐
	☐
	☐
	____________________


Blast Booth & Containment
	Item
	Pass
	Fail
	N/A
	Notes

	Verify the blast booth ventilation system is operating effectively and maintaining adequate air flow to remove dust and contaminants. (ACGIH Industrial Ventilation Manual)
	☐
	☐
	☐
	____________________

	Check dust collector filters and ensure they are clean and functioning properly. (Manufacturer's Recommendations)
	☐
	☐
	☐
	____________________

	Inspect blast booth walls, doors, and seals for damage or leaks that could allow dust to escape. (Good Engineering Practices)
	☐
	☐
	☐
	____________________

	Ensure the blast booth is properly grounded to prevent static discharge. (NFPA 77)
	☐
	☐
	☐
	____________________

	Verify all lighting within the blast booth is explosion-proof and properly maintained. (NFPA 70)
	☐
	☐
	☐
	____________________

	Maintain good housekeeping practices within the blast booth to minimize dust accumulation. (General Industry Standards)
	☐
	☐
	☐
	____________________

	Conduct air monitoring outside the blast booth to ensure dust levels are within permissible exposure limits (PELs). (OSHA 1910.1000)
	☐
	☐
	☐
	____________________

	Verify proper procedures are in place for the collection, storage, and disposal of spent abrasive material. (Local Environmental Regulations)
	☐
	☐
	☐
	____________________

	Ensure appropriate warning signs and barriers are in place to restrict access to the blasting area. (ANSI Z535)
	☐
	☐
	☐
	____________________

	Verify the blast booth has a readily accessible emergency shutdown switch. (Recommended Best Practice)
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Confirm all personnel within the blasting area are wearing appropriate PPE, including supplied air respirators, hearing protection, eye protection, and protective clothing. (OSHA 1910.132)
	☐
	☐
	☐
	____________________

	Operators perform a positive and negative pressure seal check on their respirators before each use. (OSHA 1910.134)
	☐
	☐
	☐
	____________________

	Verify hearing protection has an appropriate Noise Reduction Rating (NRR) for the noise levels in the blasting area. (OSHA 1910.95)
	☐
	☐
	☐
	____________________

	Ensure eye protection (safety glasses or face shield) is ANSI Z87.1 compliant and provides adequate protection from abrasive particles. (ANSI Z87.1)
	☐
	☐
	☐
	____________________

	Inspect protective clothing (e.g., leather or canvas suits) for damage and ensure it provides adequate coverage. (Recommended Best Practice)
	☐
	☐
	☐
	____________________

	Inspect gloves for holes, tears, and wear. Ensure they provide adequate protection from abrasion and impact. (OSHA 1910.138)
	☐
	☐
	☐
	____________________

	Verify foot protection (safety shoes or boots) meets ANSI Z41 standards and provides adequate protection from impact and compression. (ANSI Z41)
	☐
	☐
	☐
	____________________

	Are procedures in place for cleaning and maintaining PPE to ensure its effectiveness? (OSHA 1910.132)
	☐
	☐
	☐
	____________________

	PPE is stored properly to prevent damage and contamination. (OSHA 1910.132)
	☐
	☐
	☐
	____________________

	If required, is a communication system in place and functioning properly to allow operators to communicate with personnel outside the blasting area? (Recommended Best Practice)
	☐
	☐
	☐
	____________________


Documentation & Training
	Item
	Pass
	Fail
	N/A
	Notes

	Is a written hazard communication program in place, including Safety Data Sheets (SDS) for all materials used? (OSHA 1910.1200)
	☐
	☐
	☐
	____________________

	Verify employee training records are up-to-date, including training on abrasive blasting hazards, PPE use, and safe operating procedures. (OSHA 1926.21)
	☐
	☐
	☐
	____________________

	Are SDS readily available to all employees in the blasting area? (OSHA 1910.1200)
	☐
	☐
	☐
	____________________

	Is a written abrasive blasting procedure available and followed? (Recommended Best Practice)
	☐
	☐
	☐
	____________________

	Is a written emergency action plan in place, including procedures for fire, medical emergencies, and equipment failure? (OSHA 1910.38)
	☐
	☐
	☐
	____________________

	Is a first-aid kit readily available and adequately stocked? (OSHA 1910.151)
	☐
	☐
	☐
	____________________

	Are records of equipment inspections and maintenance kept and readily available? (Recommended Best Practice)
	☐
	☐
	☐
	____________________

	Are air quality test results documented and readily available? (OSHA 1910.134)
	☐
	☐
	☐
	____________________

	If blasting in a confined space, is a confined space entry permit system in place and followed? (OSHA 1910.146)
	☐
	☐
	☐
	____________________

	Is a Job Hazard Analysis (JHA) or Task Hazard Assessment (THA) completed for the specific blasting task? (Recommended Best Practice)
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
