InspectionReport
Commercial Landscaping Mower & Edger Pre-Use Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Mower & Edger - General Condition
	Item
	Pass
	Fail
	N/A
	Notes

	Is the mower/edger free of excessive dirt, debris, and grease? (Reduces fire hazard and improves visibility)
	☐
	☐
	☐
	____________________

	Inspect for fuel or oil leaks. Are any leaks present around the engine, fuel lines, or hydraulic systems?
	☐
	☐
	☐
	____________________

	Examine tires for proper inflation, cuts, bulges, or excessive wear. (Mowers only)
	☐
	☐
	☐
	____________________

	Inspect mower/edger blades for sharpness, cracks, bends, or excessive wear. Are blades properly balanced?
	☐
	☐
	☐
	____________________

	Verify that all nuts, bolts, and screws are securely tightened. Pay special attention to blade mounting hardware.
	☐
	☐
	☐
	____________________

	Check engine oil, hydraulic fluid (if applicable), and coolant levels. Are levels within the recommended range?
	☐
	☐
	☐
	____________________

	Inspect the air filter for cleanliness. Is the air filter clean and properly installed?
	☐
	☐
	☐
	____________________

	Is a spark arrestor present and in good condition (if required by local regulations)?
	☐
	☐
	☐
	____________________

	Inspect battery terminals for corrosion and ensure connections are tight. (Electric start models)
	☐
	☐
	☐
	____________________

	Verify the starter operates smoothly and the engine starts readily. (Electric start models)
	☐
	☐
	☐
	____________________


Safety Guards & Shields
	Item
	Pass
	Fail
	N/A
	Notes

	Is the mower discharge chute guard securely in place and undamaged? (Mowers only)
	☐
	☐
	☐
	____________________

	Is the edger blade guard properly installed and free from damage? (Edgers only)
	☐
	☐
	☐
	____________________

	If the mower is PTO-driven, is the PTO shaft properly shielded and in good condition?
	☐
	☐
	☐
	____________________

	Are all belt guards and shields in place and securely fastened?
	☐
	☐
	☐
	____________________

	Are pinch point guards (if equipped) properly installed and functional?
	☐
	☐
	☐
	____________________

	Inspect deflectors for damage or missing parts. Are they securely attached?
	☐
	☐
	☐
	____________________

	If equipped with a rear discharge, is the guard in place and undamaged?
	☐
	☐
	☐
	____________________

	If equipped with a side discharge, is the guard in place and undamaged?
	☐
	☐
	☐
	____________________


Controls & Safety Devices
	Item
	Pass
	Fail
	N/A
	Notes

	Verify the deadman switch (operator presence control) functions correctly. Does the engine/blades stop immediately when released?
	☐
	☐
	☐
	____________________

	Test the brakes (if equipped) for proper function. Do the brakes engage smoothly and effectively?
	☐
	☐
	☐
	____________________

	Ensure the throttle control operates smoothly and returns to idle position properly.
	☐
	☐
	☐
	____________________

	Verify steering is responsive and free from excessive play. (Mowers only)
	☐
	☐
	☐
	____________________

	Test reverse operation (if equipped). Does the mower move smoothly and safely in reverse?
	☐
	☐
	☐
	____________________

	Check all interlock systems (e.g., seat switch, blade engagement). Are they functioning correctly?
	☐
	☐
	☐
	____________________

	Verify the blade engagement mechanism operates smoothly and engages/disengages the blades properly.
	☐
	☐
	☐
	____________________

	If equipped, test the emergency stop switch. Does it immediately shut down the engine/blades?
	☐
	☐
	☐
	____________________


Rollover Protection (Mowers)
	Item
	Pass
	Fail
	N/A
	Notes

	If equipped with a Rollover Protection Structure (ROPS), inspect for damage (bends, cracks, corrosion).
	☐
	☐
	☐
	____________________

	Verify the ROPS is securely mounted to the mower frame with all original hardware.
	☐
	☐
	☐
	____________________

	If equipped with a seatbelt, inspect for wear, fraying, or damage. Ensure it buckles and unbuckles properly.
	☐
	☐
	☐
	____________________

	Verify the seatbelt is securely mounted to the seat frame.
	☐
	☐
	☐
	____________________

	Ensure proper tire pressure is maintained as specified by the manufacturer. (Affects ROPS effectiveness)
	☐
	☐
	☐
	____________________

	If wheel spacers are used, verify they are properly installed and of the correct type.
	☐
	☐
	☐
	____________________

	If ballast is used, verify it is properly installed and secured.
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Are appropriate eye protection (safety glasses or face shield) readily available and in good condition?
	☐
	☐
	☐
	____________________

	Is hearing protection (earplugs or earmuffs) readily available and in good condition?
	☐
	☐
	☐
	____________________

	Are appropriate work gloves available and in good condition?
	☐
	☐
	☐
	____________________

	Are appropriate safety shoes or boots (steel-toe recommended) being worn?
	☐
	☐
	☐
	____________________

	Are chaps or other leg protection being used when operating edgers?
	☐
	☐
	☐
	____________________

	Is high-visibility clothing (vest or shirt) being worn, especially in areas with vehicular traffic?
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
