InspectionReport
Loading Dock Safety & Vehicle Restraint Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Vehicle Restraint System Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Verify vehicle restraint engages ICC bar securely on 100% of trailers.
	☐
	☐
	☐
	____________________

	Inspect vehicle restraint for any signs of damage (cracks, bends, corrosion).
	☐
	☐
	☐
	____________________

	If hydraulic, check hydraulic pressure gauge against manufacturer specifications.
	☐
	☐
	☐
	____________________

	Inspect all electrical connections for tightness and proper insulation.
	☐
	☐
	☐
	____________________

	Test communication system (lights, alarms) between dock worker and truck driver.
	☐
	☐
	☐
	____________________

	Verify manual release mechanism functions smoothly and is easily accessible.
	☐
	☐
	☐
	____________________

	Review maintenance records to ensure regular inspections and servicing are up-to-date.
	☐
	☐
	☐
	____________________

	Confirm warning signage is clear, visible, and in good condition.
	☐
	☐
	☐
	____________________

	Inspect wheel chocks for damage and proper placement during use.
	☐
	☐
	☐
	____________________

	If equipped, verify interlock system prevents dock leveler operation when restraint is not engaged.
	☐
	☐
	☐
	____________________


Dock Leveler Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Inspect dock leveler plate for cracks, bends, or excessive wear.
	☐
	☐
	☐
	____________________

	Verify dock leveler lip extends and retracts smoothly and fully.
	☐
	☐
	☐
	____________________

	Check for hydraulic leaks around cylinders and hoses.
	☐
	☐
	☐
	____________________

	Ensure toe guards are in place and functioning correctly to prevent foot injuries.
	☐
	☐
	☐
	____________________

	Verify the leveler's capacity rating is clearly marked and not exceeded.
	☐
	☐
	☐
	____________________

	Review maintenance log for scheduled inspections and repairs.
	☐
	☐
	☐
	____________________

	Confirm operating instructions are posted and easily accessible to users.
	☐
	☐
	☐
	____________________

	Inspect return springs for proper tension and function.
	☐
	☐
	☐
	____________________

	Identify and guard against potential pinch points during leveler operation.
	☐
	☐
	☐
	____________________

	If equipped, ensure safety legs are engaged during maintenance or when the leveler is not in use.
	☐
	☐
	☐
	____________________


Communication and Signaling Systems
	Item
	Pass
	Fail
	N/A
	Notes

	Verify red/green light signals are functioning correctly and visible to both driver and dock worker.
	☐
	☐
	☐
	____________________

	Test audible horn or alarm system to ensure it is loud enough to be heard above ambient noise.
	☐
	☐
	☐
	____________________

	If equipped, test intercom system for clear communication between dock and truck.
	☐
	☐
	☐
	____________________

	Ensure all warning and instructional signage is clear, legible, and properly positioned.
	☐
	☐
	☐
	____________________

	Verify emergency stop buttons are easily accessible and functioning correctly.
	☐
	☐
	☐
	____________________

	Confirm drivers are properly notified of loading/unloading procedures and safety protocols.
	☐
	☐
	☐
	____________________

	Verify dock workers are trained on proper communication procedures and signaling systems.
	☐
	☐
	☐
	____________________

	Confirm dock workers are proficient in using standard hand signals for communication.
	☐
	☐
	☐
	____________________

	Review established communication protocols for loading and unloading operations.
	☐
	☐
	☐
	____________________

	If used, inspect glad hand locks for proper installation and functionality to prevent unauthorized trailer movement.
	☐
	☐
	☐
	____________________


Environmental Conditions & Housekeeping
	Item
	Pass
	Fail
	N/A
	Notes

	Inspect dock door seals for damage and proper sealing to prevent drafts and maintain temperature control.
	☐
	☐
	☐
	____________________

	Verify adequate lighting is provided inside the trailer and on the dock area.
	☐
	☐
	☐
	____________________

	Inspect dock floor for cracks, holes, or uneven surfaces that could create tripping hazards.
	☐
	☐
	☐
	____________________

	Ensure drainage system is clear and functioning properly to prevent water accumulation.
	☐
	☐
	☐
	____________________

	Implement a snow and ice removal plan to maintain safe walking and working surfaces during winter months.
	☐
	☐
	☐
	____________________

	Maintain a pest control program to prevent infestations that could create unsanitary conditions.
	☐
	☐
	☐
	____________________

	Ensure proper waste disposal containers are available and used to maintain a clean work area.
	☐
	☐
	☐
	____________________

	Verify aisles and walkways are clear of obstructions to allow for safe movement of personnel and equipment.
	☐
	☐
	☐
	____________________

	Maintain spill control materials and procedures to address potential spills of hazardous materials.
	☐
	☐
	☐
	____________________

	If applicable, inspect ventilation system to ensure proper air circulation and removal of fumes.
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Verify all dock workers are wearing high-visibility clothing (ANSI 107 Class 2 or 3).
	☐
	☐
	☐
	____________________

	Ensure all dock workers are wearing steel-toe safety boots meeting ASTM F2413 standards.
	☐
	☐
	☐
	____________________

	Confirm safety glasses or face shields are worn when performing tasks that could result in eye injuries.
	☐
	☐
	☐
	____________________

	Verify gloves are appropriate for the task being performed (e.g., cut-resistant, chemical-resistant).
	☐
	☐
	☐
	____________________

	Ensure hearing protection is available and used in areas with high noise levels (above 85 dBA).
	☐
	☐
	☐
	____________________

	Confirm hard hats are worn in areas where there is a risk of head injury from falling objects.
	☐
	☐
	☐
	____________________

	Inspect PPE for damage or wear before each use.
	☐
	☐
	☐
	____________________

	Verify dock workers are trained on the proper use, care, and maintenance of PPE.
	☐
	☐
	☐
	____________________

	Ensure adequate supply of PPE is readily available to all dock workers.
	☐
	☐
	☐
	____________________

	If required, verify proper respiratory protection is used and fit-tested.
	☐
	☐
	☐
	____________________


Forklift and Mobile Equipment Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Verify forklift has been inspected daily using a pre-shift checklist (Form 2551).
	☐
	☐
	☐
	____________________

	Ensure all forklift operators are properly trained and certified.
	☐
	☐
	☐
	____________________

	Test forklift horn to ensure it is functioning correctly.
	☐
	☐
	☐
	____________________

	Verify forklift headlights and taillights are functioning correctly.
	☐
	☐
	☐
	____________________

	Ensure forklift operators are wearing seatbelts at all times.
	☐
	☐
	☐
	____________________

	Enforce speed limits for forklifts in the dock area.
	☐
	☐
	☐
	____________________

	Ensure pedestrians are aware of forklift traffic and maintain a safe distance.
	☐
	☐
	☐
	____________________

	Verify forklift load capacity is not exceeded.
	☐
	☐
	☐
	____________________

	Ensure proper fueling procedures are followed for forklifts.
	☐
	☐
	☐
	____________________

	Verify forklifts are parked in designated areas when not in use.
	☐
	☐
	☐
	____________________

	If electric, inspect battery connections for corrosion and damage.
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
