InspectionReport
MEWP Pre-Use Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
Jurisdiction: Adaptable. Covers OSHA (US), PUWER and LOLER (UK), and national work-equipment rules. Adaptable to any jurisdiction with MEWP regulations. Apply only the section and thresholds for the governing jurisdiction; do not combine US and UK requirements as if they were one code.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Inspection header
	Field
	Entry

	Machine type (scissor lift / boom lift / cherry picker)
	________________________________________________

	Machine ID / serial number
	________________________________________________

	Operator / inspector name
	________________________________________________

	Date and shift
	________________________________________________


Zone 1: Ground / visual inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Hydraulic systems: no active leaks, weeping fluid, or bulging hoses
	☐
	☐
	☐
	____________________

	Tires and wheels: no chunking, missing lug nuts, adequate pressure
	☐
	☐
	☐
	____________________

	Structural welds: no cracked welds, rust, or noticeable deflection
	☐
	☐
	☐
	____________________

	Fluid levels: engine oil, hydraulic fluid, coolant, battery water at manufacturer specs
	☐
	☐
	☐
	____________________


Zone 2: Lower controls
	Item
	Pass
	Fail
	N/A
	Notes

	Emergency stop: cuts power instantly
	☐
	☐
	☐
	____________________

	Base control panel: all switches functional
	☐
	☐
	☐
	____________________

	Emergency lowering system: platform lowers without main engine power
	☐
	☐
	☐
	____________________

	Warning decals: present and legible
	☐
	☐
	☐
	____________________


Zone 3: Upper controls
	Item
	Pass
	Fail
	N/A
	Notes

	Platform: no structural damage
	☐
	☐
	☐
	____________________

	Guardrails and mid-rails: present, secure, no damage
	☐
	☐
	☐
	____________________

	Lanyard anchor points: present and undamaged
	☐
	☐
	☐
	____________________

	Tilt alarm: tested per manufacturer procedure
	☐
	☐
	☐
	____________________


Functional safety tests
	Item
	Pass
	Fail
	N/A
	Notes

	Limit switches: pothole guards (scissor lifts), boom extension limits
	☐
	☐
	☐
	____________________

	Horn and beacons: horn sounds clearly, warning lights flash
	☐
	☐
	☐
	____________________

	Operating controls: all functions responsive, no binding
	☐
	☐
	☐
	____________________


Defect action
	Item
	Pass
	Fail
	N/A
	Notes

	Defect description
	☐
	☐
	☐
	____________________

	Operation stopped: Yes / No
	☐
	☐
	☐
	____________________

	Key removed from lower control panel
	☐
	☐
	☐
	____________________

	'Out of Service' tag placed on control box
	☐
	☐
	☐
	____________________

	Site supervisor notified
	☐
	☐
	☐
	____________________

	Inspector signature
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
References consulted
OSHA 29 CFR 1910.67 – Aerial lifts
OSHA 29 CFR 1926.453 – Aerial lifts
ANSI/SAIA A92 – Mobile elevating work platforms
UK HSE – MEWPs (L113)
Verify the current edition and local adoption before use.
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
