InspectionReport
Rotary Piling Rig Safety Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Working Platform & Ground Stability
	Item
	Pass
	Fail
	N/A
	Notes

	Has a geotechnical engineer certified the working platform's ground bearing pressure is adequate for the rig's maximum operating weight (including Kelly bar, auger, and spoil)?
	☐
	☐
	☐
	____________________

	Is a daily visual inspection of the working platform performed to check for settlement, cracks, or water accumulation? Documented in daily log?
	☐
	☐
	☐
	____________________

	Is the working platform adequately sloped to ensure proper drainage and prevent water pooling near the rig's tracks or outriggers?
	☐
	☐
	☐
	____________________

	Are outriggers (if used) fully extended and placed on stable, load-distributing pads of sufficient size to prevent sinking or movement?
	☐
	☐
	☐
	____________________

	Is there a system in place to monitor groundwater levels and their potential impact on platform stability? Are dewatering measures in place if needed?
	☐
	☐
	☐
	____________________

	Are slopes surrounding the working platform stable and protected from erosion or collapse that could undermine the platform?
	☐
	☐
	☐
	____________________

	Is vibration monitoring being conducted to assess the impact of rig operations on nearby structures or utilities?
	☐
	☐
	☐
	____________________

	Are access and egress routes to the working platform clear, stable, and free from obstructions?
	☐
	☐
	☐
	____________________

	Is the working platform constructed with properly compacted materials to achieve the required ground bearing pressure?
	☐
	☐
	☐
	____________________

	Has the working platform stability been reassessed following significant rainfall or other adverse weather conditions?
	☐
	☐
	☐
	____________________


Wire Rope & Lifting Equipment
	Item
	Pass
	Fail
	N/A
	Notes

	Are wire ropes inspected daily for wear, corrosion, kinks, and broken wires, with results documented in a logbook?
	☐
	☐
	☐
	____________________

	Are wire ropes replaced when they exhibit excessive wear, corrosion, or the number of broken wires exceeds the manufacturer's recommendations?
	☐
	☐
	☐
	____________________

	Are sheaves and drums inspected for wear, cracks, and proper lubrication to prevent damage to wire ropes?
	☐
	☐
	☐
	____________________

	Are all lifting gear (slings, shackles, hooks) certified and inspected regularly, with valid documentation available on site?
	☐
	☐
	☐
	____________________

	Are hook safety latches functioning correctly and in place on all lifting hooks?
	☐
	☐
	☐
	____________________

	Is there a documented lubrication program for wire ropes and lifting equipment, using the manufacturer's recommended lubricants?
	☐
	☐
	☐
	____________________

	Is the wire rope reeving system properly installed and maintained according to the rig manufacturer's specifications?
	☐
	☐
	☐
	____________________

	Has the lifting equipment been load-tested within the past year, and is documentation available?
	☐
	☐
	☐
	____________________

	Are emergency stop buttons for the hoisting system readily accessible and functioning correctly?
	☐
	☐
	☐
	____________________

	Are tag lines used to control the load during lifting operations, preventing uncontrolled swinging?
	☐
	☐
	☐
	____________________


Underground Utilities & Excavation Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Has a comprehensive utility locate request been submitted and reviewed prior to any excavation or drilling?
	☐
	☐
	☐
	____________________

	Are all identified underground utilities clearly marked with paint, flags, or other visible means?
	☐
	☐
	☐
	____________________

	Are safe digging practices (e.g., hand digging, vacuum excavation) employed when working near marked utilities?
	☐
	☐
	☐
	____________________

	Is there a sufficient clearance distance maintained between the drilling operation and any identified underground utilities?
	☐
	☐
	☐
	____________________

	Is emergency contact information for utility companies readily available on site?
	☐
	☐
	☐
	____________________

	Is a dedicated spotter present during drilling operations near underground utilities to monitor for potential hazards?
	☐
	☐
	☐
	____________________

	Are excavations properly shored or sloped to prevent collapse, especially in unstable soil conditions?
	☐
	☐
	☐
	____________________

	Are confined space entry procedures followed if personnel are required to enter excavations?
	☐
	☐
	☐
	____________________

	Is atmospheric monitoring conducted in excavations to check for hazardous gases or oxygen deficiency?
	☐
	☐
	☐
	____________________

	Are trench boxes or shoring systems inspected daily for damage or defects?
	☐
	☐
	☐
	____________________

	Is a competent person (as defined by OSHA) on site to inspect excavations and shoring systems?
	☐
	☐
	☐
	____________________


Rig Operation & Maintenance
	Item
	Pass
	Fail
	N/A
	Notes

	Is a daily pre-start inspection of the rotary piling rig performed, including checks of fluid levels, hoses, and structural components?
	☐
	☐
	☐
	____________________

	Are maintenance records up-to-date and readily available for review?
	☐
	☐
	☐
	____________________

	Is the Kelly bar inspected for wear, cracks, and proper alignment before each shift?
	☐
	☐
	☐
	____________________

	Is the auger inspected for damaged or missing teeth, and is it appropriate for the soil conditions?
	☐
	☐
	☐
	____________________

	Are hydraulic hoses and fittings inspected for leaks and damage?
	☐
	☐
	☐
	____________________

	Are emergency shutdown procedures clearly posted and understood by all operators?
	☐
	☐
	☐
	____________________

	Are all rig operators properly trained and certified to operate the specific type of rotary piling rig being used?
	☐
	☐
	☐
	____________________

	Are load charts readily available and understood by the operator?
	☐
	☐
	☐
	____________________

	Is the rig equipped with a functioning level indicator to ensure it is operating within safe limits?
	☐
	☐
	☐
	____________________

	Are noise levels monitored, and are hearing protection measures in place if noise levels exceed permissible limits?
	☐
	☐
	☐
	____________________

	Are exhaust emissions properly controlled to prevent exposure to hazardous fumes?
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Are hard hats worn by all personnel within the work zone?
	☐
	☐
	☐
	____________________

	Are safety glasses or face shields worn to protect against flying debris?
	☐
	☐
	☐
	____________________

	Are all personnel wearing high-visibility clothing (e.g., vests, jackets)?
	☐
	☐
	☐
	____________________

	Are steel-toe boots worn to protect against foot injuries?
	☐
	☐
	☐
	____________________

	Is hearing protection available and used in areas with high noise levels?
	☐
	☐
	☐
	____________________

	Are appropriate gloves worn to protect against hand injuries?
	☐
	☐
	☐
	____________________

	Is respiratory protection required and used if there is a risk of exposure to dust or fumes?
	☐
	☐
	☐
	____________________

	Is PPE inspected regularly for damage or defects?
	☐
	☐
	☐
	____________________

	Have all personnel been trained on the proper use and maintenance of PPE?
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
