InspectionReport
PPE Inspection and Compliance Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
Jurisdiction: Adaptable. Covers OSHA 29 CFR 1910.132 (US) and UK PPER 1992. Adaptable to other jurisdictions with PPE regulations. Apply only the section and thresholds for the governing jurisdiction; do not combine US and UK requirements as if they were one code.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Hazard assessment documentation
	Item
	Pass
	Fail
	N/A
	Notes

	Written hazard assessment completed: Yes / No
	☐
	☐
	☐
	____________________

	Workplace evaluated and identified
	☐
	☐
	☐
	____________________

	Person certifying the evaluation
	☐
	☐
	☐
	____________________

	Date of hazard assessment
	☐
	☐
	☐
	____________________

	PPE matched to specific identified hazards
	☐
	☐
	☐
	____________________


Head protection (hard hats)
	Item
	Pass
	Fail
	N/A
	Notes

	Manufacturing date on shell: within 5-year lifespan
	☐
	☐
	☐
	____________________

	Inner suspension: within 1-year lifespan from first use
	☐
	☐
	☐
	____________________

	Shell condition: no crazing (UV cracks), deep gouges, or chalking
	☐
	☐
	☐
	____________________

	Suspension: no cuts, fraying, or stretched straps
	☐
	☐
	☐
	____________________


Respiratory protection
	Item
	Pass
	Fail
	N/A
	Notes

	Facepiece: no cracks, tears, distortion
	☐
	☐
	☐
	____________________

	Exhalation valves: seated correctly and clean
	☐
	☐
	☐
	____________________

	Operator clean-shaven (for tight-fitting respirators)
	☐
	☐
	☐
	____________________

	Filter / cartridge: within service life, replaced per schedule
	☐
	☐
	☐
	____________________


Hand protection
	Item
	Pass
	Fail
	N/A
	Notes

	Chemical-resistant gloves: air-inflation test for pinholes before each use
	☐
	☐
	☐
	____________________

	Leather rigging gloves: no torn stitching
	☐
	☐
	☐
	____________________

	Glove type matched to specific chemical hazard
	☐
	☐
	☐
	____________________


Eye and face protection
	Item
	Pass
	Fail
	N/A
	Notes

	Safety glasses: lenses from heavy scratches (per ANSI Z87.1)
	☐
	☐
	☐
	____________________

	Goggles: seal intact, no cracks
	☐
	☐
	☐
	____________________

	Face shields: no cracks or damage
	☐
	☐
	☐
	____________________


Component compatibility (UK PPER)
	Item
	Pass
	Fail
	N/A
	Notes

	Multiple PPE items worn simultaneously: compatible (e.g., ear defenders do not break goggles seal)
	☐
	☐
	☐
	____________________


Defect resolution
	Item
	Pass
	Fail
	N/A
	Notes

	Defective PPE removed from service: Yes / No
	☐
	☐
	☐
	____________________

	Replacement PPE issued
	☐
	☐
	☐
	____________________

	Inspector initials and date
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
References consulted
OSHA 29 CFR 1910.132 – General requirements for PPE
UK HSE – Personal Protective Equipment at Work Regulations 1992
ANSI Z87.1 – Occupational and Educational Personal Eye and Face Protection Devices
UK HSE – PPE at work (L22)
Verify the current edition and local adoption before use.
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
