InspectionReport
Rig Floor Safety Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Housekeeping & Floor Conditions
	Item
	Pass
	Fail
	N/A
	Notes

	Is the drill floor free of oil, grease, and drilling mud? (Immediate cleaning required)
	☐
	☐
	☐
	____________________

	Are spill containment measures (e.g., drip pans, absorbent materials) in place and properly used around hydraulic equipment and connections?
	☐
	☐
	☐
	____________________

	Are all hoses, cables, and lines properly routed and secured to prevent trip hazards? Are cable protectors in use where necessary?
	☐
	☐
	☐
	____________________

	Is the floor drainage system clear and functioning properly to prevent fluid accumulation?
	☐
	☐
	☐
	____________________

	Are anti-slip surfaces (e.g., mats, coatings) in good condition and properly maintained in high-traffic areas and around the rotary table?
	☐
	☐
	☐
	____________________

	Is lighting adequate (minimum 50 foot-candles) across the entire drill floor, including the red zone and around the rotary table, to ensure clear visibility?
	☐
	☐
	☐
	____________________

	Are all walking/working surfaces free from damage (e.g., holes, loose grating) that could cause slips, trips, or falls?
	☐
	☐
	☐
	____________________

	Are emergency exits clearly marked, unobstructed, and easily accessible from all areas of the drill floor?
	☐
	☐
	☐
	____________________

	Are sufficient waste receptacles available and properly used for disposal of trash, rags, and other waste materials?
	☐
	☐
	☐
	____________________

	Is the floor load rating clearly posted and adhered to? Are heavy items stored in designated areas to prevent overloading?
	☐
	☐
	☐
	____________________


Rotating Equipment & Red Zone Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Are all moving parts of the rotary table properly guarded to prevent contact? (Guards must be securely in place)
	☐
	☐
	☐
	____________________

	Is the Iron Roughneck operating smoothly and within its specified parameters? Are all safety interlocks functioning correctly?
	☐
	☐
	☐
	____________________

	Are tongs in good working condition, with properly maintained dies and secure latching mechanisms?
	☐
	☐
	☐
	____________________

	Is the 'Red Zone' around the rotary table clearly marked with highly visible paint or tape? Is access restricted to authorized personnel only?
	☐
	☐
	☐
	____________________

	Are emergency stop buttons for all rotating equipment readily accessible and functioning correctly? (Test each button)
	☐
	☐
	☐
	____________________

	Is a proper Lockout/Tagout (LOTO) procedure in place and followed for all maintenance and repair work on rotating equipment?
	☐
	☐
	☐
	____________________

	Is a clear and reliable communication system (e.g., hand signals, radio) in place between the driller and all personnel working in the red zone?
	☐
	☐
	☐
	____________________

	Have all personnel received training on pinch point hazards associated with rotating equipment and pipe handling operations?
	☐
	☐
	☐
	____________________

	Are documented inspections of all rotating equipment (rotary table, Iron Roughneck, tongs) conducted regularly and records maintained?
	☐
	☐
	☐
	____________________

	Are all hydraulic hoses and fittings on rotating equipment inspected for leaks, wear, and damage? Are they rated for the operating pressure?
	☐
	☐
	☐
	____________________


Drill Pipe Handling & Tubular Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Is the pipe racking system in good condition, with secure supports and properly functioning elevators?
	☐
	☐
	☐
	____________________

	Are all pipe handling tools (e.g., slips, elevators, spiders) inspected for wear, damage, and proper function before each use?
	☐
	☐
	☐
	____________________

	Are stabbers positioned safely and using appropriate fall protection when working at height during pipe connections?
	☐
	☐
	☐
	____________________

	Are measures in place to prevent dropped objects (e.g., tool tethers, netting, barricades) during pipe handling operations?
	☐
	☐
	☐
	____________________

	Are drill pipes and tubulars inspected for defects (e.g., cracks, corrosion) before being used in the wellbore?
	☐
	☐
	☐
	____________________

	Are pipe threads properly cleaned and lubricated before each connection to ensure proper sealing and prevent galling?
	☐
	☐
	☐
	____________________

	Is torque accurately monitored during pipe connections to prevent over- or under-tightening?
	☐
	☐
	☐
	____________________

	Are tag lines used to control the movement of drill pipe during lifting and lowering operations?
	☐
	☐
	☐
	____________________

	Are load charts for pipe handling equipment readily available and understood by all personnel involved in lifting operations?
	☐
	☐
	☐
	____________________

	Is clear communication maintained between the driller, derrickhand, and floorhands during all pipe handling operations?
	☐
	☐
	☐
	____________________

	Is drill pipe stored properly to prevent damage and ensure stability?
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Are all personnel on the drill floor wearing properly fitted and approved hard hats (ANSI Z89.1)?
	☐
	☐
	☐
	____________________

	Are all personnel wearing appropriate safety glasses or goggles (ANSI Z87.1) with side shields to protect against eye hazards?
	☐
	☐
	☐
	____________________

	Are all personnel wearing steel-toe boots (ASTM F2413) to protect against foot injuries?
	☐
	☐
	☐
	____________________

	Are appropriate gloves (e.g., leather, nitrile) worn to protect hands from cuts, abrasions, and chemical exposure?
	☐
	☐
	☐
	____________________

	Is hearing protection (e.g., earplugs, earmuffs) readily available and used in areas with high noise levels (above 85 dBA)?
	☐
	☐
	☐
	____________________

	Are all personnel wearing flame-resistant clothing (FRC) that meets NFPA 2112 standards?
	☐
	☐
	☐
	____________________

	Is respiratory protection (e.g., dust masks, respirators) required and used when exposed to airborne contaminants (e.g., dust, fumes)?
	☐
	☐
	☐
	____________________

	Is all PPE inspected regularly for damage, wear, and proper fit? Is damaged PPE replaced immediately?
	☐
	☐
	☐
	____________________

	Have all personnel received training on the proper use, care, and maintenance of required PPE?
	☐
	☐
	☐
	____________________

	Are personnel wearing high-visibility clothing (ANSI 107) when working in areas with mobile equipment or limited visibility?
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
