InspectionReport
Roof Safety and Edge Protection Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
Jurisdiction: Adaptable. Covers OSHA 29 CFR 1926.501 (US) and UK Work at Height Regulations 2005 (WAHR). Adaptable to other jurisdictions. Apply only the section and thresholds for the governing jurisdiction; do not combine US and UK requirements as if they were one code.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Inspection header
	Field
	Entry

	Site name and location
	________________________________________________

	Inspector name and date
	________________________________________________

	Roof area / zone inspected
	________________________________________________

	Weather conditions
	________________________________________________


Edge protection systems
	Item
	Pass
	Fail
	N/A
	Notes

	Guardrail top rail height: OSHA 42 inches (±3) / UK WAHR minimum 950mm
	☐
	☐
	☐
	____________________

	Intermediate (mid) rail: installed midway between top rail and walking level
	☐
	☐
	☐
	____________________

	Toe boards: minimum 3.5 inches (89mm) high (OSHA) / 150mm (UK)
	☐
	☐
	☐
	____________________

	Load resistance: withstands 200-lb downward and outward force (OSHA)
	☐
	☐
	☐
	____________________

	Gap between top rail and intermediate rail / toe board: ≤ 470mm (UK)
	☐
	☐
	☐
	____________________


Fall arrest systems
	Item
	Pass
	Fail
	N/A
	Notes

	Anchorage points: structurally sound, capable of 5,000 lbs per employee (OSHA)
	☐
	☐
	☐
	____________________

	Anchor positioning: directly above work area (minimize swing fall)
	☐
	☐
	☐
	____________________

	Connectors: self-closing and self-locking carabiners / snap hooks
	☐
	☐
	☐
	____________________


Roof hazards
	Item
	Pass
	Fail
	N/A
	Notes

	Skylights: covered, secured, marked with 'HOLE' or 'COVER'
	☐
	☐
	☐
	____________________

	Holes >6 feet above lower level: protected
	☐
	☐
	☐
	____________________

	Leading edges: fall protection plan documented if guardrails impossible
	☐
	☐
	☐
	____________________

	Roof surface condition: slippery, wet, damaged areas identified
	☐
	☐
	☐
	____________________


Access and egress
	Item
	Pass
	Fail
	N/A
	Notes

	Ladders / stairs: secure, properly angled, extending above landing
	☐
	☐
	☐
	____________________

	Roof hatches: self-closing, guarded when open
	☐
	☐
	☐
	____________________


Inspection frequency and follow-up
	Item
	Pass
	Fail
	N/A
	Notes

	Daily inspection: Yes / No
	☐
	☐
	☐
	____________________

	Inspection after high winds / heavy rain: Yes / No
	☐
	☐
	☐
	____________________

	Defects noted with location and description
	☐
	☐
	☐
	____________________

	Corrective action assigned
	☐
	☐
	☐
	____________________

	Inspector signature
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
References consulted
OSHA 29 CFR 1926.501 – Duty to have fall protection
UK HSE – Work at Height Regulations 2005
OSHA 29 CFR 1926.502 – System planning and criteria
UK HSE – Work at height: the law (INDG401)
Verify the current edition and local adoption before use.
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
