InspectionReport
Telecom Aerial Lift / Bucket Truck Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Mobile Equipment (Bucket Truck) Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Check tire pressure against manufacturer's specifications. All tires must be evenly inflated. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Inspect engine oil, coolant, hydraulic fluid, and brake fluid levels. Refill as needed. (Manufacturer's Specs)
	☐
	☐
	☐
	____________________

	Verify all lights (headlights, taillights, brake lights, turn signals, hazard lights) and audible signals (horn, backup alarm) are functioning correctly. (OSHA 1910.67)
	☐
	☐
	☐
	____________________

	Inspect steering mechanism for excessive play or binding. Ensure smooth and responsive steering. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Test service brakes and parking brake functionality. Service brakes must provide smooth, even stopping power. Parking brake must hold the truck on an incline. (OSHA 1910.67)
	☐
	☐
	☐
	____________________

	Ensure windshield wipers and washers are operational and provide clear visibility. (Local DOT Regulations)
	☐
	☐
	☐
	____________________

	Inspect mirrors for damage and ensure they are properly adjusted for clear visibility. (OSHA 1910.67)
	☐
	☐
	☐
	____________________

	Verify the backup alarm is functioning and audible. (OSHA 1926.602(a)(9)(ii))
	☐
	☐
	☐
	____________________

	Test the horn to ensure it is functioning properly. (OSHA 1926.602(a)(9)(i))
	☐
	☐
	☐
	____________________

	Confirm a fully charged and inspected fire extinguisher is present and readily accessible. (OSHA 1910.157)
	☐
	☐
	☐
	____________________


Outrigger and Stability System Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Inspect outrigger pads for damage or deterioration. Ensure they are of adequate size and load rating for the ground conditions. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Verify smooth and complete extension and retraction of all outriggers. Check for leaks or binding. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Ensure outrigger locking mechanisms are functioning correctly and securely lock the outriggers in the extended position. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Verify the accuracy of the level indicators (bubble level or electronic). Truck must be level before boom operation. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Assess ground conditions for stability. Avoid soft soil, slopes exceeding manufacturer's limits, and uneven surfaces. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Confirm the slope is within the manufacturer's specified limits for safe operation. Use a clinometer if necessary. (Manufacturer's Specs)
	☐
	☐
	☐
	____________________

	Test outrigger interlocks to ensure boom operation is prevented unless outriggers are properly deployed. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Inspect hydraulic lines and cylinders for leaks around the outriggers. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Identify and mitigate any proximity hazards (e.g., underground utilities, overhead obstructions) before deploying outriggers. (OSHA 1926 Subpart V)
	☐
	☐
	☐
	____________________


Insulated Boom and Upper Controls Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Visually inspect the insulated boom sections for cracks, damage, or contamination. Report any defects immediately. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Inspect boom for any signs of bending, buckling, or weld cracks. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Inspect hydraulic hoses and fittings for leaks along the entire boom length. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Verify smooth and responsive operation of all boom controls (elevation, rotation, extension). (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Test the emergency stop button at both the upper and lower controls. Ensure it immediately stops all boom movement. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Confirm that the lower controls can override the upper controls in an emergency. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Inspect the bucket for cracks, damage, or debris. Ensure the bucket floor is clean and slip-resistant. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Inspect the bucket liner (if equipped) for damage or contamination. Ensure it is properly installed and provides adequate insulation. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Verify minimum approach distances (MAD) from energized power lines are maintained. Use a spotter if necessary. (OSHA 1926.950)
	☐
	☐
	☐
	____________________

	Test boom interlocks to prevent operation outside of safe operating parameters (e.g., exceeding reach limits). (ANSI A92.2)
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE) and Fall Protection
	Item
	Pass
	Fail
	N/A
	Notes

	Inspect full-body harness for rips, tears, fraying, or damage. Ensure it fits properly. (OSHA 1926.502(d))
	☐
	☐
	☐
	____________________

	Inspect lanyard for cuts, abrasions, or damage to the snap hooks. Use a lanyard of appropriate length. (OSHA 1926.502(d))
	☐
	☐
	☐
	____________________

	Inspect dielectric gloves for holes, tears, or contamination. Test gloves per manufacturer's instructions. (OSHA 1910.137)
	☐
	☐
	☐
	____________________

	Ensure appropriate eye protection (safety glasses or face shield) is worn. (OSHA 1926.102)
	☐
	☐
	☐
	____________________

	Verify hard hat is in good condition and properly fitted. (OSHA 1926.100)
	☐
	☐
	☐
	____________________

	Ensure appropriate footwear (steel-toed boots) is worn. (OSHA 1926.96)
	☐
	☐
	☐
	____________________

	Verify that the fall arrest system (harness and lanyard) is properly connected to the designated anchor point in the bucket. (OSHA 1926.502)
	☐
	☐
	☐
	____________________

	Ensure all tools used in the bucket are secured with tool lanyards to prevent dropped objects. (Company Policy)
	☐
	☐
	☐
	____________________

	Confirm clothing is appropriate for the weather conditions and does not pose a snag hazard. (Company Policy)
	☐
	☐
	☐
	____________________


Documentation and Training
	Item
	Pass
	Fail
	N/A
	Notes

	Verify the operator is certified and trained to operate the specific type of bucket truck. (OSHA 1910.67)
	☐
	☐
	☐
	____________________

	Review previous inspection records to identify any recurring issues. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Review maintenance records to ensure the bucket truck has been properly maintained according to the manufacturer's recommendations. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Ensure the load chart is present and legible in the bucket truck. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Confirm the operator's manual is available in the bucket truck. (ANSI A92.2)
	☐
	☐
	☐
	____________________

	Ensure a daily inspection log is being maintained and completed before each shift. (Company Policy)
	☐
	☐
	☐
	____________________

	Verify a rescue plan is in place in case of an emergency or fall from the bucket. (Company Policy)
	☐
	☐
	☐
	____________________

	Confirm a reliable method of communication (e.g., radio, cell phone) is available for emergencies. (Company Policy)
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
