InspectionReport
Warehouse Racking Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
Jurisdiction: UK. Based on UK PUWER 1998 and SEMA traffic light risk system. Adaptable to other jurisdictions with work equipment regulations.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Inspection header
	Field
	Entry

	Warehouse / facility name
	________________________________________________

	Inspector name and designation (PRRS / SARI)
	________________________________________________

	Inspection date
	________________________________________________

	Inspection type (daily visual / weekly monthly internal / annual expert)
	________________________________________________


Uprights and columns
	Item
	Pass
	Fail
	N/A
	Notes

	Base of uprights (first meter): dents, bends, twisting, rust
	☐
	☐
	☐
	____________________

	Upright frame integrity: no structural deformation
	☐
	☐
	☐
	____________________

	Floor fixings and anchors: securely anchored, bolts undamaged
	☐
	☐
	☐
	____________________


Beams and connectors
	Item
	Pass
	Fail
	N/A
	Notes

	Beam deflection: visually straight when empty, no excessive bowing
	☐
	☐
	☐
	____________________

	Beam-to-upright connectors: locking safety pins in place
	☐
	☐
	☐
	____________________

	Beam engagement: fully seated in upright slots
	☐
	☐
	☐
	____________________


Load notices and configuration
	Field
	Entry

	Safe Working Load (SWL) notices: present, legible, accurate for current configuration
	________________________________________________

	Beam levels match SWL notice ratings
	________________________________________________


SEMA traffic light damage classification
	Item
	Pass
	Fail
	N/A
	Notes

	Red risk: severe buckling, torn metal, sheared connectors → immediate offload and tape off
	☐
	☐
	☐
	____________________

	Amber risk: dents/bends exceeding SEMA tolerances → do not reload after current dispatch
	☐
	☐
	☐
	____________________

	Green risk: superficial scrapes within safe margins → observe and monitor
	☐
	☐
	☐
	____________________


Aisle and operational checks
	Item
	Pass
	Fail
	N/A
	Notes

	Aisle clearances: unobstructed for forklift operation
	☐
	☐
	☐
	____________________

	End-of-aisle protection: guard posts / impact protection present
	☐
	☐
	☐
	____________________

	Pallet placement: no overhang beyond beam edge
	☐
	☐
	☐
	____________________


Corrective action
	Item
	Pass
	Fail
	N/A
	Notes

	Damage description and location (bay, level, upright number)
	☐
	☐
	☐
	____________________

	Risk classification (Red / Amber / Green)
	☐
	☐
	☐
	____________________

	Immediate action taken
	☐
	☐
	☐
	____________________

	Follow-up action required
	☐
	☐
	☐
	____________________

	Inspector signature
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
References consulted
UK HSE – PUWER 1998 (Provision and Use of Work Equipment Regulations)
SEMA – Storage Equipment Manufacturers' Association
UK HSE – Inspection of warehouse racking (HSG76)
SEMA – Rack inspection guidelines
Verify the current edition and local adoption before use.
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
