InspectionReport
Aviation Maintenance Hangar FOD Walk Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Tool Control & Accountability
	Item
	Pass
	Fail
	N/A
	Notes

	Does the tool inventory match the shadow board or tool box manifest at the start of the shift? (SAE AS9100)
	☐
	☐
	☐
	____________________

	Are all tools permanently etched or marked with a unique identification number? (14 CFR Part 145)
	☐
	☐
	☐
	____________________

	Are tools used at height properly tethered to prevent drops? (ANSI/ISEA 121-2018)
	☐
	☐
	☐
	____________________

	Is there a documented procedure for handling broken or missing tools? (Company Policy)
	☐
	☐
	☐
	____________________

	Are toolboxes and storage areas clean, organized, and free of FOD? (Best Practice)
	☐
	☐
	☐
	____________________

	Are calibrated tools (e.g., torque wrenches) within their calibration period? (ISO 17025)
	☐
	☐
	☐
	____________________

	Are tools inspected for damage (e.g., cracks, worn edges) before each use? (Best Practice)
	☐
	☐
	☐
	____________________

	Are foam inserts used in toolboxes to quickly identify missing tools? (Best Practice)
	☐
	☐
	☐
	____________________

	Is the tool shadow board in good condition, with all tools clearly visible and accounted for? (Best Practice)
	☐
	☐
	☐
	____________________

	Have all AMTs received documented training on tool control procedures? (Company Policy)
	☐
	☐
	☐
	____________________


Ground Service Equipment (GSE) & Mobile Equipment
	Item
	Pass
	Fail
	N/A
	Notes

	Is the tow bar free from cracks, bends, and corrosion? (SAE ARP4276)
	☐
	☐
	☐
	____________________

	Do all GSE vehicles have functional parking brakes? (OSHA 1910.178(m)(7))
	☐
	☐
	☐
	____________________

	Are GSE tires properly inflated and free from excessive wear or damage? (Manufacturer's Specifications)
	☐
	☐
	☐
	____________________

	Are there any visible fluid leaks (oil, hydraulic fluid) from GSE vehicles? (EPA Regulations)
	☐
	☐
	☐
	____________________

	Is the horn on all GSE vehicles functional? (OSHA 1910.178(p)(1))
	☐
	☐
	☐
	____________________

	Are headlights, taillights, and brake lights on all GSE vehicles working properly? (OSHA 1910.178(h)(3))
	☐
	☐
	☐
	____________________

	Is the grounding cable on fuel trucks in good condition and properly connected during refueling operations? (NFPA 407)
	☐
	☐
	☐
	____________________

	Are speed limits clearly posted and enforced for GSE vehicles within the hangar? (Company Policy)
	☐
	☐
	☐
	____________________

	Are all GSE operators properly trained and certified to operate the equipment? (OSHA 1910.178(l))
	☐
	☐
	☐
	____________________

	Are maintenance records for GSE vehicles up-to-date and readily available? (Company Policy)
	☐
	☐
	☐
	____________________


Hangar Floor & Site Conditions
	Item
	Pass
	Fail
	N/A
	Notes

	Is the hangar floor clean and free from debris, tools, hardware, and other potential FOD? (Best Practice)
	☐
	☐
	☐
	____________________

	Are spill control materials (e.g., absorbent pads, booms) readily available and properly stocked? (EPA Regulations)
	☐
	☐
	☐
	____________________

	Are there any Skydrol spills present on the hangar floor? (Immediately clean and report any spills) (Company Policy)
	☐
	☐
	☐
	____________________

	Is lighting adequate throughout the hangar to ensure good visibility? (OSHA 1910.22(a)(1))
	☐
	☐
	☐
	____________________

	Are any tripping hazards (e.g., cables, hoses) properly marked and secured? (OSHA 1910.22(a)(2))
	☐
	☐
	☐
	____________________

	Are floor drains clear and free from obstructions? (Best Practice)
	☐
	☐
	☐
	____________________

	Are sufficient waste receptacles available and properly labeled for different types of waste? (EPA Regulations)
	☐
	☐
	☐
	____________________

	Are good housekeeping practices being followed throughout the hangar? (OSHA 1910.22)
	☐
	☐
	☐
	____________________

	Are fire extinguishers readily accessible and properly charged? (NFPA 10)
	☐
	☐
	☐
	____________________

	Are emergency exits clear and unobstructed? (OSHA 1910.36)
	☐
	☐
	☐
	____________________

	Are first-aid supplies readily available and adequately stocked? (ANSI Z308.1)
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Are safety glasses worn at all times in designated areas? (OSHA 1910.133)
	☐
	☐
	☐
	____________________

	Is hearing protection available and used in areas with high noise levels? (OSHA 1910.95)
	☐
	☐
	☐
	____________________

	Are steel-toe boots worn to protect against foot injuries? (ANSI Z41)
	☐
	☐
	☐
	____________________

	Are appropriate gloves worn when handling chemicals or sharp objects? (OSHA 1910.138)
	☐
	☐
	☐
	____________________

	Are respirators used when required, and are they properly fit-tested? (OSHA 1910.134)
	☐
	☐
	☐
	____________________

	Is high-visibility clothing worn when working near moving equipment? (ANSI/ISEA 107)
	☐
	☐
	☐
	____________________

	Is all PPE in good condition and properly maintained? (OSHA 1910.132)
	☐
	☐
	☐
	____________________

	Have all employees received training on the proper use and care of PPE? (OSHA 1910.132(f))
	☐
	☐
	☐
	____________________

	Is an eyewash station readily accessible in areas where chemicals are used? (ANSI Z358.1)
	☐
	☐
	☐
	____________________

	Is there a designated area for storing PPE when not in use? (Best Practice)
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
