InspectionReport
Commercial Kitchen Grease Trap Service Safety Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Mobile Equipment & Vehicle Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Is a current vehicle inspection report available and up-to-date, including brakes, lights, and tires?
	☐
	☐
	☐
	____________________

	Does the vehicle's parking brake effectively hold the vehicle on an incline?
	☐
	☐
	☐
	____________________

	Are wheel chocks available and used when parking on sloped surfaces during pumping operations?
	☐
	☐
	☐
	____________________

	Inspect suction hose for cuts, abrasions, or kinks before each use. Replace if damaged.
	☐
	☐
	☐
	____________________

	Are hose restraints (e.g., straps, chains) used to prevent uncontrolled hose movement if a coupling fails?
	☐
	☐
	☐
	____________________

	Is the vacuum pump equipped with a functioning emergency shut-off switch, easily accessible to the operator?
	☐
	☐
	☐
	____________________

	Is adequate lighting (minimum 5 foot-candles) provided around the work area and vehicle, especially during night operations? (Use portable lighting if needed)
	☐
	☐
	☐
	____________________

	Is a spill kit readily available on the vehicle, containing absorbent materials, PPE, and disposal bags?
	☐
	☐
	☐
	____________________

	Is a fully charged and inspected fire extinguisher (minimum 20-ABC rating) present on the vehicle?
	☐
	☐
	☐
	____________________

	Is the vehicle horn operational?
	☐
	☐
	☐
	____________________


Site Conditions & Hazard Control
	Item
	Pass
	Fail
	N/A
	Notes

	Are walkways and work areas free of slip, trip, and fall hazards (e.g., grease spills, water, debris)?
	☐
	☐
	☐
	____________________

	Are 'Wet Floor' signs prominently displayed in areas where cleaning or pumping operations create a slip hazard?
	☐
	☐
	☐
	____________________

	Is there adequate ventilation in the area around the grease interceptor to prevent the buildup of toxic fumes (H2S, methane)?
	☐
	☐
	☐
	____________________

	If entry into the grease interceptor is required, is a confined space entry permit in place, including atmospheric testing, ventilation, and rescue plan?
	☐
	☐
	☐
	____________________

	Is adequate traffic control in place to protect workers from vehicle traffic (e.g., cones, barriers, flaggers)?
	☐
	☐
	☐
	____________________

	Is the suction hose routed safely to avoid creating trip hazards or obstructing walkways?
	☐
	☐
	☐
	____________________

	Is there a plan and equipment in place to contain any effluent spills during pumping operations?
	☐
	☐
	☐
	____________________

	Are all electrical cords and equipment properly grounded and free from damage?
	☐
	☐
	☐
	____________________

	Is there adequate overhead clearance for the vacuum truck and hose boom?
	☐
	☐
	☐
	____________________

	Has the restaurant manager been notified of the service and any potential disruptions?
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Are safety glasses or goggles worn to protect against splashes and debris?
	☐
	☐
	☐
	____________________

	Are chemical-resistant gloves worn to protect against contact with grease and effluent?
	☐
	☐
	☐
	____________________

	Is respiratory protection (e.g., half-face respirator with appropriate cartridges) worn if there is a risk of exposure to toxic fumes (H2S, methane)?
	☐
	☐
	☐
	____________________

	Are slip-resistant and chemical-resistant safety boots worn?
	☐
	☐
	☐
	____________________

	Is high-visibility clothing (e.g., safety vest) worn to increase visibility to vehicle traffic?
	☐
	☐
	☐
	____________________

	Is hearing protection (e.g., earplugs or earmuffs) worn if noise levels exceed 85 dBA?
	☐
	☐
	☐
	____________________

	Inspect all PPE for damage (tears, cracks, etc.) before each use. Replace damaged PPE immediately.
	☐
	☐
	☐
	____________________

	Ensure all PPE fits properly and is worn correctly.
	☐
	☐
	☐
	____________________

	Is a hard hat worn if there is a risk of head injury from falling objects?
	☐
	☐
	☐
	____________________


Pumping Operations
	Item
	Pass
	Fail
	N/A
	Notes

	Are all hose connections properly tightened and secured to prevent leaks or accidental disconnections?
	☐
	☐
	☐
	____________________

	Monitor the vacuum gauge during pumping to prevent over-pressurization or damage to the system.
	☐
	☐
	☐
	____________________

	Avoid kinking or sharp bends in the suction hose, which can restrict flow and damage the hose.
	☐
	☐
	☐
	____________________

	Implement spill prevention measures during hose connections and disconnections (e.g., drip pans, absorbent pads).
	☐
	☐
	☐
	____________________

	Monitor the tank level on the vacuum truck to prevent overfilling.
	☐
	☐
	☐
	____________________

	Use hose supports or stands to prevent the hose from dragging on the ground and becoming damaged.
	☐
	☐
	☐
	____________________

	Establish clear communication protocols between the technician operating the vacuum truck and the technician handling the hose at the interceptor.
	☐
	☐
	☐
	____________________

	Verify the vacuum truck's pressure relief valve is functioning correctly.
	☐
	☐
	☐
	____________________

	Visually inspect the hose during pumping operations for any signs of leaks or damage.
	☐
	☐
	☐
	____________________


Documentation & Training
	Item
	Pass
	Fail
	N/A
	Notes

	Are Material Safety Data Sheets (MSDS) or Safety Data Sheets (SDS) readily available for all chemicals used during the service?
	☐
	☐
	☐
	____________________

	Are training records available to verify that all technicians are trained in safe grease trap service procedures, confined space entry (if applicable), and hazard communication?
	☐
	☐
	☐
	____________________

	Is an emergency contact list readily available, including phone numbers for emergency services, the restaurant manager, and the company's safety officer?
	☐
	☐
	☐
	____________________

	Has a site-specific risk assessment been conducted before starting the service, identifying potential hazards and control measures?
	☐
	☐
	☐
	____________________

	If the grease interceptor is classified as a permit-required confined space, is a valid entry permit completed and posted?
	☐
	☐
	☐
	____________________

	Are equipment maintenance logs maintained for the vacuum truck and pumping equipment?
	☐
	☐
	☐
	____________________

	Is there a documented incident reporting procedure in place?
	☐
	☐
	☐
	____________________

	Obtain customer sign-off on the service report, acknowledging completion of the work and any observed issues.
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
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	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
