InspectionReport
Industrial Laundry & Dry Cleaning Safety Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Steam System Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Are all steam valve seals inspected monthly for leaks using a calibrated ultrasonic leak detector? (Record dB levels)
	☐
	☐
	☐
	____________________

	Are steam traps tested quarterly for proper functionality (e.g., temperature differential, visual inspection of condensate discharge)?
	☐
	☐
	☐
	____________________

	Is insulation intact on all steam pipes and equipment to prevent contact burns? (Surface temperature < 140°F)
	☐
	☐
	☐
	____________________

	Are pressure relief valves (PRVs) on steam boilers and pressure vessels inspected annually and tested every 3 years? (Documented inspection)
	☐
	☐
	☐
	____________________

	Is the condensate return system free from leaks and blockages, ensuring efficient steam system operation?
	☐
	☐
	☐
	____________________

	Is boiler water treatment program in place and followed to prevent scale buildup and corrosion? (Review chemical analysis reports)
	☐
	☐
	☐
	____________________

	Are steam hoses inspected before each use for damage (cracks, bulges, abrasions) and properly rated for steam pressure and temperature?
	☐
	☐
	☐
	____________________

	Are emergency shutdown valves for the steam system clearly marked and easily accessible?
	☐
	☐
	☐
	____________________

	Have all employees working with or near steam systems received documented training on safe operating procedures and emergency response?
	☐
	☐
	☐
	____________________

	Are all steam pipes and equipment properly grounded to prevent static electricity buildup?
	☐
	☐
	☐
	____________________


Dry Cleaning (PERC) Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Is PERC vapor concentration monitored regularly (at least weekly) in the breathing zone using a calibrated monitoring device? (Results < 25 ppm TWA)
	☐
	☐
	☐
	____________________

	Is the dry cleaning machine fully enclosed and properly ventilated to prevent PERC vapor leaks?
	☐
	☐
	☐
	____________________

	Are PERC machines inspected daily for leaks (seals, hoses, connections) using a halogen leak detector?
	☐
	☐
	☐
	____________________

	Is a spill containment system (e.g., berms, absorbent materials) in place to prevent PERC spills from reaching drains or the environment?
	☐
	☐
	☐
	____________________

	Is PERC waste (sludge, filters) properly stored, labeled, and disposed of according to hazardous waste regulations?
	☐
	☐
	☐
	____________________

	Are employees provided with and using appropriate PPE (gloves, respirators, eye protection) when handling PERC?
	☐
	☐
	☐
	____________________

	Have all employees working with PERC received documented training on its hazards, safe handling procedures, and emergency response?
	☐
	☐
	☐
	____________________

	Is a fire suppression system (e.g., CO2, FM-200) in place to protect the dry cleaning area in case of a fire?
	☐
	☐
	☐
	____________________

	Is the dry cleaning machine maintained per manufacturer's recommendations, including regular filter changes and solvent recovery system checks?
	☐
	☐
	☐
	____________________

	Is an emergency eyewash station readily accessible near the PERC handling area?
	☐
	☐
	☐
	____________________


Laundry Operations & Ergonomics
	Item
	Pass
	Fail
	N/A
	Notes

	Are laundry carts equipped with brakes and are they used on inclines to prevent runaway carts?
	☐
	☐
	☐
	____________________

	Are laundry carts loaded within their rated weight capacity to prevent tipping and ergonomic strain? (Post weight limits clearly)
	☐
	☐
	☐
	____________________

	Have employees received training on proper lifting techniques to minimize the risk of back injuries? (Documented training)
	☐
	☐
	☐
	____________________

	Have ergonomic assessments been conducted for workstations involving repetitive tasks (e.g., folding, sorting) to identify and mitigate risk factors?
	☐
	☐
	☐
	____________________

	Are work surfaces adjustable to accommodate different employee heights and prevent awkward postures?
	☐
	☐
	☐
	____________________

	Are anti-fatigue mats provided in areas where employees stand for extended periods?
	☐
	☐
	☐
	____________________

	Are mechanical assist devices (e.g., conveyors, lift tables) used to reduce manual lifting and carrying of heavy loads?
	☐
	☐
	☐
	____________________

	Are laundry chutes properly maintained and equipped with safety interlocks to prevent accidental falls?
	☐
	☐
	☐
	____________________

	Are laundry areas kept clean and free from clutter to prevent slips, trips, and falls?
	☐
	☐
	☐
	____________________

	Are chemical injection systems properly calibrated and maintained to prevent over- or under-dosing of detergents and other chemicals?
	☐
	☐
	☐
	____________________

	Are incompatible chemicals stored separately to prevent dangerous reactions?
	☐
	☐
	☐
	____________________


Fire Prevention & Electrical Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Are dryer lint traps cleaned daily to prevent lint buildup, which is a fire hazard? (Document cleaning schedule)
	☐
	☐
	☐
	____________________

	Is there adequate clearance (3 feet) around electrical panels to allow for safe access and maintenance?
	☐
	☐
	☐
	____________________

	Are extension cords used only temporarily and are they properly rated for the intended use? (No daisy-chaining)
	☐
	☐
	☐
	____________________

	Are ground-fault circuit interrupters (GFCIs) installed in wet locations (e.g., near washing machines) to protect against electrical shock?
	☐
	☐
	☐
	____________________

	Are fire extinguishers inspected monthly and serviced annually by a qualified technician? (Documented inspections)
	☐
	☐
	☐
	____________________

	Are exit routes clearly marked and free from obstructions?
	☐
	☐
	☐
	____________________

	Is emergency lighting functional and tested regularly to ensure adequate illumination during power outages?
	☐
	☐
	☐
	____________________

	Are hot work permits required for welding, cutting, or grinding activities in the laundry facility?
	☐
	☐
	☐
	____________________

	Are measures in place to control static electricity buildup, especially in areas where flammable solvents are used?
	☐
	☐
	☐
	____________________

	Is electrical equipment inspected regularly for damage (frayed cords, loose connections) and repaired or replaced as needed?
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
