InspectionReport
Municipal Sewer Confined Space Entry Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Pre-Entry Permit and Documentation
	Item
	Pass
	Fail
	N/A
	Notes

	Is the confined space entry permit completed, signed, and dated by an authorized entry supervisor?
	☐
	☐
	☐
	____________________

	Is a comprehensive hazard assessment documented, addressing potential atmospheric, physical, and engulfment hazards?
	☐
	☐
	☐
	____________________

	Has the entry team (entrant, attendant, supervisor) been thoroughly briefed on the permit, hazards, and emergency procedures?
	☐
	☐
	☐
	____________________

	Is an entry log available to track entry and exit times for all personnel?
	☐
	☐
	☐
	____________________

	Is a non-entry rescue plan documented and readily available?
	☐
	☐
	☐
	____________________

	Is there a log documenting the inspection of all entry equipment (gas monitors, retrieval systems, PPE) prior to use?
	☐
	☐
	☐
	____________________

	Is the communication system between the entrant and attendant tested and confirmed to be working effectively?
	☐
	☐
	☐
	____________________

	Are isolation procedures (lockout/tagout) verified to be in place for all potential energy sources and flow hazards?
	☐
	☐
	☐
	____________________


Atmospheric Testing and Monitoring
	Item
	Pass
	Fail
	N/A
	Notes

	Is the oxygen level within the acceptable range (19.5% - 23.5%)?
	☐
	☐
	☐
	____________________

	Is the H2S level below the permissible exposure limit (PEL) as defined by OSHA?
	☐
	☐
	☐
	____________________

	Are combustible gases below 10% of the Lower Explosive Limit (LEL)?
	☐
	☐
	☐
	____________________

	Is the gas monitor calibrated within the manufacturer's recommended timeframe, and is calibration documented?
	☐
	☐
	☐
	____________________

	Is atmospheric testing documented before entry and at regular intervals during entry?
	☐
	☐
	☐
	____________________

	Are the gas monitor's audible and visual alarms functioning correctly?
	☐
	☐
	☐
	____________________

	Was a bump test performed on the gas monitor prior to entry to verify sensor response?
	☐
	☐
	☐
	____________________

	If ventilation is required, is it in operation and positioned to effectively remove contaminants?
	☐
	☐
	☐
	____________________


Retrieval Systems and Fall Protection
	Item
	Pass
	Fail
	N/A
	Notes

	Is the tripod or retrieval system properly set up, stable, and anchored (if necessary)?
	☐
	☐
	☐
	____________________

	Is the retrieval line in good condition, free from cuts, abrasions, or other damage?
	☐
	☐
	☐
	____________________

	Is the entrant wearing a properly fitted full-body harness with a retrieval attachment point?
	☐
	☐
	☐
	____________________

	Is a mechanical advantage system (e.g., winch) available for non-entry rescue?
	☐
	☐
	☐
	____________________

	Is fall protection adequate for the specific entry point and potential fall hazards?
	☐
	☐
	☐
	____________________

	Is the retrieval system rated for the weight of the entrant plus any equipment?
	☐
	☐
	☐
	____________________

	If a self-retracting lifeline (SRL) is used, is it inspected and functioning correctly?
	☐
	☐
	☐
	____________________

	Is edge protection in place to prevent the retrieval line from being damaged?
	☐
	☐
	☐
	____________________

	Are rescue personnel trained in the proper use of the retrieval system?
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Is appropriate respiratory protection (e.g., SCBA, supplied air respirator) available and properly fitted if atmospheric hazards cannot be controlled?
	☐
	☐
	☐
	____________________

	Is appropriate eye protection (e.g., safety glasses, goggles) provided and worn?
	☐
	☐
	☐
	____________________

	Are chemical-resistant gloves worn to protect against potential contact with sewage or other contaminants?
	☐
	☐
	☐
	____________________

	Is appropriate protective clothing (e.g., coveralls, Tyvek suits) worn to prevent skin contamination?
	☐
	☐
	☐
	____________________

	Is head protection (hard hat) worn and in good condition?
	☐
	☐
	☐
	____________________

	Is appropriate foot protection (e.g., steel-toed boots) worn?
	☐
	☐
	☐
	____________________

	Is hearing protection available if noise levels exceed permissible limits?
	☐
	☐
	☐
	____________________

	Has all PPE been inspected for damage or defects prior to use?
	☐
	☐
	☐
	____________________


Site Control and Emergency Preparedness
	Item
	Pass
	Fail
	N/A
	Notes

	Are barricades or warning signs in place to prevent unauthorized access to the confined space?
	☐
	☐
	☐
	____________________

	Is emergency contact information readily available at the site?
	☐
	☐
	☐
	____________________

	Is a fully stocked first-aid kit available at the site?
	☐
	☐
	☐
	____________________

	Is a reliable method of communication established between the entrant, attendant, and emergency services?
	☐
	☐
	☐
	____________________

	Has the local rescue team been notified of the entry and potential hazards?
	☐
	☐
	☐
	____________________

	Is adequate lighting provided at the entry point and within the confined space?
	☐
	☐
	☐
	____________________

	Is the ventilation equipment positioned so that it does not create a trip hazard or obstruct the entry point?
	☐
	☐
	☐
	____________________

	Is traffic control in place to protect the entry team from vehicular traffic?
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
