InspectionReport
Film Production Pyrotechnics Safety Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Pre-Take Safety Meeting & Communication
	Item
	Pass
	Fail
	N/A
	Notes

	Was a pre-take safety briefing conducted with ALL personnel involved, including background actors, outlining potential hazards and emergency procedures?
	☐
	☐
	☐
	____________________

	Are emergency stop signals and evacuation routes clearly communicated and understood by all crew members?
	☐
	☐
	☐
	____________________

	Are the qualifications and certifications of the pyrotechnics team (Pyrotechnician in Charge, assistants) verified and documented?
	☐
	☐
	☐
	____________________

	Has the SPFX script and storyboard been thoroughly reviewed by the Pyrotechnician in Charge and Stunt Coordinator to identify all potential hazards?
	☐
	☐
	☐
	____________________

	Is a reliable communication system (e.g., radios) in place and tested for clear communication between the Pyrotechnician in Charge, First AD, and Stunt Coordinator?
	☐
	☐
	☐
	____________________

	Have weather conditions (wind, rain) been assessed and their potential impact on the pyrotechnic effects evaluated?
	☐
	☐
	☐
	____________________

	Has a safety bulletin outlining the specific hazards and safety precautions for the pyrotechnic effects been distributed to all crew members?
	☐
	☐
	☐
	____________________

	Is emergency contact information (local fire department, hospital) readily available and posted in a visible location?
	☐
	☐
	☐
	____________________

	Is a system in place to account for all personnel before and after each pyrotechnic effect?
	☐
	☐
	☐
	____________________

	Is there a clearly defined 'Hold Fire' protocol understood by all crew members, allowing anyone to immediately stop the sequence if a safety concern arises?
	☐
	☐
	☐
	____________________


Perimeter Security & Explosive Zone Control
	Item
	Pass
	Fail
	N/A
	Notes

	Is a clearly defined and marked perimeter established around the pyrotechnic area, with appropriate signage indicating 'No Entry'?
	☐
	☐
	☐
	____________________

	Is the perimeter actively monitored by security personnel to prevent unauthorized access?
	☐
	☐
	☐
	____________________

	Has the blast radius for each pyrotechnic effect been calculated and the perimeter established accordingly, considering potential debris and concussion?
	☐
	☐
	☐
	____________________

	Are measures in place to prevent public access to the pyrotechnic area, including crowd control and barriers?
	☐
	☐
	☐
	____________________

	Are all pyrotechnic materials and equipment stored securely in a locked and labeled container, away from potential ignition sources?
	☐
	☐
	☐
	____________________

	Are all unauthorized personnel kept outside the established perimeter during pyrotechnic operations?
	☐
	☐
	☐
	____________________

	Is vehicle access to the pyrotechnic area restricted and controlled to prevent accidental ignition or obstruction of emergency routes?
	☐
	☐
	☐
	____________________

	Are fire lanes clear and unobstructed to allow for rapid access by emergency vehicles?
	☐
	☐
	☐
	____________________

	Are all potential ignition sources (e.g., open flames, smoking) prohibited within the perimeter?
	☐
	☐
	☐
	____________________

	For squib effects, is the placement verified to ensure no direct contact with skin and appropriate padding is used?
	☐
	☐
	☐
	____________________


Fire Suppression & Emergency Response
	Item
	Pass
	Fail
	N/A
	Notes

	Are appropriate fire extinguishers (Type ABC and/or appropriate for the specific pyrotechnic materials) readily available and accessible within the perimeter?
	☐
	☐
	☐
	____________________

	Are fire extinguishers inspected monthly and tagged to indicate they are fully charged and in good working order?
	☐
	☐
	☐
	____________________

	Are trained fire watch personnel equipped with fire extinguishers and communication devices stationed within the perimeter during and after pyrotechnic effects?
	☐
	☐
	☐
	____________________

	Is a readily available water source (e.g., fire hydrant, water truck) with sufficient pressure and flow rate accessible for fire suppression?
	☐
	☐
	☐
	____________________

	Are emergency medical services (EMS) on standby or readily available to respond to any injuries?
	☐
	☐
	☐
	____________________

	Is a fully stocked first-aid kit readily available and accessible within the perimeter?
	☐
	☐
	☐
	____________________

	Are burn treatment supplies (e.g., sterile burn dressings, burn gel) included in the first-aid kit?
	☐
	☐
	☐
	____________________

	Is a written emergency evacuation plan in place and communicated to all crew members, including designated assembly points?
	☐
	☐
	☐
	____________________

	Are spill control procedures in place for handling and cleaning up any spilled pyrotechnic materials?
	☐
	☐
	☐
	____________________

	Is a thorough inspection conducted after each pyrotechnic effect to ensure all materials have been consumed or properly disposed of and no smoldering embers remain?
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Is appropriate hearing protection (e.g., earplugs or earmuffs with a Noise Reduction Rating (NRR) of at least 29 dB) provided to and worn by all personnel within the perimeter?
	☐
	☐
	☐
	____________________

	Is appropriate eye protection (e.g., safety glasses or goggles) provided to and worn by all personnel within the perimeter?
	☐
	☐
	☐
	____________________

	Are fire-resistant clothing (e.g., Nomex) provided to and worn by the pyrotechnics team and stunt performers in close proximity to the effects?
	☐
	☐
	☐
	____________________

	Are appropriate gloves (e.g., leather or fire-resistant) provided to and worn by personnel handling pyrotechnic materials?
	☐
	☐
	☐
	____________________

	Is appropriate foot protection (e.g., steel-toed boots) required for all personnel within the perimeter?
	☐
	☐
	☐
	____________________

	Are face shields provided to and worn by personnel in close proximity to potential flying debris?
	☐
	☐
	☐
	____________________

	Is respiratory protection (e.g., dust masks or respirators) provided to and worn by personnel if exposed to potentially harmful fumes or dust?
	☐
	☐
	☐
	____________________

	Is all PPE inspected before each use to ensure it is in good condition and properly fitted?
	☐
	☐
	☐
	____________________

	Have all personnel been trained on the proper use, maintenance, and limitations of their PPE?
	☐
	☐
	☐
	____________________

	Is PPE use consistently enforced within the perimeter?
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
