InspectionReport
Sewing Machine Safety Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Machine Guarding & Safety Devices
	Item
	Pass
	Fail
	N/A
	Notes

	Is the needle guard properly installed and free from damage, ensuring it effectively prevents finger contact with the needle? (Daily Check)
	☐
	☐
	☐
	____________________

	Is the thread take-up lever guard securely in place, preventing accidental contact with moving parts? (Daily Check)
	☐
	☐
	☐
	____________________

	Are all belt guards and covers in good condition and securely fastened, preventing access to moving belts and pulleys?
	☐
	☐
	☐
	____________________

	Does the emergency stop button function correctly, immediately stopping the machine when activated?
	☐
	☐
	☐
	____________________

	Is the foot pedal guarded to prevent accidental activation?
	☐
	☐
	☐
	____________________

	Does the machine have an automatic shut-off feature that activates when the needle guard is removed or compromised?
	☐
	☐
	☐
	____________________

	Is the motor fully enclosed to prevent contact with moving parts and electrical hazards?
	☐
	☐
	☐
	____________________

	Are lubrication points easily accessible without removing guards or exposing operators to hazards?
	☐
	☐
	☐
	____________________

	Is there any evidence of tampering with or bypassing of safety guards or interlocks?
	☐
	☐
	☐
	____________________

	If equipped, does the reverse feed mechanism operate smoothly and safely?
	☐
	☐
	☐
	____________________


Ergonomics & Workstation Setup
	Item
	Pass
	Fail
	N/A
	Notes

	Is the operator's chair adjustable for height, back support, and tilt to promote proper posture?
	☐
	☐
	☐
	____________________

	Is the work surface height appropriate for the operator to minimize bending and reaching?
	☐
	☐
	☐
	____________________

	Is a footrest provided for operators whose feet do not comfortably reach the floor?
	☐
	☐
	☐
	____________________

	Are tools and materials positioned within easy reach to minimize excessive reaching and twisting?
	☐
	☐
	☐
	____________________

	Are vibration-dampening pads or mounts used to reduce vibration transmitted to the operator?
	☐
	☐
	☐
	____________________

	Is the workstation adequately lit to minimize eye strain, with adjustable task lighting provided?
	☐
	☐
	☐
	____________________

	Are operators provided with scheduled breaks to reduce repetitive motion strain?
	☐
	☐
	☐
	____________________

	Is the workstation clean and free from clutter to prevent tripping hazards and promote efficient work?
	☐
	☐
	☐
	____________________

	Have operators received training on proper posture and ergonomic principles?
	☐
	☐
	☐
	____________________

	Is the stitch count monitored to ensure operators are not exceeding safe limits for repetitive motions?
	☐
	☐
	☐
	____________________

	Is anti-fatigue matting provided for operators who stand for extended periods?
	☐
	☐
	☐
	____________________


Electrical Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Is the power cord free from damage, fraying, or exposed wires?
	☐
	☐
	☐
	____________________

	Is the machine properly grounded to prevent electrical shock?
	☐
	☐
	☐
	____________________

	Is the electrical outlet in good condition and properly grounded?
	☐
	☐
	☐
	____________________

	Are extension cords used appropriately and not overloaded?
	☐
	☐
	☐
	____________________

	Is the electrical panel easily accessible and free from obstructions?
	☐
	☐
	☐
	____________________

	Are circuit breakers clearly labeled to identify the corresponding sewing machine?
	☐
	☐
	☐
	____________________

	Is GFCI (Ground Fault Circuit Interrupter) protection provided for outlets near water sources?
	☐
	☐
	☐
	____________________

	Are lockout/tagout procedures in place and followed during maintenance and repairs?
	☐
	☐
	☐
	____________________

	Are electrical conduits and wiring properly installed and protected from damage?
	☐
	☐
	☐
	____________________

	Are measures in place to control static electricity, especially when working with synthetic fabrics?
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Are operators wearing appropriate eye protection (safety glasses) to protect against flying debris?
	☐
	☐
	☐
	____________________

	Are finger guards or thimbles available and used to protect fingers during sewing?
	☐
	☐
	☐
	____________________

	Is hearing protection required and used in areas with high noise levels?
	☐
	☐
	☐
	____________________

	Are operators wearing appropriate clothing that is not loose or likely to get caught in the machine?
	☐
	☐
	☐
	____________________

	Are hair restraints used to keep long hair away from moving parts?
	☐
	☐
	☐
	____________________

	Is PPE in good condition and properly maintained?
	☐
	☐
	☐
	____________________

	Have operators received training on the proper use and care of PPE?
	☐
	☐
	☐
	____________________

	Is PPE readily available and accessible to all operators?
	☐
	☐
	☐
	____________________

	Are gloves provided and used when handling sharp objects or materials?
	☐
	☐
	☐
	____________________

	Is respiratory protection required and used when working with materials that generate dust or fumes?
	☐
	☐
	☐
	____________________


Housekeeping & General Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Are aisles and walkways clear of obstructions to prevent tripping hazards?
	☐
	☐
	☐
	____________________

	Are waste materials (fabric scraps, thread) disposed of properly and regularly?
	☐
	☐
	☐
	____________________

	Are fire extinguishers readily accessible and properly maintained?
	☐
	☐
	☐
	____________________

	Is a first-aid kit readily available and adequately stocked?
	☐
	☐
	☐
	____________________

	Are emergency exits clearly marked and unobstructed?
	☐
	☐
	☐
	____________________

	Are spill control procedures in place for handling lubricants and other fluids?
	☐
	☐
	☐
	____________________

	Are sewing machines securely mounted and stable to prevent tipping or movement during operation?
	☐
	☐
	☐
	____________________

	Are compressed air lines properly connected and free from leaks?
	☐
	☐
	☐
	____________________

	Are safety signs and warnings clearly visible and legible?
	☐
	☐
	☐
	____________________

	Are operator training records up-to-date and readily available?
	☐
	☐
	☐
	____________________

	Is a regular machine maintenance schedule in place and followed?
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
