InspectionReport
Shipyard Confined Space & Hot Work Inspection Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Marine Chemist Certification & Documentation
	Item
	Pass
	Fail
	N/A
	Notes

	Is a valid Marine Chemist Certificate conspicuously posted at the entrance to the confined space, specifying acceptable entry conditions?
	☐
	☐
	☐
	____________________

	Does the Marine Chemist Certificate clearly state the specific spaces certified and any limitations or endorsements?
	☐
	☐
	☐
	____________________

	Verify that the marine chemist's testing equipment (e.g., gas detectors) has current calibration certificates.
	☐
	☐
	☐
	____________________

	Are records of atmospheric testing (oxygen, LEL, toxic gases) available and consistent with the Marine Chemist Certificate?
	☐
	☐
	☐
	____________________

	Confirm that the Marine Chemist Certificate has not expired and is valid for the current work shift.
	☐
	☐
	☐
	____________________

	Has the Marine Chemist communicated all potential hazards and certificate requirements to the shipyard competent person and affected employees?
	☐
	☐
	☐
	____________________

	Is a hot work permit issued and signed by the shipyard competent person, referencing the Marine Chemist Certificate?
	☐
	☐
	☐
	____________________

	Is the hot work permit displayed prominently at the hot work location?
	☐
	☐
	☐
	____________________

	Are any amendments or changes to the Marine Chemist Certificate properly documented and communicated?
	☐
	☐
	☐
	____________________


Confined Space Entry Procedures
	Item
	Pass
	Fail
	N/A
	Notes

	Is a written confined space entry program in place, including a permit system?
	☐
	☐
	☐
	____________________

	Are entrants and attendants properly trained and aware of their roles and responsibilities?
	☐
	☐
	☐
	____________________

	Is continuous atmospheric monitoring being conducted during confined space entry?
	☐
	☐
	☐
	____________________

	Is adequate ventilation provided to maintain a safe atmosphere within the confined space?
	☐
	☐
	☐
	____________________

	Is a rescue plan in place and readily available, including necessary equipment and trained personnel?
	☐
	☐
	☐
	____________________

	Is a reliable communication system established between the entrant and the attendant?
	☐
	☐
	☐
	____________________

	Are all potential hazards (e.g., pipelines, electrical sources) properly isolated and locked out/tagged out?
	☐
	☐
	☐
	____________________

	Is appropriate emergency equipment (e.g., self-contained breathing apparatus, retrieval equipment) readily available?
	☐
	☐
	☐
	____________________

	Is adequate lighting provided within the confined space to ensure safe working conditions?
	☐
	☐
	☐
	____________________

	Are all entrants aware of the hazards within the confined space and the necessary precautions?
	☐
	☐
	☐
	____________________


Hot Work Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Is a certified fire watch present with appropriate fire extinguishing equipment?
	☐
	☐
	☐
	____________________

	Verify that fire extinguishers are readily accessible, fully charged, and recently inspected.
	☐
	☐
	☐
	____________________

	Have all combustible materials been removed or protected from ignition sources within 35 feet of the hot work area?
	☐
	☐
	☐
	____________________

	Inspect welding leads for damage, proper insulation, and secure connections.
	☐
	☐
	☐
	____________________

	Are welding machines properly grounded to prevent electrical shock hazards?
	☐
	☐
	☐
	____________________

	Is adequate ventilation provided to remove welding fumes and prevent the accumulation of flammable gases?
	☐
	☐
	☐
	____________________

	Is slag and sparks contained to prevent fire hazards and injuries to personnel?
	☐
	☐
	☐
	____________________

	Are welders and fire watches wearing appropriate personal protective equipment (PPE), including eye protection, gloves, and flame-resistant clothing?
	☐
	☐
	☐
	____________________

	Is the hot work area kept clean and free of debris to prevent fire hazards?
	☐
	☐
	☐
	____________________

	Will the fire watch remain in the area for at least 30 minutes after completion of hot work to monitor for smoldering fires?
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Are appropriate respirators (e.g., supplied air respirators) provided and used when atmospheric hazards are present?
	☐
	☐
	☐
	____________________

	Are appropriate eye protection (e.g., safety glasses, welding helmets) worn by all personnel in the area?
	☐
	☐
	☐
	____________________

	Is hearing protection provided and used in areas with high noise levels?
	☐
	☐
	☐
	____________________

	Is appropriate protective clothing (e.g., flame-resistant clothing, gloves) worn to protect against burns and other hazards?
	☐
	☐
	☐
	____________________

	Are safety shoes or boots worn to protect against foot injuries?
	☐
	☐
	☐
	____________________

	Inspect harnesses and lanyards for damage before each use, if fall protection is required.
	☐
	☐
	☐
	____________________

	Ensure all PPE fits properly and is in good working condition.
	☐
	☐
	☐
	____________________

	Have all employees been trained on the proper use, maintenance, and limitations of PPE?
	☐
	☐
	☐
	____________________

	Are face shields used when grinding or performing other tasks that generate flying debris?
	☐
	☐
	☐
	____________________


Housekeeping & General Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Are walking and working surfaces free of slip, trip, and fall hazards?
	☐
	☐
	☐
	____________________

	Is adequate lighting provided in all work areas?
	☐
	☐
	☐
	____________________

	Are access and egress routes clear and unobstructed?
	☐
	☐
	☐
	____________________

	Are electrical cords and equipment in good condition and properly grounded?
	☐
	☐
	☐
	____________________

	Are compressed gas cylinders properly secured and stored?
	☐
	☐
	☐
	____________________

	Are fire extinguishers, fire hoses, and other fire protection equipment readily accessible and in good working order?
	☐
	☐
	☐
	____________________

	Is a first-aid kit readily available and adequately stocked?
	☐
	☐
	☐
	____________________

	Are spill control materials available and readily accessible in areas where hazardous materials are used or stored?
	☐
	☐
	☐
	____________________

	Are waste materials properly disposed of to prevent fire hazards and environmental contamination?
	☐
	☐
	☐
	____________________

	Are appropriate safety signs and postings displayed in relevant areas?
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
