InspectionReport
Offshore Platform Dropped Object (DROPS) Prevention Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Derrick & Crane DROPS Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Are all tools used at height within the derrick properly tethered with a load-rated lanyard? Verify tether SWL exceeds tool weight by a factor of 2.
	☐
	☐
	☐
	____________________

	Inspect all lighting fixtures within the derrick. Are safety pins and secondary retention cables properly installed and secured?
	☐
	☐
	☐
	____________________

	Visually inspect all grating surfaces within the derrick for corrosion, damage, or missing sections. Are any sections compromised?
	☐
	☐
	☐
	____________________

	Check for any loose equipment or materials stored improperly on the derrick structure. Is all equipment secured or removed?
	☐
	☐
	☐
	____________________

	Are all hoses and cables within the derrick properly restrained to prevent swinging or falling hazards?
	☐
	☐
	☐
	____________________

	Verify that all lubrication equipment (grease guns, oil cans) are secured with tethers when used at height in the derrick.
	☐
	☐
	☐
	____________________

	Inspect all rigging hardware (shackles, hooks, slings) for proper locking mechanisms and absence of damage. Are any locking mechanisms missing or damaged?
	☐
	☐
	☐
	____________________

	Are taglines used during lifting operations in the derrick and are they in good condition (no cuts, frays, or knots)?
	☐
	☐
	☐
	____________________

	Confirm a tool inventory is maintained for all tools used in the derrick, and that a system is in place to track tools in and out of the area.
	☐
	☐
	☐
	____________________

	Assess the general housekeeping within the derrick. Is the area free from tripping hazards and debris that could become dropped objects?
	☐
	☐
	☐
	____________________


Process Area DROPS Inspection
	Item
	Pass
	Fail
	N/A
	Notes

	Inspect all pipe supports and clamps for corrosion or damage. Are any supports showing signs of weakness or failure?
	☐
	☐
	☐
	____________________

	Verify that all valve handles are securely attached and cannot be easily dislodged. Are any handles loose or missing securing hardware?
	☐
	☐
	☐
	____________________

	Check that all instrumentation (gauges, transmitters) are properly mounted and secured. Are any instruments loose or vibrating excessively?
	☐
	☐
	☐
	____________________

	Inspect cable trays for proper support and secure cable routing. Are any cables hanging loose or unsupported?
	☐
	☐
	☐
	____________________

	Verify that all lighting fixtures are securely mounted and have secondary retention. Are any fixtures missing safety cables or mounting hardware?
	☐
	☐
	☐
	____________________

	Inspect all walkways and platforms for damaged or missing grating. Are any sections of grating compromised, creating a potential fall or DROPS hazard?
	☐
	☐
	☐
	____________________

	Check that all signage is securely mounted and legible. Are any signs loose, damaged, or missing?
	☐
	☐
	☐
	____________________

	Ensure any temporary equipment (scaffolding, ladders) is properly secured and does not pose a DROPS hazard. Is all temporary equipment properly tagged and inspected?
	☐
	☐
	☐
	____________________

	Verify that hoses are properly stored and secured when not in use to prevent them from becoming a trip or dropped object hazard.
	☐
	☐
	☐
	____________________

	Confirm that the 'Red Zone' areas are clearly marked and access is controlled to prevent unauthorized personnel from entering areas with high DROPS potential.
	☐
	☐
	☐
	____________________


General Platform DROPS Prevention
	Item
	Pass
	Fail
	N/A
	Notes

	Are 3.5-inch toeboards installed on all open sides of elevated platforms and walkways?
	☐
	☐
	☐
	____________________

	Is debris netting installed below elevated work areas to catch falling objects?
	☐
	☐
	☐
	____________________

	Is the platform free of loose materials, tools, and debris that could become dropped objects?
	☐
	☐
	☐
	____________________

	Are toolboxes equipped with secure latches and handles to prevent accidental opening and spillage?
	☐
	☐
	☐
	____________________

	Is equipment stored in designated areas and secured to prevent movement or falling?
	☐
	☐
	☐
	____________________

	Are DROPS awareness signs prominently displayed throughout the platform?
	☐
	☐
	☐
	____________________

	Are drainage systems clear and free of obstructions that could cause water accumulation and corrosion, leading to DROPS hazards?
	☐
	☐
	☐
	____________________

	Are ventilation systems properly maintained and free of loose components that could detach and fall?
	☐
	☐
	☐
	____________________

	Verify that emergency equipment (fire extinguishers, first aid kits) are securely mounted and readily accessible.
	☐
	☐
	☐
	____________________

	Ensure adequate lighting is provided in all work areas to facilitate visual inspection for potential DROPS hazards.
	☐
	☐
	☐
	____________________


Dropped Object Prevention Program
	Item
	Pass
	Fail
	N/A
	Notes

	Is a comprehensive DROPS prevention program documented and readily available?
	☐
	☐
	☐
	____________________

	Have all personnel received adequate training on DROPS prevention and hazard identification?
	☐
	☐
	☐
	____________________

	Are routine DROPS inspections conducted and documented?
	☐
	☐
	☐
	____________________

	Is there a system in place for reporting and addressing potential DROPS hazards?
	☐
	☐
	☐
	____________________

	Is there a tool control program in place to manage and track tools used at height?
	☐
	☐
	☐
	____________________

	Is there a preventative maintenance program in place to address potential DROPS hazards related to equipment and infrastructure?
	☐
	☐
	☐
	____________________

	Are DROPS risk assessments conducted for all tasks involving work at height?
	☐
	☐
	☐
	____________________

	Are lessons learned from previous DROPS incidents incorporated into the DROPS prevention program?
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required
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Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
