InspectionReport
Smart Meter Installation Safety Checklist
Documentation aid only. Adapt this resource to the site, manufacturer instructions, and applicable local requirements. It does not replace a competent person, professional judgment, legal advice, or a required statutory form.
	Site / Project: ______________________________
	Address: ______________________________

	Inspector name: ______________________________
	Company: ______________________________

	Date: ______________________________
	Time: ______________________________


Inspection checklist
Pre-Installation Assessment & Planning
	Item
	Pass
	Fail
	N/A
	Notes

	Was a pre-pull voltage check performed on the meter base using a calibrated voltage tester (e.g., Fluke T6-1000) to verify absence of voltage? Document readings and socket condition with photos.
	☐
	☐
	☐
	____________________

	Visually inspect the meter base for signs of corrosion, arcing, or overheating (hot sockets). Document any defects with photos before proceeding.
	☐
	☐
	☐
	____________________

	Assess the property for potential animal hazards (dogs, cats, etc.). Have a plan for safe interaction or containment (e.g., customer notification, use of deterrents).
	☐
	☐
	☐
	____________________

	Verify that no backup power sources (generators, solar panels) are connected to the customer's electrical system without proper isolation or transfer switches. Confirm with homeowner.
	☐
	☐
	☐
	____________________

	Evaluate weather conditions (rain, snow, extreme temperatures). Are conditions safe for electrical work? Postpone if necessary.
	☐
	☐
	☐
	____________________

	Establish clear communication protocols with the homeowner regarding the installation process, potential power outages, and safety precautions.
	☐
	☐
	☐
	____________________

	Confirm the new smart meter is the correct type and rating for the existing meter base and service. Check AMI system for correct meter number.
	☐
	☐
	☐
	____________________

	Verify that emergency contact information (supervisor, utility dispatch) is readily available and accessible.
	☐
	☐
	☐
	____________________

	Confirm that a site-specific Lockout/Tagout (LOTO) procedure is in place and understood for disconnecting and reconnecting the meter.
	☐
	☐
	☐
	____________________

	If a ladder is needed, is it the correct type (fiberglass, rated for electrical work) and in good condition (no damage, current inspection tag)?
	☐
	☐
	☐
	____________________


Personal Protective Equipment (PPE)
	Item
	Pass
	Fail
	N/A
	Notes

	Are properly rated and tested rubber insulating gloves (e.g., Class 0 or Class 00) being worn and inspected for damage before each use? Use leather protectors.
	☐
	☐
	☐
	____________________

	Are safety glasses with side shields being worn to protect against arc flash and debris?
	☐
	☐
	☐
	____________________

	Is appropriate arc-rated clothing (e.g., shirt, pants) being worn based on the potential arc flash hazard assessment? (Minimum ATPV rating of 4 cal/cm²)
	☐
	☐
	☐
	____________________

	Are all hand tools being used (e.g., screwdrivers, pliers) insulated and rated for the voltage being worked on (1000V)?
	☐
	☐
	☐
	____________________

	Are steel-toe boots being worn to protect against foot injuries?
	☐
	☐
	☐
	____________________

	Is high-visibility clothing (e.g., vest or shirt) being worn to ensure visibility to others?
	☐
	☐
	☐
	____________________

	Is hearing protection available and used if noise levels exceed 85 dBA?
	☐
	☐
	☐
	____________________

	Is a face shield available and used for additional arc flash protection during meter removal and installation?
	☐
	☐
	☐
	____________________


On-Site Safety Procedures
	Item
	Pass
	Fail
	N/A
	Notes

	Is a clear and safe work zone established around the meter base to prevent unauthorized access?
	☐
	☐
	☐
	____________________

	After LOTO, re-verify absence of voltage at the meter base using a calibrated voltage tester before commencing work.
	☐
	☐
	☐
	____________________

	Are proper lifting techniques being used to prevent back injuries when handling the smart meter?
	☐
	☐
	☐
	____________________

	Ensure the meter base is securely mounted and in good condition before installing the new smart meter. Repair or replace if necessary.
	☐
	☐
	☐
	____________________

	Ensure all connections and enclosures are properly weatherproofed to prevent moisture ingress.
	☐
	☐
	☐
	____________________

	Verify the meter seal is intact and properly installed to prevent tampering.
	☐
	☐
	☐
	____________________

	Maintain a clean and organized work area, free of debris and tripping hazards.
	☐
	☐
	☐
	____________________

	Maintain open communication with the homeowner throughout the installation process, addressing any questions or concerns.
	☐
	☐
	☐
	____________________

	After installation, verify the smart meter is operating correctly and transmitting data to the AMI system.
	☐
	☐
	☐
	____________________

	Conduct a post-installation inspection to ensure all connections are secure, the meter is properly seated, and the area is clean.
	☐
	☐
	☐
	____________________


Vehicle & Equipment Safety
	Item
	Pass
	Fail
	N/A
	Notes

	Is the vehicle inspected daily (tires, lights, brakes, fluid levels) using a pre-trip inspection checklist?
	☐
	☐
	☐
	____________________

	Is the vehicle parked safely, avoiding obstructions to traffic or pedestrian walkways?
	☐
	☐
	☐
	____________________

	Is the ladder properly secured in the vehicle to prevent shifting or damage during transport?
	☐
	☐
	☐
	____________________

	Are tools and equipment properly secured in the vehicle to prevent them from becoming projectiles in the event of an accident?
	☐
	☐
	☐
	____________________

	Is a fully stocked first-aid kit available in the vehicle?
	☐
	☐
	☐
	____________________

	Is a properly charged and inspected fire extinguisher available in the vehicle?
	☐
	☐
	☐
	____________________

	Are traffic control devices (cones, signs) available and used when working near roadways?
	☐
	☐
	☐
	____________________

	Is the voltage tester calibrated per manufacturer's recommendations and within the calibration period? Document calibration date.
	☐
	☐
	☐
	____________________


Findings
	#
	Item
	Location
	Severity
	Action required

	1
	
	
	
	

	2
	
	
	
	

	3
	
	
	
	

	4
	
	
	
	

	5
	
	
	
	

	6
	
	
	
	

	7
	
	
	
	

	8
	
	
	
	


Signature
Inspector signature: ______________________________    Name: ______________________________
Date: ______________________________
Free resource from inspectionreport.app - build an evidence-backed report from photos at https://www.inspectionreport.app/new-report
